# CDMA PDSN Registration Failures (contd..)

This dialog box is applicable to Controller, Member, and Peer to Peer clusters. From here, you can view rejected registration statistics.

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN Registration Failures (contd..).

The following data is displayed:

> Registration Request Failed Unknown HA/PDSN (cCdmaRpRegUnknownPdsnFailures)

> Registration Request Failed Reverse Tunnel (cCdmaRPRegNoRevTunnelFailures)

> Registration Request Failed T bit (cCdmaRPRegTBitNotSetFailures)

> Registration Request Failed CVSE (cCdmaRPRegBadCVSEFailures)

### Registration Request Failed Unknown HA/PDSN (cCdmaRpRegUnknownPdsnFailures)

Number of registration requests that failed due to an unknown packet data serving node (PDSN) or Home Agent (HA) address since the system was last restarted.

### Registration Request Failed Reverse Tunnel (cCdmaRPRegNoRevTunnelFailures)

Number of registration requests that failed due to a Foreign Agent (FA) to HA tunnel setup failure since system startup.

### Registration Request Failed T bit (cCdmaRPRegTBitNotSetFailures)

Number of registration requests that failed due to an unset T bit since system startup.

### Registration Request Failed CVSE (cCdmaRPRegBadCVSEFailures)

Number of registration requests that failed due to an unsupported vendor code in CVSE since system startup.