# SSG General Information

The SSG General Information category of the Configure dialog box displays general information on the service selection gateway (SSG).

## Procedure

1. Right-click the device, then select Configure, or double-click the device.

2. Select SSG General Information from the Category list.

The following information appears:

Time Interval (cssgCfgAutoLogOffInterval)

ICMP Ping Retries (cssgCfgAutoLogOffIcmpRetries)

Maximum Service (cssgCfgMaxServicesPerUser)

Default Ip Address Type (cssgCfgDefaultNetWorkType)

Default Ip Address (cssgCfgDefaultNetWork)

Access Request Receipt Port (cssgCfgRadiusAuthenPort)

Accounting Receipt Port (cssgCfgRadiusAccountingPort)

Authenticated TCP Group (cssgCfgTCPRedirGrpForUnAuthUsers)

Unauthorized TCP Group (cssgCfgTCPRedirGrpForUnAuthServ)

SMTP TCP Group (cssgCfgTcpRedirGrpForSMTP)

Initial Captivation TCP Group (cssgCfgTcpRedirGrpForInitialCapt)

Advertising Captivation TCP Group (cssgCfgTcpRedirGrpForAdvCapt)

### Time Interval (cssgCfgAutoLogOffInterval)

Interval at which connectivity to a host is checked.

If the host is not reachable, service selection gateway (SSG) logs off the host if the auto-logoff feature is enabled.

### ICMP Ping Retries (cssgCfgAutoLogOffIcmpRetries)

Number of ICMP ping attempts made by service selection gateway (SSG) to check connectivity to a host.

### Maximum Service (cssgCfgMaxServicesPerUser)

Maximum number of services allowed per user.

### Default Ip Address Type (cssgCfgDefaultNetWorkType)

Type of the IP address stored in cssgCfgDefaultNetwork.

### Default Ip Address (cssgCfgDefaultNetWork)

IP address or subnet that users can access without authentication. This is the address where the Cisco service selection dashboard or subscriber-edge service manager resides.

### Access Request Receipt Port (cssgCfgRadiusAuthenPort)

Port on which service selection gateway (SSG) receives access request packets from remote authentication dial-in user service clients.

### Accounting Receipt Port (cssgCfgRadiusAccountingPort)

Port on which service selection gateway (SSG) receives accounting packets from remote authentication dial-in user service clients.

### Authenticated TCP Group (cssgCfgTCPRedirGrpForUnAuthUsers)

TCP redirect group to which service selection gateway (SSG) directs unauthenticated users.

### Unauthorized TCP Group (cssgCfgTCPRedirGrpForUnAuthServ)

TCP redirect group to which service selection gateway (SSG) directs unauthorized service access users.

### SMTP TCP Group (cssgCfgTcpRedirGrpForSMTP)

TCP redirect group to which service selection gateway (SSG) redirects SMTP traffic.

### Initial Captivation TCP Group (cssgCfgTcpRedirGrpForInitialCapt)

TCP redirect group for initial captivation.

### Advertising Captivation TCP Group (cssgCfgTcpRedirGrpForAdvCapt)

TCP redirect group for advertising captivation.