# Transmit side High Priority Traffic Statistics

Use this option to monitor statistics of high priority traffic reception to physical medium-dependent layer in a particular interval for a particular side of a particular SRP interface.

## Procedure

To access high priority traffic information:

1. Right-click the port and select SRP Interface Statistics from the pop-up menu.

Media Dependent Statistics dialog box appears.

2. Select Tx Physical Layer Statistics from the Category menu to display Transmit Physical Layer Statistics dialog box.

3. Select High Priority Traffic from the Category menu to display high priority traffic information.

High Priority Traffic dialog box displays:

Unicast High Priority Packets (srpRingIntUcastHighPriPktsOut)

Unicast High Priority Octets (srpRingIntUcastHighPriOctetsOut)

Multicast High Priority Packets (srpRingIntMcastHighPriPktsOut)

Multicast High Priority Octets (srpRingIntMcastHighPriOctetsOut)

### Unicast High Priority Packets (srpRingIntUcastHighPriPktsOut)

Number of high priority unicast packets going to physical medium-dependent layer during a 15-minute interval in past 24 hours.

### Unicast High Priority Octets (srpRingIntUcastHighPriOctetsOut)

Number of high priority unicast octets going to physical medium dependent layer during a 15-minute interval during past 24 hours.

### Multicast High Priority Packets (srpRingIntMcastHighPriPktsOut)

Number of high priority multicast packets going to physical medium dependent layer during a 15-minute interval during past 24 hours.

### Multicast High Priority Octets (srpRingIntMcastHighPriOctetsOut)

Number of high priority multicast octets going to physical medium dependent layer during a 15-minute interval during past 24 hours.

## Related Topics

The CiscoView Monitor Window

Monitoring Ports

Monitoring the Device

Monitoring the Device Environment

Monitoring Devices and Components