PATH=/ciscoview/Routershare/monitor/AAA_Accounting.htm TITLE=AAA_Accounting TEXT=AAA Accounting The AAA Accounting monitors accounting statistics of the server. The statistics is the delta value(present Right-click previous value) information polling interval and unit measurement Nos/Interval Procedure device, then select row (casAcctServerErrorResponses) Configuration Table, button following appears: (casAcctRequests) (casAcctRequestTimeouts) (casAcctUnexpectedResponses) (casAcctIncorrectResponses) Error Incorrect (casAcctTransactionSuccesses) Successes (casAcctTransactionFailures) Number requests. since system reinitialization. Retransmissions due timeouts are counted distinct timedout results retransmission request. stop when reaches maximum. unexpected responses received from reinitialization; example, delayed These indicate that identified its operation. unprocessed Reasons inability decrypt response, invalid fields, successful transactions performed includes multiple occur. responds with either pass fail. failed failure occurs resends aborts transaction.
PATH=/ciscoview/Routershare/monitor/AAA_Accounting_Sessions_Total_Session_Statistics.htm TITLE=AAA_Accounting_Sessions_Total_Session_Statistics TEXT=AAA Accounting Sessions-Total Session Statistics The AAA Accounting Sessions- Total Sessions Statistics, provides data information based Authentication, Authorization, Accounting. Procedure Right-click device, select Click Monitor Statistics. following appears: (casnTotalSessions) (casnDisconnectedSessions) Number of since last system reinitialization. Includes all casnActiveTable and previous sessions, whether terminated via another method. disconnected using still with value true(1) that result settings.
PATH=/ciscoview/Routershare/monitor/AAA_Authentication.htm TITLE=AAA_Authentication TEXT=AAA Authentication AAA Authentication monitors the authentication statistics of the server. The statistics delta value(present Right-click previous value) information polling interval and unit measurement Nos/Interval Procedure device, select row (casAuthenServerErrorResponses) Configuration Table, following appears: (casAuthenRequests) (casAuthenRequestTimeouts) (casAuthenUnexpectedResponses) (casAuthenIncorrectResponses) Error Incorrect (casAuthenTransactionSucesses) Successes (casAuthenTransactionFailures) Number requests. when active. Retransmissions due timeouts are counted distinct timed since was made results retransmission request. stop reaches maximum. unexpected responses received For example, delayed These mean that identified with its operation. unprocessed Reasons inability decrypt response, invalid fields, successful transactions this includes multiple occur. responds either pass fail. failed failure occurs resends aborts transaction.
PATH=/ciscoview/Routershare/monitor/AAA_Authorization.htm TITLE=AAA_Authorization TEXT=AAA Authorization The AAA Authorization monitors authorization statistics of the server. The statistics delta value(present Right-click previous value) information polling interval and unit measurement Nos/Interval Procedure device, then select row (casAuthorServerErrorResponses) Configuration Table, Authorization. following appears: (casAuthorRequests) (casAuthorRequestTimeouts) (casAuthorUnexpectedResponses) (casAuthorIncorrectResponses) Error Incorrect (casAuthorTransactionSuccesses) Successes (casAuthorTransactionFailures) Number requests. since was made active. Retransmissions due timeouts are counted distinct It not instantiated protocols that do support function. timed results retransmission request. stop when reaches maximum. unexpected responses received from active; example, delayed These show identified its operation. unprocessed Reasons inability decrypt response, invalid fields, successful transactions with this includes multiple occur. responds either pass fail. failed failure occurs resends aborts transaction.
PATH=/ciscoview/Routershare/monitor/AAL5_VCC_Traffic.htm TITLE=AAL5 VCC Traffic TEXT=The ATM Adaptation Layer type 5 Virtual Circuit Connections (AAL5 VCC) Traffic dialog box displays AAL5 for selected sub interfaces; VPI port, VCI values. Procedure Right-click then Monitor. Select Performance from Category list. row and displayed. following details are PDUs Received (cAal5VccInPkts) Transmitted (cAal5VccOutPkts) (cAal5VccInOctets) (cAal5VccOutOctets) number of Layer5 CPCS associated with entity. octets
PATH=/ciscoview/Routershare/monitor/Access_Point_Monitor2.htm TITLE=Access Point Monitor2 TEXT=GGSN Access Point PDPs Procedure Right-click the device, then select Monitor . Select GGSN Access Point Statistics from Category list. row and PDPs. following details are displayed: (cgprsAccPtActivePdps) contexts Count deactivation procedures. completed (cgprsAccPtSuccGgsDeactivatedPdps) (cgprsAccPtGgsnDeactivatedPdps) No of (cgprsAccPtNetworkInitPdps) Initiated Successfully (cgprsAccPtSuccNetworkInitPdps) (cgprsAccPtUpstreamTrafficVol) Payload (cgprsAccPtDownstreamTrafficVol) total number network by GGSN. current active this APN. volume. upstream traffic. Data flow MS PDN considered downstream as
PATH=/ciscoview/Routershare/monitor/AHDLC_Dropped_Packets.htm TITLE=AHDLC Dropped Packets TEXT=The AHDLC Dropped Packets dialog box allows you to view information about the dropped packets. Procedure Right-click device, then select Configure double-click device. Engine Details from Category list. and following appears: Decoding (cCdmaAhdlcDropPktsDec) Encoding (cCdmaAhdlcDropPktsEnc) (cCdmaAhdlcCRCDropPkts) Error Insufficient Memory During (cCdmaAhdlcMemDropPktsDec) (cCdmaAhdlcMemDropPktsEnc) Queue (cCdmaAhdlcOverflowDropPktsDec) (cCdmaAhdlcOverflowDropPktsEnc) Invalid (cCdmaAhdlcInvSizeDropPktsDec) (cCdmaAhdlcInvSizeDropPktsEnc) Number of by asynchronous high-level data link control (AHDLC) since system was last restarted. counter value could have discontinuities when management reinitialized other times shown cCdmaAhdlcDiscontinuityTime. because overflow size
PATH=/ciscoview/Routershare/monitor/AHDLC_Traffic_Details.htm TITLE=AHDLC Traffic Details TEXT=The AHDLC Traffic Details dialog box allows you to monitor delivery and generation information about asynchronous high-level data link control (AHDLC) engine. traffic. Procedure Right-click device, then select Configure double-click device. from Category list. following appears: Active (cCdmaAhdlcEngineChannelsInUse) (cCdmaAhdlcOutgoingOctetsToEncode) (cCdmaAhdlcOutgoingOctetsEncoded) (cCdmaAhdlcOutgoingPktsEncoded) Packets (cCdmaAhdlcOutgoingPktsToEncode) (cCdmaAhdlcIncomingOctetsToDecode) (cCdmaAhdlcIncomingOctetsDecoded) (cCdmaAhdlcIncomingPktsToDecode) (cCdmaAhdlcIncomingPktsDecoded) Number of channels handled by Total outgoing octets delivered encoding since system was last restarted. counter value could have discontinuities when management reinitialized other times shown cCdmaAhdlcDiscontinuityTime. generated through incoming decoding dropped due insufficient memory during
PATH=/ciscoview/Routershare/monitor/Airlink_RP_Registration_Request_Errors.htm TITLE=Airlink RP Registration Request Errors TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cCdmaRegReqInitNoSetupErrs) Record Not Received (cCdmaRegReqStartBeforeSetupErrs) De-Registration (cCdmaRegReqStartOnCloseErrs) (cCdmaRegReqStartOnActiveErrs) Session (cCdmaRegReqStopOnDormantErrs) Dormant Initial (cCdmaRegReqInitRcvdStopErrs) (cCdmaRegReqInitRcvdSDBErrs) setup since system was last restarted. before already active stop
PATH=/ciscoview/Routershare/monitor/BGP_FSM_Transitions_Monitoring.htm TITLE=BGP4 FSM Transitions TEXT=The BGP4 FSM Transitions category in the Monitor BGP4 Traffic dialog box enables you to monitor established transitions. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure device, double-click Device Configuration appears. Protocols from list. SelectProtocol Details button. (bgpPeerFsmEstablishedTransitions) Information rows table. and later: list, Note left frame displays categories right If displayed, variable which indexed key values of are listed below category. view particular Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane box. A following appears: (bgpPeerFsmEstablishedTime) Related Topic Messages Total number times transitioned state. Indicates period, seconds, peer has been since was last object set zero when new configured router booted.
PATH=/ciscoview/Routershare/monitor/BGP_Messages_Monitoring.htm TITLE=BGP4 Messages TEXT=The BGP4 Messages category of the Monitor BGP4 Traffic dialog box enables you to monitor BGP4 update and total that have been transmitted received. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure list, double-click Device Configuration appears. Protocols from list. indexed SelectProtocol Details button. (bgpPeerInUpdates) Information rows table. later: Note left frame displays categories right If displayed, variable which key values are listed below category. view particular Multiple indexes table, any, nested manner. about value. lowest indexing row. pane box. A following appears: Rx Count Last (bgpPeerInUpdateElapsedTime) Time Tx (bgpPeerOutUpdates) (bgpPeerInTotalMessages) (bgpPeerOutTotalMessages) Related Topic FSM Transitions Number connection. object initialized zero. when established. time, seconds, since message was peer. Each incremented, this set remote
PATH=/ciscoview/Routershare/monitor/BGP_Policy_Accounting_Traffic.htm TITLE=BGP Policy Accounting Traffic TEXT=The BGP Policy Accounting Traffic Monitor dialog box monitors a particular type of traffic on a particular interface. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure list, double-click Device Configuration appears. Protocols from Category list. BGP4 SelectProtocol Details button. Peer Information rows table. and later: Note left frame displays categories right If displayed, variable which indexed key values are listed below category. view Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane box. following appears: Received Packets (cbpAcctInPacketCount) Octets (cbpAcctInOctetCount) Related Topics Messages FSM Transitions Total number
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_a11_reg_denial_stats.htm TITLE=CDMA PDSN A11 Registration Denial Statistics TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cCdmaRpDeRegHandoffDeniedReqs) De-established R-P Conn Initial (cCdmaRpInitRegDiscardedReqs) Re-Registration (cCdmaRpReRegDiscardedReqs) De-Registration (cCdmaRpDeRegDiscardedReqs) (cCdmaRpHandoffRegDeniedReqs) (cCdmaRpHandoffRegDiscardedReqs) (cCdmaRpInterPCFActiveHandoffs) (cCdmaRpInterPCFDormantHandoffs) Handoffs Dormant total number denied Requests meant de-establishing connections with Packet Control Function (PCF) which mobile node was handed since system last restarted. Code field corresponding Reply message set non-zero. silently discarded handoff already existing sessions active
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_a11_reg_stats.htm TITLE=CDMA PDSN A11 Registration Statistics TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cCdmaRpDeRegHandoffAcceptedReqs) De-established R-P Conn Initial (cCdmaRpInitRegReceivedReqs) Re-Registration (cCdmaRpReRegReceivedReqs) De-Registration (cCdmaRpDeRegReceivedReqs) (cCdmaRpHandoffRegReceivedReqs) (cCdmaRpHandoffRegAcceptedReqs) (cCdmaRpReRegAirlinkStarts) Start (cCdmaRpReRegAirlinkStops) (cCdmaRpDeRegAirlinkStops) total number accepted Requests meant de-establishing already connections with Packet Control Function (PCF) which mobile node was handed since system last restarted. Code field corresponding Reply message set zero. received handoff existing session, containing
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_Addressing_Schema_Statistics.htm TITLE=CDMA PDSN Addressing Schema Statistics TEXT=The CDMA PDSN Addressing Schema Statistics category of the Monitor Device dialog box displays the handoff packet data servicing node (PDSN). Procedure Right-click device, then select appears. from list. following information appears: (cCdmaAddressStaticSIPs) (cCdmaAddressDynamicSIPs) negotiated byProxy Simple (cCdmaAddressDynamicMIPs) MOIP (cCdmaAddressStaticMIPs) Proxy (cCdmaAddressStaticPMIPs) (cCdmaAddressDynamicPMIPs) byVPDN (cCdmaAddressStaticVPDNs) (cCdmaAddressDynamicVPDNs) Ip Total number calls that static addresses. dynamic mobile
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_closed_rp_reg_stat.htm TITLE=CDMA PDSN Closed RP Registration Statistics TEXT=Procedure Right-click the device and then select Monitor . Select CDMA PDSN Closed RP Registration Statistics from Category list. following information appears: PCF IP (ccpcPcfIpAddress) address of that serves mobile node.
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_closed_rp_reg_stat_1.htm TITLE=CDMA PDSN Closed RP Registration Statistics - 1 TEXT=Procedure Right-click the device and then select Monitor . Select CDMA PDSN Closed RP Registration Statistics from Category list. row Monitor. following information appears: Incoming-Call-Connected Incoming-Call-Requests Requests (ccpcPcfRcvdIcrqs) Accepted (ccpcPcfAcptdIcrqs) Denied (ccpcPcfDroppedIcrqs) Incoming-Call-Replies (ccpcPcfSentIcrps) Received (ccpcPcfRcvdIccns) (ccpcPcfAcptdIccns) Total number of established L2TP session since tunnel was with PCF. sent messages
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_closed_rp_reg_stat_2.htm TITLE=CDMA PDSN Closed RP Registration Statistics - 2 TEXT=Procedure Right-click the device and then select Monitor . Select CDMA PDSN Closed RP Registration Statistics from Category list. row Monitor. following information appears: Incoming-Call-Connected (ccpcPcfDroppedIccns) Call-Disconnect-Notify Received (ccpcPcfRcvdCdns) (ccpcPcfSentCdns) (ccpcPcfDroppedCdns) Zero-Length-Buffer Recieved (ccpcPcfRcvdZlbs) (ccpcPcfSentZlb) Total number of messages accepted since L2TP tunnel was established with PCF. tear down session sent dropped
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_Cluster.htm TITLE=CDMA PDSN Cluster TEXT=The CDMA PDSN Cluster category of the Monitor Device dialog box displays the handoff statistics of the packet data servicing node (PDSN). Procedure Right-click device, then select appears. from list. following information appears: (CdmaClusterTotalSessions) Sessions number session records controller.
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_feature_overview.htm TITLE=CDMA PDSN feature overview TEXT=CDMA PDSN Overview This overview module describes the Cisco Packet Data Serving Node (Cisco PDSN) feature. It includes following sections: System Benefits For More Information Related Features, Standard Technologies Documents hardware IOS software that enables 7500 series router, Protocol-Independent function IP-based gateway between wireless Radio Access Network (RAN) Internet. With enabled stationary roaming mobile user can Internet, corporate intranet, Application (WAP) services. supports both Simple IP. operation. Note operation, which referred types. available determined by offered provider. context PDSN, end CDMA2000 architecture defined TIA/EIA/IS-835 (also known 3GPP2 TSG-P TR45.6). typical terminal equipment, termination, transceiver stations (BTS), controllers (BSC), PDSNs, other entities. cellular network, interfaces. router. Common Services Layer Each aligned Second generation (2G) investment. third (3G) seamless delivery Core all Air Interfaces existing Consistent wireline evolution. hybrid, multi-standard networks. Proxy benefit from mobility. Improves customer experience minimizing disruption applications when handoff occurs. Intelligent Selection Selects best workload prior sessions. optimal performance. Scales without service. platforms proven some largest world. runs set, rich IP, security, QoS, voice-data integration capability. Routing Configuration Guide Protocols Configuring Release 12.1 No. 1078 Point-to-Point protocol (PPP) Authentication Authorization Accounting (AAA) Virtual Private (VPDN) Remote Dial-In (RADIUS) Security Command Reference Topics Statistics PCF Session Registration RP Update
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_Handoff_Statistics.htm TITLE=CDMA PDSN Handoff Statistics TEXT=The CDMA PDSN Handoff Statistics category of the Monitor Device dialog box displays the handoff statistics packet data servicing node (PDSN). Procedure Right-click device, then select appears. from list. following information appears: (cCdmaInterPcfHandoffs) (PCF) (cCdmaInterPdsnHandoffs) CANID/PANID changes, (cCdmaIdChangeHandoffs) Total number inter control function handoffs, since system last restarted. because
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_interpcf_rgnupdate_failures.htm TITLE=CDMA PDSN Inter PCF Handoff Registration Update Failures TEXT=Use this option to view Inter Packet Control Function (PCF) Handoff Registration Update Failures. Procedure access information Right-click Authentication device select Monitor from popup menu. Category following appears: Unspecified (cCdmaRpUpdHandoffReaUnSpecFails) Administrative (cCdmaRpUpdHandoffAdmProhibFails) (cCdmaRpUpdHandoffMNAuthenFails) ID (cCdmaRpUpdHandoffIdMismatchFails) (cCdmaRpUpdHandoffBadReqFails) Request Note: All these statistics are result handoffs. Number updated registrations that failed due reason sincesystem startup. prohibition failure identity mismatch poorly formed
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_interpcf_rgnupdate_stats.htm TITLE=CDMA PDSN Inter PCF Handoff Registration Update Statistics TEXT=Use this option to view Inter Packet Control Function (PCF) Handoff Registration Update Statistics . Procedure access Statisticsinformation: Right-click these device select Monitor from popup menu. Category following appears: Updates by (cCdmaRpUpdPcfHandoffs) (cCdmaRpUpdHandoffNotAckedReqs) Acknowledged (cCdmaRpUpdHandoffReceivedAcks) (cCdmaRpUpdHandoffAcceptedReqs) (cCdmaRpUpdHandoffDeniedReqs) Acknowledgements (cCdmaRpUpdHandoffDiscardedAcks) Initial Sent(cCdmaRpUpdHandoffInitTxdReqs) Retransmitted (cCdmaRpUpdHandoffReTxdReqs) Note: All are theresult handoffs. Number updated registrations sent was ofinter unacknowledgedsince system startup. A11 received that were with Status fieldset non-zero discarded because not denied
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_pcf_service_option_rp_session_update_stats.htm TITLE=CDMA PDSN PCF and Service Option based RP Session Update Statistics TEXT=CDMA PDSN PCF and Service Option-based RP Session Update Statistics Right-click the device, and select Configure list. from category row Monitor1 button. following information appears: A11 Sessions Transmitted (cCdmaPcfSoRpSessUpdTxdReqs) Acknowledged (cCdmaPcfSoRpSessUpdAcptdReqs) (cCdmaPcfSoRpSessUpdDeniedReqs) Registration Acknowledgements (cCdmaPcfSoRpSessUpdNotAckedReqs) Initial Updates (cCdmaPcfSoRpSessUpdInitTxdReqs) Re-transmitted (cCdmaPcfSoRpSessUpdReTxdReqs) Since Restart (cCdmaPcfSoRpSessUpdRcvdAcks) (cCdmaPcfSoRpSessUpdDiscardedAcks) total number of system was last restarted. received with Status field set non-zero, (indicating that corresponding accepted) denied sent, which were excluding updates, discarded
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_pcf_service_option_rp_session_update_stats_contd.htm TITLE=CDMA PDSN PCF and Service Option based RP Session Update Statistics Contd TEXT=CDMA PDSN PCF and Service Option-based RP Session Update Statistics Contd Right-click the device, and select Configure list. from category row Monitor2 button. following information appears: (cCdmaPcfSoRpSessUpdAlwaysOn) On Registration Updates TNPDIT downloaded (cCdmaPcfSoRpSessUpdRNPDIT) Parameter not (cCdmaPcfSoRpSessUpdParamNotUpdated) Unspecified Reason Failures (cCdmaPcfSoRpSessUpdReaUnSpecFails) (cCdmaPcfSoRpSessUpdMNAuthFails) Authentication Identity Mismatch (cCdmaPcfSoRpSessUpdIdMismatFails) Poorly Formed Request (cCdmaPcfSoRpSessUpdBadReqFails) total number of initial A11 sent due since system was last restarted. that failed being updated failure
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_pcf_so_ppp_stats.htm TITLE=PPP Setup Statistics TEXT=Use this option to view Packet Control Function (PCF) and Service Option (SO) based PPP Setup Statistics. Procedure access information: Right-click startup,the device select Monitor from popup menu. CDMA PDSN & Category any row following appears Active Connections(cCdmaPcfSoPppConnSuccesses) (cCdmaPcfSoPppCurrentConns) (cCdmaPcfSoPppConnInitiateReqs) Requests Sent Successful (cCdmaPcfSoPppConnSuccesses) Failed (cCdmaPcfSoPppConnFails) Negotiations Aborted (cCdmaPcfSoPppConnAborts) Number power-off currently connections. initiate out since system startup. that were successfully brought state have terminated prematurely due Mobile Node (MN)
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_pcf_so_rpreg_denied_stats.htm TITLE=RP Registration Denied Statistics TEXT=This dialog box displays Packet Control Function (PCF) and Service Option (SO) - based RP Registration Statistics. Navigation Right-click the device, select Monitor CDMA PDSN & from Category list. row button following information appears : Requests (cCdmaPcfSoRpRegDeniedReqs) (cCdmaPcfSoRpRegDiscardedReqs) New Connection (cCdmaPcfSoRpInitRegDeniedReqs) Re-registration (cCdmaPcfSoRpReRegDeniedReqs) De-registration (cCdmaPcfSoRpDeRegDeniedReqs) (cCdmaPcfSoRpHandoffRegDeniedReqs) A11 number since system startup. silently discarded startup, meant de-establishing R-P connections. refreshing established total handoff already existing session,
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_pcf_so_rpreg_failures.htm TITLE=RP Registration Failures TEXT=Use this option to view Packet Control Function (PCF) and Service Option (SO) based RP Registration Failures. Procedure access information: Right-click Authentication device select Monitor from popup menu. CDMA PDSN's & Statistics Category any row following appears Unknown (cCdmaPcfSoRpRegPcfUnknwnFails) Administrative (cCdmaPcfSoRpRegAdmnFails Insufficient Resource (cCdmaPcfSoRpRegNoRsrcFails) (cCdmaPcfSoRpRegMNAuthFails) ID Mismatch (cCdmaPcfSoRpRegIdMismatFails) (cCdmaPcfSoRpRegBadReqFails) Request Since system startup, number of requests that failed when address did not list configured PCFs unspecified reason. startup. sessions reached maximum, resources were insufficient. due Mobile Node (MN) failure identification badly formed
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_pcf_so_rpreg_failures_contd.htm TITLE=RP Registration Failures(contd..) TEXT=RP Registration Failures (contd..) Use this option to view Packet Control Function (PCF) and Service (SO) based Failures. Procedure access information: Right-click the device select Monitor from popup menu. CDMA PDSN/HA & Statistics Category any row following appears Unknown (cCdmaPcfSoRpRegUnkPdsnFails) Reverse Tunnel Setup (cCdmaPcfSoRpRegNoRevTunFails) T-Bit (cCdmaPcfSoRpRegTBitNSetFails) (cCdmaPcfSoRpRegBadCVSEFails) (CVSE) Number of requests that failed due address since system startup. failure Foreign Agent (FA) Home (HA) because required was not set unsupported vendor codes Customer/Vendor Specific Extension
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_pcf_so_rpreg_stats.htm TITLE=RP Registration Accepted Statistics TEXT=This dialog box displays Packet Control Function (PCF) and Service Option (SO)-based Radio Packet (RP) . Navigation Right-click theestablished device, select Monitor CDMA PDSN & Based from Category list. row button. following information appears : Requests Received (cCdmaPcfSoRpRegRcvdReqs) (cCdmaPcfSoRpRegAcptdReqs) New Connection (cCdmaPcfSoRpInitRegAcptdReqs) Re-registration (cCdmaPcfSoRpReRegAcptdReqs) De-registration (cCdmaPcfSoRpDeRegAcptdReqs) (cCdmaPcfSoRpHandoffRegAcptdReqs) A11 Registrations number since system startup. startup, meant de-establishing R-P connections. refreshing The total handoff already existing session,
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_pcf_so_rpupd_add_stats.htm TITLE=RP Update Additional Statistics TEXT=Use this to view Packet Control Function (PCF) and Service Option (SO) based RP UpdateStatistics. Procedure access information: Right-click (cCdmaPcfSoRpUpdOtherReaReqs) device select Monitor from popup menu. CDMA PDSN & Category any row following appears Registration Acknowledgements Received (cCdmaPcfSoRpUpdRcvdAcks) (cCdmaPcfSoRpUpdDiscardedAcks) Lifetime Expiry Updates (cCdmaPcfSoRpUpdRpLifeExpReqs) (cCdmaPcfSoRpUpdPPPtermReqs) Termination Reason Number of A11 since system startup. discarded startup, initial sent due expiry. result termination. reasons other than
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_pcf_so_rpupd_failures.htm TITLE=RP Update Failures TEXT=Use this option to view Packet Control Function (PCF) and Service Option (SO) based RP Update Failures. Procedure access information: Right-click Authentication device select Monitor from popup menu. CDMA PDSN & Statistics Category any row following appears Unknown (cCdmaPcfSoRpUpdReaUnSpecFails) Administrative (cCdmaPcfSoRpUpdAdmnFails) (cCdmaPcfSoRpUpdMNAuthFails) ID Mismatch (cCdmaPcfSoRpUpdIdMismatFails) (cCdmaPcfSoRpUpdBadReqFails) Request Number of registrations updates that failed unspecified reason since system startup. startup, due prohibition. Mobile Node (MN) failure. identity poorly formed request.
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_pcf_so_rpupd_stats.htm TITLE=RP Update Statistics TEXT=Use this to view Packet Control Function (PCF) and Service Option (SO) based RP UpdateStatistics. Procedure access information: Right-click the device select Monitor from popup menu. CDMA PDSN & Category any row following appears Updates Transmitted (cCdmaPcfSoRpUpdTxdReqs Accepted (cCdmaPcfSoRpUpdAcptdReqs) (cCdmaPcfSoRpUpdDeniedReqs) (cCdmaPcfSoRpUpdNotAckedReqs) Acknowledged Initial (cCdmaPcfSoRpUpdInitTxdReqs) Retransmitted (cCdmaPcfSoRpUpdReTxdReqs Number of A11 registration since system startup. startup, correspondingacknowledgements received with Status fieldset non-zero. sent when were excluding re-transmitted updates.
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_pcf_so_table.htm TITLE=CDMA PDSN PCF & SO Based Statistics TEXT=Use this option to view CDMA PDSN Packet Control Function (PCF) & Service Option (SO) Based Statistics. Procedure access : Right-click the device and select Monitor from popup menu. Category following information appears IP Address (cCdmaPcfSoRpRegIpAddr) (cCdmaPcfSoRpRegServiceOption) of that serves mobile node. received part registration request.
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_PPP_Abnormal_Release_Statistics.htm TITLE=CDMA PDSN PPP Abnormal Release Statistics TEXT=Use this option to view PPP abnormal statistics for a release. Procedure To access CDMA PDSN PPP abnormal information: Right-click (cCdmaPppOtherReasonReleases) device and select Monitor from popup menu. dialog box appears. Category displays: Released Due (cCdmaPppIdleTimeoutReleases) (cCdmaPppSessTimeoutReleases) L2TP (cCdmaPppL2tpTunnelReleases) Insufficient Resources (cCdmaPppInsufResReleases) Session Service Interruption (cCdmaPppSrvIntReleases) Unavailability (cCdmaPppSrvUnavailReleases) Reasons Number of connections idle timeout since system startup. tunnel was last restarted. unknown
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_PPP_Authentication_Failures.htm TITLE=CDMA PDSN PPP Authentication Failures TEXT=Use this option to view PPP authentication failures. Procedure To access CDMA PDSN PPP authentication information: Right-click device and select Monitor from popup menu. dialog box appears. Category displays: MSCHAP (cCdmaPppAuthChapFailures) PAP (cCdmaPppAuthPapFailures) (cCdmaPppAuthMschapFailures) EAP (cCdmaPppAuthEapFailures) MSID Tried (cCdmaPppAuthMsidAttempts) (cCdmaPppAuthMsidFailures) Note: The following variable available PSDNv2.0. (cCdmaPppAuthAAATimeouts) Timeout Number of times failed since system startup. requests sent was last restarted. that restarted, authentications due timeouts
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_PPP_Authentication_Statistics.htm TITLE=CDMA PDSN PPP Authentication Stats TEXT=CDMA PDSN PPP Authentication Statistics Use this option to view PPP authentication statistics. Procedure access information: Right-click device and select Monitor from popup menu. dialog box appears. Category displays: MSCHAP Requests Sent (cCdmaPppAuthChapAttempts) (cCdmaPppAuthChapSuccesses) PAP (cCdmaPppAuthPapAttempts) (cCdmaPppAuthPapSuccesses) (cCdmaPppAuthMschapAttempts) (cCdmaPppAuthMschapSuccesses) EAP (cCdmaPppAuthEapAttempts) (cCdmaPppAuthEapSuccesses) MSID (cCdmaPppAuthMsidSuccesses) Number of out since system startup. successes that were successfully was last restarted.
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_ppp_authentication_stats_contd.htm TITLE=CDMA PDSN PPP Authentication Statistics Contd TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: MSCHAP (cCdmaPppAuthChapTimeouts) PAP (cCdmaPppAuthPapTimeouts) (cCdmaPppAuthMschapTimeouts) Skipped (cCdmaPppAuthSkips) total number of timeouts due mobile node not responding request since system was last restarted. sending negotiations that authentication,
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_PPP_Compression_Statistics.htm TITLE=CDMA PDSN PPP Compression Statistics TEXT=Use this option to view PPP compression statistics. Procedure To access CDMA PDSN PPP compression statistics information: Right-click (cCdmaPppCompressOtherCons) device and select Monitor from popup menu. dialog box appears. Stats Category displays: Connections With Negotiated (cCdmaPppCompressNegoCons) Microsoft, (cCdmaPppCompressMsftCons) (cCdmaPppCompressAscendCons) Statck (cCdmaPppCompressStackCons) (cCdmaPppCompressDeflateCons) (PDSN MS) Number that type since system startup. stack deflate other than negotiated, Ascend,
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_PPP_Flow_Type_Statistics.htm TITLE=CDMA PDSN Flow Type Statistics TEXT=Use this option to view success flow statistics. Procedure To access CDMA PDSN flow type statistics information: Right-click the device and select Monitor from popup menu. dialog box appears. Category displays: (cCdmaFlowSimpleIpSuccesses) IP Flows Established Mobile (cCdmaFlowMobilIpSuccesses) (cCdmaFlowProxyIpSuccesses) VPDN (cCdmaFlowVpdnSuccesses) (cCdmaFlowSimpleIpFailures) (cCdmaFlowMobilIpFailures) (cCdmaFlowProxyIpFailures) (cCdmaFlowVpdnFailures) (cCdmaFlowUnknownTypeFailures) Number of simple that have been since system startup. proxy successfully Total setup requests, failed last reboot. with unknown type,
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_PPP_Miscellaneous_Stats.htm TITLE=CDMA PDSN PPP Miscellaneous Stats TEXT=CDMA PDSN PPP Miscellaneous Statistics Use this option to view PPP miscellaneous connections. Procedure access information: Right-click the device (Bandwidth select Monitor from popup menu. dialog box appears. Category displays: Connections With Negotiated MRRU (cCdmaPppNegoMrruCons) IPX Protocol) (cCdmaPppNegoIpxCons) (cCdmaPppNegoIpCons) VJ-Compression (cCdmaPppNegoVjCompCons) BAP (cCdmaPppNegoBapCons) (cCdmaPppConFormedBundles) Formed Number of that have since system startup. header Allocation bundles
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_ppp_misc_stats_contd.htm TITLE=CDMA PDSN PPP Miscellaneous Stats Contd TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: Compression Negotiation (cCdmaPppCompressNegoFailures) LCP (cCdmaPppTransmittedEchoReqs) Requests Transmitted (cCdmaPppRetransmittedEchoReqs) Reply (cCdmaPppReceivedEchoReplies) Timed Out (cCdmaPppEchoRequestTimeouts) Unidentified (cCdmaPppUnknownProtocolPktDiscards) Packets Discarded (cCdmaPppBadLengthPktDiscards) Length total number of negotiations that failed due failure since system was last restarted. retransmitted replies received stack protocol value not being identified, bad length,
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_PPP_Negotiate_Stats.htm TITLE=CDMA PDSN PPP Renegotiate Stats TEXT=CDMA PDSN PPP Renegotiation Statistics Use this option to view PPP renegotiation statistics. Procedure access information: Right-click (cCdmaPppRenegOtherReasonReqs) device and select Monitor from popup menu. dialog box appears. Category displays: (cCdmaPppRenegTotalReqs) Renegotiated (PDSN MS) by (cCdmaPppRenegByPdsnReqs) (cCdmaPppRenegByMobileReqs) During Setup stages) (cCdmaPppRenegLcpIpcpReqs) Due IPCP Address (cCdmaPppRenegAddrMismatchReqs) Reasons Note: The following variables are available PSDNv2.0. Successful Rerenegotiations (cCdmaPppRenegSuccesses) Failed Renegotiations (cCdmaPppRenegFailures) (cCdmaPppRenegConnectionsAborted) Number power-off connections either mobile node since system startup. requests initiated stratup. sent (LCP mismatch other than that were successfully brought active state terminated prematurely MN (Mobile Node) reasons.
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_PPP_Release_Statistics.htm TITLE=CDMA PDSN PPP Release Statistics TEXT=CDMA PDSN PPP Normal Release Statistics This dialog displays point-to-point protocol (PPP) statistics for release. Navigation Right-click either device, Commands select Monitor Device box appears. from Category list. following information appears: (cCdmaPppTotalReleases) Connections Released (PDSN MS) by (cCdmaPppPdsnReleases) (cCdmaPppMobileReleases) Due Ingress (cCdmaPppAddrFilterReleases) Filtering (cCdmaPppAdminReleases) LCP (cCdmaPppLcpTermReleases) Reqs (cCdmaPppDeregisterByPcfReleases) Registration Request Session (cCdmaPppLifetimeExpiryReleases) Expires number of active mobile node since system startup. The connection requests initiated releases address administrative term REQ total pcf sends deregistration lifetime expires,
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_ppp_renegotiation_stats_contd.htm TITLE=CDMA PDSN PPP Renegotiation Statistics Contd TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: Connections Renegotiated (cCdmaPppRenegAnidChanges) total number handoff. due access-network (anid) change during session
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_ppp_setup_a10_release_stats.htm TITLE=CDMA PDSN  PPP Setup A10 Release Stats TEXT=CDMA PDSN PPP Setup A10 Release Stats Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. from Category list. following information appears: before (cCdmaPppPreLCPPdsnA10Releases) Negotiation Phase PCF (cCdmaPppPreLCPPcfA10Releases) (cCdmaPppLCPPdsnA10Releases) (cCdmaPppLCPPcfA10Releases) Authentication (cCdmaPppAuthPdsnA10Releases) (cCdmaPppAuthPcfA10Releases) (cCdmaPppIPCPPdsnA10Releases) (cCdmaPppIPCPPcfA10Releases) total number of connections released by enters phase. during
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_ppp_setup_connection_term_stats_contd.htm TITLE=CDMA PDSN PPP Setup Connection Termination Stats TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: Conns Released of node MN (IPCP) (cCdmaPppNoRemoteIpAddressReleases) Terminated (RP), Disconnect (cCdmaPppLowerLayerReleaseFailures) Receiving Request (cCdmaPppIpcpPhaseReceivedTermreqs) Sending (cCdmaPppIpcpPhaseSentTermreqs) Authentication (cCdmaPppAuthPhaseReceivedTermreqs) (cCdmaPppAuthPhaseSentTermreqs) LCP (cCdmaPppLcpPhaseReceivedTermreqs) (cCdmaPppLcpPhaseSentTermreqs) Miscellaneous Reason (cCdmaPppConnectionOtherFailures) total number connections because mobile address rejects allocated by Packet Data Serving (PDSN). lower layer, such Radio disconnected. negotiations due term during Internet Protocol Control phase. reasons.
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_PPP_Setup_Failures.htm TITLE=CDMA PDSN PPP Setup Failures TEXT=Use this option to view PPP requests that are rejected. Procedure To access CDMA PDSN PPP setup failure information: Right-click authentication device and select Monitor from popup menu. dialog box appears. Category displays: (cCdmaPppConnectionFailures) Reqs Failed (cCdmaPppConnectionsAborted) LCP stage (cCdmaPppLcpFailures) AUTH (cCdmaPppAuthFailures) IPCP (cCdmaPppIpcpFailures) Note: following variables available PSDNv2.0. after Maximum Retransmission(cCdmaPppLcpFailuresMaxRetrans) Due Reason(cCdmaPppLcpFailuresUnknown) (cCdmaPppIpcpFailuresMaxRetrans) (cCdmaPppIpcpFailuresUnknown) Negotiations Aborted Prematurely Number power-off. times connections since system startup. startup, retransmissions. unknown reason. retransmission. terminated MN
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_PPP_Setup_Statistics.htm TITLE=CDMA PDSN PPP Setup Statistics TEXT=Use this option to view valid and accepted PPP setup requests. Procedure To access CDMA PDSN PPP setup information: Right-click authentication device select Monitor from popup menu. dialog box appears. Category displays: Currently Active (cCdmaPppCurrentConnections) (cCdmaPppConnectionInitiateReqs) Reqs Sent Succeessfully (cCdmaPppConnectionSuccesses) Entering LCP stage (cCdmaPppEnterLcpNums) AUTH (cCdmaPppEnterAuthNums) IPCP (cCdmaPppEnterIpcpNums) Number of connections. initiation out since system startup. Successfully made
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_ppp_setup_stats_contd.htm TITLE=CDMA PDSN PPP Setup Stats Contd TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (LCP) Negotiation (cCdmaPppLcpOptionIssueFailures) IPCP) (cCdmaPppIpcpOptionIssueFailures) Authentication Stage (cCdmaPppAuthMaxRetransFailures) Successfully Conn (cCdmaPppLcpSuccesses) (cCdmaPppIpcpSuccesses) (cCdmaPppAuthSuccesses) total number of connections terminated due Link Control Protocol options failure, such was call back user not negotiating option. Internet address negotiation. requests that failed after maximum retransmissions since system last restarted. entered successfully. succeeded authentication.
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_Registration_Denied_Stats.htm TITLE=CDMA PDSN Registration Denied Statistics TEXT=Use this option to view registration statistics of denied requests. Procedure To access registration information: Right-click these device and select Monitor from popup menu. dialog box appears. Stats Category displays: Request (cCdmaRpRegDeniedReqs) (cCdmaRpRegDiscardedReqs) New Disconnection (cCdmaRpInitRegDeniedReqs) Refreshing (cCdmaRpReRegDeniedReqs) (cCdmaRpDeRegDeniedReqs) Number A-11 since system startup. that are used deactivating established R-P connections. code field reply setup non-zero. discarded not returned establishing contain airlink record. The
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_Registration_Failures.htm TITLE=CDMA PDSN Registration Failures TEXT=Use this option to view rejected registration statistics. Procedure To access CDMA PDSN registration failure information: Right-click Authentication device and select Monitor from popup menu. dialog box appears. Category displays: (cCdmaRPRegBadRequestFailures) Failed Unspecified (cCdmaRPRegReasonlUnSpecFailures) Administrative (cCdmaRPRegAdminProhibFailures) (cCdmaRPRegInsuffResFailures) Resource (cCdmaRPRegMNAuthenFailures) Poor Identity (cCdmaRPRegIdentMismatchFailures) Number of requests when PCF (Packet Control Function) address not configured Data Serving Node) list reason since system startup. due prohibition maximum session poorly formed mismatch
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_Registration_Failures_contd.htm TITLE=CDMA PDSN Registration Failures (contd..) TEXT=Use this option to view rejected registration statistics. Procedure To access CDMA PDSN registration failure information: Right-click the device and select Monitor from popup menu. dialog box appears. Category displays: Request Failed (cCdmaRpRegUnknownPdsnFailures) PDSN/HA Reverse (cCdmaRPRegNoRevTunnelFailures) bit (cCdmaRPRegTBitNotSetFailures) (cCdmaRPRegBadCVSEFailures) Number of requests due unknown (Home Agent) address since system startup. FA (Foreign tunnel setup unset unsupported vendor code
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_session_flow_stats.htm TITLE=CDMA PDSN SESSION FLOW Statistics TEXT=CDMA PDSN Session Flow Statistics Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. from Category list. following information appears: (cCdmaPPPoGRESessionTotal) (cCdmaEstablishedSessions) (cCdmaHDLCoGRESessionTotal) Established (cCdmaReleasedSessions) (cCdmaMSIDFlowTotal) Flows (cCdmaVPDNFlowTotal) number of sessions currently with this system. since was last restarted. released using service.
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_session_update_denial_stats.htm TITLE=CDMA PDSN Session Update Denial Statistics TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: Registration (cCdmaRpSessUpdDeniedReqs) (cCdmaRpSessUpdDiscardedAcks) Ack Unknown (cCdmaRpSessUpdReasonUnSpecFailures) Incorrect Parameter (cCdmaRpSessUpdReasonParamNotUpdated) (cCdmaRpSessUpdMNAuthenFailures) Auth Identity (cCdmaRpSessUpdIdentMismatchFailures) Poor Request (cCdmaRpSessUpdBadReqFailures) number of A11 acknowledgements received with Status field set non-zero indicating that corresponding was denied since system last restarted. discarded registrations failed unspecified reason due parameters not updated mobile node authentication failure mismatch poorly formed
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_session_update_stats.htm TITLE=CDMA PDSN Session Update Statistics TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: Updates, (cCdmaRpSessUpdTransmittedReqs) Registration (cCdmaRpSessUpdAcceptedReqs) Unacknowledged (cCdmaRpSessUpdNotAckedReqs) Initial (cCdmaRpSessUpdInitTransmittedReqs) Retransmitted (cCdmaRpSessUpdReTransmittedReqs) Acknowledged (cCdmaRpSessUpdReceivedAcks) (cCdmaRpSessUpdAlwaysON) On (cCdmaRpSessUpdRNPDIT) number of A11 since system was last restarted. Acknowledgements received with Status field set zero (indicating that corresponding accepted) sent, which excluding re-transmitted due Note this count does not include any retransmissions. value downloaded,
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_Status_Change_Statistics.htm TITLE=CDMA PDSN Status Change Statistics TEXT=The CDMA PDSN Status Change Statistics category of the Monitor Device dialog box displays the handoff packet data servicing node (PDSN). Procedure Right-click device, then select appears. from list. following information appears: (cCdmaStatusIS2OOSes) (cCdmaStatusOOS2ISes) Total number changes service (IS). out (OOS).
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_Traffic_(Pkts)_Statistics.htm TITLE=CDMA PDSN Traffic (Pkts) Statistics TEXT=Use this option to view CDMA service level traffic statistics for packets. Procedure To access CDMA information: Right-click the device and select Monitor from popup menu. dialog box appears. Category Packet displays: Simple IP Data (cCdmaTransmittedSipPkts) (cCdmaReceivedSipPkts) Mobile (cCdmaTransmittedMipPkts) (cCdmaReceivedMipPkts) Proxy (cCdmaTransmittedPmipPkts) (cCdmaReceivedPmipPkts) Number of sent stations since system startup. received
PATH=/ciscoview/Routershare/monitor/cdma_pdsn_traffic_pkts_stats_contd.htm TITLE=CDMA PDSN Traffic (Pkts) Statistics Contd TEXT=Navigation Right click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cCdmaTransmittedSDBPkts) Marked Data Packets (cCdmaNoGREKeyPktDiscards) Key Missing Discarded (cCdmaNoSessionPktDiscards) Not Found Protocol (cCdmaInvGREProtoPktDiscards) Invalid Checksum (cCdmaInvCheckSumPktDiscards) total number of sent PCF since system was last restarted. because session due
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_Traffic_Statistics.htm TITLE=CDMA PDSN Traffic Statistics TEXT=CDMA PDSN Traffic (Octets) Statistics This dialog displays the CDMA service level traffic statistics for octets. Navigation Right-click device, and select Monitor Device box appears. from Category list. following information appears: Simple IP (cCdmaTransmittedSipKiloOctets) (cCdmaTransmittedMipKiloOctets) (cCdmaReceivedSipKiloOctets) Mobile (cCdmaReceivedMipKiloOctets) Proxy (cCdmaTransmittedPmipKiloOctets) (cCdmaReceivedPmipKiloOctets) (cCdmaTransmittedSDBOctets) Marked Data number of (in units 1024 octets) sent stations since system startup. received total PCF
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_Update_Additional_Statistics.htm TITLE=CDMA PDSN Update Additional Statistics TEXT=Use this option to view valid and accepted registration updates. Procedure To access CDMA PDSN update information: Right-click Reason(cCdmaRpUpdOtherReasonReqs) device select Monitor from popup menu. dialog box appears. Category displays: (cCdmaRpUpdReceivedAcks) Received Discarded(cCdmaRpUpdDiscardedAcks) (cCdmaRpUpdRpLifeExpReqs) Lifetime Expiry Termination(cCdmaRpUpdPPPtermReqs) &#150; Number of A-11 acknowledgements since system startup. discarded initial due RP expiration. Note: count does not include any re-transmissions. sent result termination The code field reply message set non-zero. reasons other than
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_Update_Failures.htm TITLE=CDMA PDSN Update Failures TEXT=Use this option to view registration updates that are rejected. Procedure To access CDMA PDSN registration failure information: Right-click Authentication device and select Monitor from popup menu. dialog box appears. Category displays: Request Failed Unspecified (cCdmaRpUpdReasonUnSpecFailures) Administrative (cCdmaRpUpdAdminProhibFailures) (cCdmaRpUpdMNAuthenFailures) Identity (cCdmaRpUpdIdentMismatchFailures) Poor (cCdmaRpUpdBadReqFailures) Number of updated requests. since system startup reason. due prohibition. failure. mismatch. poorly formed
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN_Update_Statistics.htm TITLE=CDMA PDSN Update Statistics TEXT=Use this option to view valid and accepted registration updates. Procedure To access CDMA PDSN update information: Right-click the device select Monitor from popup menu. dialog box appears. Category displays: Requests (cCdmaRpUpdTransmittedReqs) (cCdmaRpUpdAcceptedReqs) Denied(cCdmaRpUpdDeniedReqs) Acknowledged(cCdmaRpUpdNotAckedReqs) Acknowledged Initial (cCdmaRpUpdInitTransmittedReqs) Retransmitted (cCdmaRpUpdReTransmittedReqs) Numberof of A-11 since system startup. acknowledgements received, with status field set non-zero (indicating that corresponding accepted). denied), sent, which are excluding re-transmitted
PATH=/ciscoview/Routershare/monitor/CDMA_PDSN__Registration_Statistics.htm TITLE=CDMA PDSN Registration Accepted Statistics TEXT=Use this option to view registration statistics of valid and accepted requests. Procedure To access information: Right-click the device select Monitor from popup menu. dialog box appears. Stats Category displays: Request (cCdmaRpRegReceivedReqs) (cCdmaRpRegAcceptedReqs) New Connection (cCdmaRpInitRegAcceptedReqs) Refreshing (cCdmaRpReRegAcceptedReqs) Disconnection (cCdmaRpDeRegAcceptedReqs) Number A-11 received since system startup. code field reply setup zero. that are used establishing R-P connections. These contain airlink record. established deactivating
PATH=/ciscoview/Routershare/monitor/FA_Reg_Statistics.htm TITLE=Foreign Agent Registration Statistics TEXT=The dialog box displays the following information: Regn Requests Count Total (faRegRequestsReceived) Relayed (faRegRequestsRelayed) (faReasonUnspecified) Unspecified Regns Rejected(faVJCompressionUnavailable) Administratively (faAdmProhibited) (faInsufficientResource) Resources- (faMNAuthenticationFailure) Failure- (faRegLifetimeTooLong) Lifetime- (faPoorlyFormedRequests) well-formed (faEncapsulationUnavailable) Unavailable VJ Comp faHAUnreachable) Unreachable- (faRegRepliesRecieved) (faRegRepliesRelayed) (faHAAuthenticationFailure) (faPoorlyFormedReplies) number of valid received. too home by agent. denied agent- reason (codes 64) prohibited 65) -insufficient resources 66) -mobile node failed authentication 67) requested life long 69) -poorly 70) encapsulation 72) Van-Jacobson header compression 73) unreachable 80-95) replies from 68) reply 71)
PATH=/ciscoview/Routershare/monitor/foreign_agent_asym_link_support.htm TITLE=Foreign Agent Asymmetric Link Support TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. Configs from Category list. row Monitor button. following information appears: Registration Requests Received (CoA) (cmiFaCoaRegAsymLink) Specifies whether interface associated with this care-of-addresses should advertised. only not. If true, other configured will be
PATH=/ciscoview/Routershare/monitor/foreign_agent_visitors_stats_dereg.htm TITLE=Foreign Agent Visitors Statistics - De-Registration TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select Statistics-De-Registration from Category list. following information appears: (cmiFaDeRegRequestsReceived) Received (cmiFaDeRegRequestsRelayed) (cmiFaDeRegRequestsDenied) (cmiFaDeRegRequestsDiscarded) (cmiFaDeRegRepliesValidFromHA) (cmiFaDeRegRepliesValidRelayToMN) total number of requests by agent. relayed home denied discarded valid replies mobile node
PATH=/ciscoview/Routershare/monitor/foreign_agent_visitors_stats_init_reg.htm TITLE=Foreign Agent Visitors Statistics - Initial Registration TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select Statistics-Initial from Category list. following information appears: (cmiFaInitRegRequestsReceived) Received (cmiFaInitRegRequestsRelayed) (cmiFaInitRegRequestsDenied) (cmiFaInitRegRequestsDiscarded) (cmiFaInitRegRepliesValidFromHA) Reply (cmiFaInitRegRepliesValidRelayMN) List (cmiFaRegTotalVisitors) total number of requests by agent. relayed home denied discarded valid replies mobile nodes. current entries faVisitorTable which contains agent's visitor updates this table response events
PATH=/ciscoview/Routershare/monitor/foreign_agent_visitors_stats_rereg.htm TITLE=Foreign Agent Visitors Statistics Re-Registration TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select Statistics-Re-Registration from Category list. following information appears: (cmiFaReRegRequestsReceived) Received (cmiFaReRegRequestsRelayed) (cmiFaReRegRequestsDenied) (cmiFaReRegRequestsDiscarded) (cmiFaReRegRepliesValidFromHA) Reply (cmiFaReRegRepliesValidRelayToMN) total number of requests by mobile nodes. relayed agent. denied discarded valid replies home Re-egistration
PATH=/ciscoview/Routershare/monitor/foreign_agent_visitors_stat_reg_req_deny.htm TITLE=Foreign Agent Visitors Statistics Registration Requests Deny TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select Statistics-Registration from Category list. following information appears: (cmiFaReverseTunnelUnavailable) (cmiFaReverseTunnelBitNotSet) Unavailable Denied-No Bit MN (cmiFaMnTooDistant) Distant (Number of (cmiFaDeliveryStyleUnsupported) Denied-Challenge (cmiFaUnknownChallenge) (cmiFaMissingChallenge) Stale) Denied-Unsupported Vendor-ID ID by (cmiFaCvsesFromMnRejected) (cmiFaCvsesFromHaRejected) total number denied -- requested reverse tunnel (Code 74). mandatory not set 75). mobile node too 76). delivery style 79). challenge was unknown 104). missing 105). stale 106). unable interpret Vendor-CVSE-Type sent 100). replies home 101).
PATH=/ciscoview/Routershare/monitor/foreign_agent_visitors_stat_reg_req_from_entity.htm TITLE=Foreign Agent Visitors Statistics - Registration Request from Entity TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select Statistics-Registration Category list. followingin information appears: (cmiFaTotalRegRequests) with Vendor-NVSE-Type by MN-AAA (cmiFaNvsesFromMnNeglected) HA (cmiFaNvsesFromHaNeglected) MA (cmiFaTotalRegReplies) FA Authentication Fails (cmiFaMnFaAuthFailures) Denied Due (cmiFaMnAAAAuthFailures) total number of requests extension one sent mobile node-AAA agent: Unsupported Vendor-ID Unable interpret home received agent. replies failures.
PATH=/ciscoview/Routershare/monitor/GGSN_Access_Point.htm TITLE=GGSN Access Point TEXT=The GGSN Access Point Monitor dialog box lists the IP addresses allocated to MS. Procedure Right-click device and then select Statistics from Category list. row following information appears: No. of (cgprsAccPtIpAddrAllocations) Total PDP Context (cgprsAccPtMsActivatedPdps) Successfully Completed (cgprsAccPtSuccMsActivatedPdps) Dynamic (cgprsAccPtMsActivatedDynPdps) (cgprsAccPtSuccMsActivatedDynPdps) Deactivation (cgprsAccPtMsDeactivatedPdps) (cgprsAccPtSuccMsDeactivatedPdps) Number procedures initiated. by any this APN. When requests PLMN,
PATH=/ciscoview/Routershare/monitor/GGSN_Access_Point_Violation_and_Redirection.htm TITLE=GGSN Access Point Violation and Redirection TEXT=Use this dialog to view access point violation and inter mobile redirection statistics. Procedure Right-click the device then select Monitor Statistics from Category list. row following information appears: (cgprsAccPtSourceAddrViolTpdus) Address Destination (cgprsAccPtDestAddrViolTpdus) Redirected InterMobile Communication (cgprsAccPtRedirInterMobilTraffic) Number of upstream TPDU's (Payload GPRS Tunneling Protocol) that have been dropped due source as specified by cgprsAccPtVerifyUpStrTpduSrcAddr. cgprsAccPtVerifyUpStrTpduDstAddr. packets, pertaining communication, cgprsAccPtRedirInterMobilAddr.
PATH=/ciscoview/Routershare/monitor/ggsn_access_pt_throput_stat.htm TITLE=GGSN Access Point Throughput Statistics TEXT=Procedure Right-click the device and then select Monitor . Select category GGSN Access Point Throughput following information appears: (cgprsAccPtIndex) Collection (cgprsAccPtThruputInterval) locally unique identifier this GGSN. object represents time interval which are sampled. configuration out of scope CISCO-GGSN-MIB. covered
PATH=/ciscoview/Routershare/monitor/ggsn_access_pt_throput_stat_mon.htm TITLE=GGSN Access Point Throughput Statistics TEXT=Procedure Right-click the device and then select Monitor . Select category GGSN Access Point Throughput row following information appears: (cgprsAccPtThruPutLastCollected) Collected Time Upstream Bytes (cgprsAccPtUpstrByteCount) Downstream (cgprsAccPtDownstrByteCount) Packets (cgprsAccPtUpstrPktCount) (cgprsAccPtDownstrPktCount) This object represents delta value between when data been retrieved. total payload volume traffic APN last sampling period specified by cgprsAccPtThruputInterval. number of
PATH=/ciscoview/Routershare/monitor/ggsn_access_pt_traffic_stat.htm TITLE=GGSN Access Point Traffic Statistics TEXT=Procedure Right-click the device and then select Monitor . Select GGSN Access Point Statistics from Category list. row Monitor. following information appears: (cgprsAccPtRevUpstreamTrafficVol) Bytes (cgprsAccPtDownstreamPacketCount) (cgprsAccPtRevDownstrTrafficVol) Packets (cgprsAccPtUpstreamPacketCount) DHCP Address (cgprsAccPtDhcpAddrRequests) Succesful (cgprsAccPtSuccDhcpAddrRequests) (cgprsAccPtDhcpAddrReleases) This object indicates total payload volume upstream traffic. Data flow MS PDN. considered number downstream represents of APN. counter triggered when being routed request by Trigger Condition: create pdp message. successful release delete
PATH=/ciscoview/Routershare/monitor/GGSN_Charging.htm TITLE=GGSN Charging TEXT=The GGSN Charging category of the Chassis Monitoring dialog box displays GGSN Charging statistics. Note This can Number viewed if cGtpGSNService set 'ggsn'. Procedure Right-click device and then select from list. following information appears: State Transitions (cgprsCgDownTimes) Count Access Points (cgprsCgAccPtNum) (cgprsCgCdrOpenedNum) G-CDRs (cgprsCgCdrClosedNum) Current (cgprsCgContainerNum) (cgprsCgPendingMsgNum) Transmitted (cgprsCgSentMsgNum) (cgprsCgTotalCdrOpened) opened containers. created (cgprsCgTotalContainerCreated) times cgprsCgAlarmEchoFailure trap transitioned since system startup. which data collected. GGSN. when PDP. context activated. closed that have not been sent CG. encountering trigger conditions. In event remains active, new pending output messages. service was enabled. got response GGSN, either last cleared.
PATH=/ciscoview/Routershare/monitor/ggsn_charging_stats_contd.htm TITLE=GGSN Charging Statistics Contd TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: Received (cgprsCgTotalServiceRecords) Reflects total number of service-aware records created GGSN, either since system startup time feature enabled. Trigger Condition: This counter triggered when closed.
PATH=/ciscoview/Routershare/monitor/ggsn_csg_stats.htm TITLE=GGSN CSG Statistics TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cGgsnSACsgOutboundMsgs) Packets Sent (cGgsnSACsgOutboundOctets) (cGgsnSACsgInboundMsgs) Received (cGgsnSACsgInboundOctets) Initial (cGgsnSACsgQuotaReturns) Grant (cGgsnSACsgServiceAuthReqs) Re-Authorization Request (cGgsnSACsgServiceAuthResps) (cGgsnSACsgServiceReAuthReqs) Return Messages aggregate number of echo request, response, node alive sent. terms octets. received. requests. by Content Gateway. quota particular category. allows only synchronous grants (that is, due explicit it). responses given service reauthorization Indicates verification. sends message, when validity timer expires there server. On receipt returns usage
PATH=/ciscoview/Routershare/monitor/ggsn_csg_stats_contd.htm TITLE=GGSN CSG Statistics Contd TEXT=Navigation Right click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: QS (cGgsnSACsgQuotaReturnReqs) Return Messages (cGgsnSACsgQuotaPushResps) Responses (cGgsnSACsgServiceStopMsgs) (cGgsnSACsgServiceStopReqs) Received (cGgsnSACsgQuotaPushMsgs) (cGgsnSACsgQuotaPushRsps) GTP (cGgsnSACsgGtpAcks) Indicates number of quota. requests. by server. may sends this message, cause Content Gateway. (CSG) unused target service. when validity timer, expires; triggers Credit Control Request (CCR) update. Diameter Application (DCCA) grants response. request. pushed purpose mainly convey session. ID server, associated that can save subsequent transactions originates. (stop) summarizes situations under which user disconnected service: removes RADIUS Accounting each had active idle expires, category. reports usage remaining sent GGSN. conditions: returns non-zero blacklisted unknown. retransmit (Tx) with client, expires. not required. responds element header success failure. whose must statically configured, If reject 255 its level acknowledgements some (e.g., request). do contain index TLVs, are helpful lookup. However, they sequence matches corresponding
PATH=/ciscoview/Routershare/monitor/GGSN_Current_State.htm TITLE=GGSN Current State TEXT=GGSN Statistics The GGSN Statistics category of the Chassis Monitoring dialog box lists details of the GGSN. Note This can number viewed if cGtpGSNService set 'ggsn'. Procedure Right-click device and then select from list. following information appears: PDP Contexts (cGgsnTotalCreatedPdps) (cGgsnTotalDeletedPdps) (cGgsnTotalNetworkInitPdps) Initiated PPP-Regen (cGgsnTotalPppPdpsCreated) (cGgsnTotalPppPdpsDeleted) Rejected requests (unavailable resource) (cGgsnOutofResourcePppRegenPdps) (cGgsnDroppedPppRegenPdps) (max regeneration. reached) (cGgsnActiveNetworkInitPdps) (cGgsnActivePppPdps) regenerated (cGgsnActivePppRegenPdps) (cGgsnPendingPppRegenPdps) created. since system startup. deleted. by PDN that were activated context due dropped threshold limit being maximum sessions. allowed network are currently active. pending
PATH=/ciscoview/Routershare/monitor/GGSN_GTP.htm TITLE=GGSN GTP TEXT=The GGSN GTP category of the Chassis Monitoring dialog box lists GGSN GTP statistics. Note This dialog can Number viewed if cGtpGSNService set 'ggsn'. Procedure Right-click device and then select from list. following information appears: Failures (cGtpPathFailureOccurrences) (cGtpTotalDroppedPackets) Dropped times that any one GSN's peers failed respond Echo Request message during waiting intervals. packets were received but could not processed hence since system started.
PATH=/ciscoview/Routershare/monitor/GGSN_GTP_Director_Status.htm TITLE=GGSN GTP Director Status TEXT=The GGSN GTP Director Status category of the Chassis Monitoring dialog box lists GGSN GTP Director status. Note This can Number viewed if cGtpGSNService set 'ggsn'. Procedure Right-click device and then select from list. following information appears: (cgdPendingPdps) create PDP requests Unique forwarded (cgdCreatePdpRequestFwded) (cgdTotalCreatePdpRequestFwded) rejected (cgdCreateRequestRejected) (cgdTotalUnsupportedMessages) signaling messages dropped. (cgdPdpRequestDropped) whose connection retry timer not expired. by GDM. GGSN. does includes retransmissions. any signalling other than request. receives unsupported message, will gives total received due routing failures, which occur, unable pass packet IP.
PATH=/ciscoview/Routershare/monitor/GGSN_GTP_Director_Status_.htm TITLE=GGSN GTP Director Status TEXT=The GGSN GTP Director Status category of the Chassis Monitoring dialog box lists GGSN GTP Director status. Note This can Number viewed if cGtpGSNService set 'ggsn'. Procedure Right-click device and then select from list. following information appears: (cgdPendingPdps) create PDP requests Unique forwarded (cgdCreatePdpRequestFwded) (cgdTotalCreatePdpRequestFwded) rejected (cgdCreateRequestRejected) (cgdTotalUnsupportedMessages) signaling messages dropped. (cgdPdpRequestDropped) whose connection retry timer not expired. by GDM. GGSN. does includes retransmissions. any signalling other than request. receives unsupported message, will gives total received due routing failures, which occur, unable pass packet IP.
PATH=/ciscoview/Routershare/monitor/GGSN_GTP_VS_PDP_Context.htm TITLE=GTP VS PDP Context TEXT=Use this dialog to view active Packet Data Protocol (PDP) traffic for various GTP versions. Procedure In the Chassis view, right-click device and select Monitor from popup menu. following information appears: v0 (cGgsnActiveGtpVersion0Pdps) v1 (cGgsnActiveGtpVersion1Pdps) Number of contexts.
PATH=/ciscoview/Routershare/monitor/GGSN_Incoming_PDP_Statistics.htm TITLE=Incoming PDP Statistics TEXT=GGSN Incoming PDP Statistics Use this dialog to view incoming Packet Data Protocol (PDP) error statistics. Procedure the Chassis view, right-click device and select Monitor from popup menu. following information appears: TFTs (cGgsnTftSemanticErrorPdps) (cGgsnTftSyntacticErrorPdps) (cGgsnPktFilterSemanticErrorPdps) (cGgsnPktFilterSyntacticErrorPdps) Number of received context messages that had with semantic errors. syntactic filters
PATH=/ciscoview/Routershare/monitor/ggsn_psd_stats.htm TITLE=GGSN PSD Statistics TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cPsdClientDSWriteReq) Data Record Transfer Request (cPsdClientDSReadReq) Retransmission (cPsdClientDSRdWrRetrans) State Transitions (cPsdClientDSDiskFullTrans) number of (for write) messages sent server. This counters incremented when FIFO client. read) (retransmission) does not differentiate between original request. two previous can used tally received by read/write are made 'disk available' full'. receives indication
PATH=/ciscoview/Routershare/monitor/GGSN_QOS.htm TITLE=GGSN QOS TEXT=The GGSN QOS category of the Chassis Monitoring dialog box lists the quality of service (QOS) statistics. Note This canonical(2). best-effort viewed if cGtpGSNService set 'ggsn'. Procedure Right-click device (cggsnQosCurrentUsedBandwidth) then select from list. following information appears: Resource Used (cggsnQosPremiumMeanThroughput) Class (cggsnQosNormalMeanThroughput) Normal Best-effort (cggsnQosBestEffortMeanThroughput) Amount bandwidth GGSN. object retrieved only cggsnQosMappingMethod Sum mean throughput premium users
PATH=/ciscoview/Routershare/monitor/GGSN_QOS_Mapping.htm TITLE=GGSN QOS Mapping TEXT=The GGSN QOS Mapping dialog box lists the active PDP contexts that have cggsnQosClass. Note This dialog can Number viewed if cGtpGSNService set Monitor 'ggsn' Procedure Right-click device. and then select Configure , Category double-click from list. row table button. following information appears: Count (cggsnQosCurrentPdps) of class.
PATH=/ciscoview/Routershare/monitor/ggsn_quota_server_error_stats.htm TITLE=GGSN Quota Server Error Statistics TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cGgsnSAQsRcvdNegativeResponses) (cGgsnSAQsUnknownResponses) (CSG). Pending (cGgsnSAQsRequestsUnreplied) Improper Sequence (cGgsnSAQsSeqnumFailures) (cGgsnSAQsDroppedMsgs) Messages (cGgsnSAQsUnknownMsgs) QS (cGgsnSAQsIEErrorMsgs) number. of negative responses received Content Service Gateway. sends GTP acknowledgement failure cause code push response. requests that are waiting without uses different pools numbers, management path messages. To these utilizes manager. For messages, start 1, increases till 65535, then wraps around. dropped verifies header before queuing. inbound process. If any field bad, drops unknown server. by error.
PATH=/ciscoview/Routershare/monitor/ggsn_quota_server_error_stats_contd.htm TITLE=GGSN Quota Server Error Statistics Contd TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cGgsnSAQsBadSrcAddressMsgs) Source Higher (cGgsnSAQsVersionUnSupportedMsgs) TLV. (cGgsnSAQsMandTlvMissingMsgs) (cGgsnSAQsMandTlvIncorrectMsgs) Unexpected Length (cGgsnSAQsInvalidMsgFormats) CSG (cGgsnSAQsNoResponseToMsgs) Response number of messages. with bad address. version. Content Service Gateway use zero (0) GTP communication between them. If sends version, will respond not supported sent by mandatory missing; these are dropped. incorrect length. drops which there after n3/t3 retransmission.
PATH=/ciscoview/Routershare/monitor/ggsn_quota_server_stats.htm TITLE=GGSN Quota Server Statistics TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cGgsnSAQsRcvdRequests) Received (CSG). (cGgsnSAQsSentResponses) (cGgsnSAQsRcvdResponse) (cGgsnSAQsSentRequests) Echo request. / Node Alive (cGgsnSAQsRcvdPathRequests) Management (cGgsnSAQsRcvdPathResponses) QS Message (cGgsnSAQsSentPathRequests) (cGgsnSAQsSentPathResponses) Indicates number profile messages: Content Service Gateway. counter. incremented when receives these User reauthorization responses corresponding requests. sent every server, such as: return stop disconnect Both use echoes detect health path between them. sends real address while sending server. by check made with valid restart
PATH=/ciscoview/Routershare/monitor/GGSN_Received.htm TITLE=GGSN Received TEXT=The GGSN Received category of the Chassis Monitoring dialog box lists statistics of what the GGSN received. Note This can Number viewed Notifications cGtpGSNService set 'ggsn' Procedure Right-click device Mandatory then select following information appears: GTP. (cGgsnReceivedSigMessages) (cGgsnUnexpectedSigMessages) G-PDU (cGgsnReceivedGPDUs) Total bytes (cGgsnHCReceivedGPDUOctets) (cGgsnUnexpectedGPDUs) PDPs (cGgsnActivationRejectedPdps) (cGgsnOutOfResourcePdps) Resources Wrong Value (cGgsnParserErrorMessages) (cGgsnGeneratedNotifs) Less Severe (cGgsnIgnoredAlarms) signalling messages. GGSN. unexpected (cGgsnReceivedGPDUOctets) sent messages, example non existent contexts ACL denial, which activation request was rejected due its running out transmitting packets. Examples would be: memory reached limit All dynamic addresses are occupied with value. Reasons include: optional element duplicated, missing, unknown, incorrect, order. too short hold header unsupported version. type unknown. cGgsnNotification that have been generated. since sysUpTime. alarms sysUpTime, were than cGgsnNotifLeastSeverLevel,
PATH=/ciscoview/Routershare/monitor/ggsn_redundancy_stats.htm TITLE=GGSN Redundancy Statistics TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cGgsnTotalMessages) (PDP) (cGgsnContextSetupMessages) Modify/Update (cGgsnContextModifyMessages) Delete (cGgsnContextRemoveMessages) SGSN/GGSN (cGgsnPathSetupMessages) (cGgsnPathModifyMessages) Removal (cGgsnPathRemoveMessages) Maintains counter (of total number messages. all kinds. Packet Data Protocol context checkpointed. standby. only after goes active. setup Trigger Condition: This updated, whenever When modified categories get affected new quota assigned them. must object modify that are incremented deleted, deletion event standby, so corresponding backup well. removed. which every any kind, such create/delete on) indicate presence other GSNs. between they transmit contains path. GGSN. sent. element (IE) recovery used restart change related will Keeps track As long remains established, alive. last released echo timer not enabled, started within expected keep live; expires, triggered
PATH=/ciscoview/Routershare/monitor/ggsn_redundancy_stats_contd.htm TITLE=GGSN Redundancy Statistics Contd TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following: information appears: Charging Gateway (cGgsnCGFReadyMessages) (cGgsnInternalStateMsgs) Change (cGgsnCGFModifyMessages) Removal (cGgsnCGFRemoveMessages) GSN/CGF CAC (cGgsnSlbCacFailures) (cGgsnSlbSessionFailures) sent gateway. GTP protocol used between them. This object consists of total number ready messages. Trigger Condition: counter incremented whenever checkpointed standby. Significant related state. must GGSN. indicates modify received. triggered there Counts all responsible removal. context deleted. sends certain other GSNs (SGSN) CGF. On failover, remain consistent. includes element recovery path management, local record sequence ID, so on. each these kinds Tracks failure notifications SLB. session
PATH=/ciscoview/Routershare/monitor/ggsn_service_aware_fail_stats.htm TITLE=GGSN Service Aware Failure Statistics TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cGgsnSATotalGgsnFailures) (CSG), (cGgsnSATotalCsgFailures) (DCCA) (cGgsnSATotalDccaFailures) (cGgsnSARejDccaFailures) (cGgsnSARejCsgFailures) number of failures, such as communicating with Content Gateway receiving response Diameter Credit Control Application server. quota Packet Data Protocol (PDP) sessions that have been rejected due failure. PDPs
PATH=/ciscoview/Routershare/monitor/ggsn_service_aware_stats_1.htm TITLE=GGSN Service Aware Statistics 1 TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (APNs). (cGgsnSANumServiceAwareApns) (cGgsnSATotalGgsnEvents) CSG (cGgsnSATotalCsgEvents) (DCCA) (cGgsnSATotalDccaEvents) (cGgsnSATotalCreatedCategories) (cGgsnSATotalCreatedSyncObjs) Synchronization Objects Authorization (cGgsnSATotalServiceAuthMsgs) (cGgsnSATotalServiceStopMsgs) (cGgsnSATotalQuotaGranted) Granted number of Access Point Names events. Content Gateway. Diameter Credit Control Application categories. that created. will not statically configured GGSN. learns about particular PDP session dynamically by server get each triggers, which keep track affected their current state. object. contains: Type List messages sent stop received. total amount quota granted.
PATH=/ciscoview/Routershare/monitor/ggsn_service_aware_stats_2.htm TITLE=GGSN Service Aware Statistics 2 TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: Blacklisted (cGgsnSATotalBlackListCategories) Reauthorization (cGgsnSATotalRAREvents) (cGgsnSATotalDeletedCategories) PDPs (cGgsnSATotalDeletePdps) Prepaid (cGgsnSAFinalConvertToPostpaidPdps) after (cGgsnSATotalQuotaPushAcks) Usage Synchronization (cGgsnSATotalDeletedSyncObjects) Ack Received Push CSG (cGgsnSATotalServiceReAuthMsgs) (cGgsnSATotalQuotaReturns) Message number of categories that blacklisted. (RAR) events. deleted. converted postpaid reporting final quota. steps involved are: Send return request Content Gateway. and, if there object. Gn side trigger, update response sync Create new this event. Make part have been objects acknowledgements Re-authorization messages sent by
PATH=/ciscoview/Routershare/monitor/ggsn_service_aware_stats_3.htm TITLE=GGSN Service Aware Statistics 3 TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from (cGgsnSACategoryFsmRtnErrors) list. following information appears: Terminated (cGgsnSATotalTerminateCategories) (cGgsnSATotalUnknownCategories) (cGgsnSATotalRatingChanges) Condition Change Events (cGgsnSATotalPostpaidConversions) (cGgsnSATotalPrepaidUsers) (cGgsnSATotalPostpaidUsers) (cGgsnSATotalDummyQuotas) Quota Pushed Users FSM. Errors number of categories. that terminated. unknown rating events. typically update request SGSN involving QOS change. conversions prepaid postpaid. total amount dummy Content Gateway. users. returned by category
PATH=/ciscoview/Routershare/monitor/ggsn_sgsn_stat.htm TITLE=GGSN - SGSN Statistics TEXT=Procedure Right-click the device and then select Monitor . Select GGSN - SGSN Statistics from the Category drop-down box. following information appears: Remote (cGtpPathAddress) (cGtpPathPort) Collection (cGgsnSgsnThruPutInterval) An address that uniquely identifies node. which this path established. objects port values of zero invalid. should be one set cGgsnThruputIntervalOne cGgsnThruputIntervalTwo except '0', means throughput disabled.
PATH=/ciscoview/Routershare/monitor/ggsn_sgsn_stat_mon.htm TITLE=GGSN - SGSN Statistics - Monitor TEXT=GGSN - SGSN Throughput Statistics Procedure Right-click the device and then select Monitor . Select GGSN from Category list. row following information appears: Data (cGgsnSgsnThruPutLastCollected) Collected Upstream Packets Sent (cGgsnSgsnUpStreamPktCnt) Bytes (cGgsnSgsnUpStreamByteCnt) Downstream (cGgsnSgsnDownStreamPktCnt) (cGgsnSgsnDownStreamByteCnt) This object represents delta value between time when retrieved. total number of path. flow MS PDN considered traffic.
PATH=/ciscoview/Routershare/monitor/GGSN_Transmitted.htm TITLE=GGSN Transmitted TEXT=The GGSN Transmitted category of the Chassis Monitoring dialog box lists statistics of what the GGSN transmitted. Note This can Number viewed if cGtpGSNService set 'ggsn'. Procedure Right-click device and then select following information appears: GTP (cGgsnSentSigMessages) G-PDU (cGgsnSentGPDUs) Total bytes, sent (cGgsnHCSentGPDUOctets) (cGgsnSentGPDUOctets) signalling messages. GGSN. messages,
PATH=/ciscoview/Routershare/monitor/HA_Reg_Statistics.htm TITLE=Home Agent Registration Statistics TEXT=The dialog box displays the following information: Regns Accepted (haRegistrationAccepted)Vs Regn Requests Received (haRegRequestsReceived): Mobility (haMultiBindingUnsupported) Unsupported (haReasonUnspecified) Unspecified Administratively (haAdmProhibited) (haInsufficientResource) Resources (haMNAuthenticationFailure) haFAAuthenticationFailure) Failure FA Identification (haIDMismatch) (haPoorlyFormedRequest) Formed Innumerous (haTooManyBindings) (haUnknownHA) Address Unknown Gratuition (haGratuitiousARPsSent) (haProxyARPsSent) Proxy Sent(haRegRepliesSent)Vs DeRegn (haDeRegRepliesSent): (haDeRegRequestsReceived): (haRegistrationAccepted): Total number of (requests by (code 130) agent. -- simultaneous bindings 131) denied reason 128) prohibited 129) insufficient resource mobile nodes. failed authentication foreign 132) mismatch 133) poorly 134) too many 135) 136) sent behalf Sent(haRegRepliesSent): replies response deregister. with lifetime zero deregister)
PATH=/ciscoview/Routershare/monitor/HA_Reg_Statistics_Per_Node.htm TITLE=Home Agent Registration Statistics Per Node TEXT=The dialog box displays the following information: Accepted Requests Count (haServiceRequestsAccepted) Denied (haServiceRequestsDenied) (haOverallServiceTime) Time Total number of service mobile by agent. (code 0 + 1) sum registrations with 128 through 159) time, seconds, that has been accumulated since last rebooted.
PATH=/ciscoview/Routershare/monitor/High_Priority_Traffic_Media_Dependent_Statistics.htm TITLE=High Priority Traffic TEXT=Use this option to monitor high priority traffic reception statistics from physical medium-dependent layer information: current interval. of particular side SRP interface. Procedure access Right-click the port and select Interface pop-up menu. Media dialog box appears. Rx Category displays: information. Unicast Packets (SrpRingCurUcastHighPriPktsIn) (SrpRingCurUcastHighPriOctetsIn) Multicast (SrpRingCurMcastHighPriPktsIn) (SrpRingCurMcastHighPriOctetsIn) Number high-priority received during 15-minute octets Related Topics Using CiscoView Main Menu Selecting Components Configuring Devices Monitoring
PATH=/ciscoview/Routershare/monitor/High_Priority_Traffic_Physical_Layer.htm TITLE=High Priority Traffic TEXT=Use this option to monitor statistics of high priority traffic transmission to physical medium-dependent layer information: current interval. particular side SRP interface. Procedure access Right-click the port and select Interface from pop-up menu. Media Dependent dialog box appears. Tx Category displays: information. Unicast Packets (SrpRingCurUcastHighPriPktsOut) (SrpRingCurUcastHighPriOctetsOut) Multicast (SrpRingCurMcastHighPriPktsOut) (SrpRingCurMcastHighPriOctetsOut) Number high-priority going during 15-minute octets Related Topics Using CiscoView Main Menu Selecting Components Configuring Devices Monitoring
PATH=/ciscoview/Routershare/monitor/home_agent_redundancy_stats_ack.htm TITLE=Home Agent Redundancy Statistics - Acknowledgement TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cmiHaRedunReceivedBIAcks) (cmiHaRedunDroppedBIAcks) Security (cmiHaRedunSecViolations) total number of acknowledgements received response binding replies sent by agent. dropped since there are corresponding it. violations caused processing packets peer can occur reasons: Authenticator value invalid. stored identification field
PATH=/ciscoview/Routershare/monitor/home_agent_redundancy_stats_bind_info.htm TITLE=Home Agent Redundancy Statistics - Binding Information TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select –Binding from Category list. following appears: (cmiHaRedunReceivedBIReps) Replies (cmiHaRedunDroppedBIReps) (cmiHaRedunSentBIAcks) (cmiHaRedunSentBIReps) Requests (cmiHaRedunReceivedBIReqs) No Acknowledgement (cmiHaRedunFailedBIReps) (cmiHaRedunTotalSentBIReps) total number of received standby agent. dropped since there corresponding request sent acknowledgements response which including retransmissions same reply.
PATH=/ciscoview/Routershare/monitor/home_agent_redundancy_stats_bind_updates.htm TITLE=Home Agent Redundancy Statistics - Binding Updates TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select Statistics-Binding from Category list. following information appears: (cmiHaRedunSentBUs) Updates-No (cmiHaRedunReceivedBUAcks) (cmiHaRedunFailedBUs) (cmiHaRedunReceivedBUs) (cmiHaRedunTotalSentBUs) Bindings (cmiHaRedunSentBUAcks) Requests (cmiHaRedunSentBIReqs) (cmiHaRedunFailedBIReqs) (cmiHaRedunTotalSentBIReqs) total number of sent standby agent. which acknowledgements received response including retransmissions same update. reply active
PATH=/ciscoview/Routershare/monitor/home_agent_reg_proc_stats_init_reg.htm TITLE=Home Agent Registration Processing Statistics - Initial Registration TEXT=Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select Home Agent Statistics-Initial from Category list. following information appears: No (cmiHaEncapUnavailable) (cmiHaNAICheckFailures) Check Fails (cmiHaInitRegRequestsReceived) Received (cmiHaInitRegRequestsAccepted) (cmiHaInitRegRequestsDenied) (cmiHaInitRegRequestsDiscarded) MB haMobilityBindingTable. Entries (cmiHaRegTotalMobilityBindings) total number of requests denied by due unsupported encapsulation. failures. agent. accepted reasons which denies include: Cannot allocate IP address MN. parsing failed. length. exceeds packet discarded discards mobile service enabled. HA-CHAP authentication nodes. security association retrieval current contains agent's mobility binding updates this table response events
PATH=/ciscoview/Routershare/monitor/home_agent_reg_proc_stats_reg_req.htm TITLE=Home Agent Registration Processing Statistics - Registration Requests TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select – from Category list. following information appears: (cmiHaRegTotalProcLocRegs) (cmiHaRegMaxProcLocInMinRegs) Processed (cmiHaRegProcLocInLastMinRegs) by HA-CHAP (cmiHaRegTotalProcByAAARegs) (cmiHaRegMaxProcByAAAInMinRegs) Minute (cmiHaRegProcAAAInLastByMinRegs) (cmiHaRegRequestsReceived) (cmiHaRegRequestsDenied) (cmiHaRegRequestsDiscarded) total number of agent. Includes only those that were authenticated locally maximum during last server. minute. received initial requests, re-registration de-registration requests. denied Reasons which denies include: Cannot allocate IP address mobile node. parsing failed. NAI length. exceeds packet discarded discards service enabled. authentication security association retrieval
PATH=/ciscoview/Routershare/monitor/home_agent_reg_proc_stats_reg_req_deny.htm TITLE=Home Agent Registration Processing Statistics - Registration Request - Deny TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select Statistics-Registration from Category list. followingin information appears: Vendor-CVSE-Type (cmiHaCvsesFromFaRejected) FA Vendor-NVSE-Type. MN (cmiHaNvsesFromMnNeglected) (cmiHaNvsesFromFaNeglected) (cmiHaMnHaAuthFailures) Fails (cmiHaMnAAAAuthFailures) total number of requests denied by -- Unsupported Vendor-ID. unable interpret sent foreign (Code 141). with extension, one mobile node-AAA agent: due authentication failures.
PATH=/ciscoview/Routershare/monitor/home_agent_reg_proc_stats_rereg.htm TITLE=Home Agent Registration Processing Statistics - Re-registration TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select –Re-registration from Category list. following information appears: Re-Reg (cmiHaReRegRequestsReceived) (cmiHaReRegRequestsAccepted) (cmiHaReRegRequestsDenied) (cmiHaReRegRequestsDiscarded) De-Reg (cmiHaDeRegRequestsReceived) (cmiHaDeRegRequestsAccepted) (cmiHaDeRegRequestsDenied) (cmiHaDeRegRequestsDiscarded) total number of requests received by agent. accepted denied reasons which denies include: Cannot allocate IP address MN. parsing failed. NAI length. exceeds packet discarded discards mobile service enabled. HA-CHAP authentication node security association retrieval de-registration
PATH=/ciscoview/Routershare/monitor/home_agent_reg_proc_stats_rev_tunnel.htm TITLE=Home Agent Registration Processing Statistics - Reverse Tunnel TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select –Reverse from Category list. following information appears: No-T (cmiHaReverseTunnelUnavailable) (cmiHaReverseTunnelBitNotSet) (cmiHaEncapsulationUnavailable) Vendor-CVSE-Type (cmiHaCvsesFromMnRejected) total number of requests denied by -- requested unavailable (Code 137). mandatory bit not set 138). encapsulation 72). Unsupported Vendor-ID unable interpret sent mobile node 140).
PATH=/ciscoview/Routershare/monitor/home_agent_reg_stats_per_node.htm TITLE=Home Agent Registration Statistics per Node TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. Request Configs from Category list. row Monitor button. following information appears: (cmiHaRegServAcceptedRequests) Accepted (cmiHaRegServDeniedRequests) total number of service requests mobile by (Code 0 + 1). denied (sum all registrations with 128 through 159).
PATH=/ciscoview/Routershare/monitor/invalid_rp_reg_update_ack_err_stats.htm TITLE=Invalid RP Registration Update Ack Errors Stats TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cCdmaRegUpdAckInvPakLenErrs) (cCdmaRegUpdAckInvProtocolErrs) Value Authentication (cCdmaRegUpdAckInvRUAEKeyErrs) (cCdmaRegUpdAckInvSPIErrs) (cCdmaRegUpdAckInvConnectionIDErrs) (cCdmaRegUpdAckInvMNIDErrs) (cCdmaRegUpdAckInvMNIDTypeErrs) Type (cCdmaRegUpdAckInvMSIDLenErrs) Length number of packet while parsing since system was last restarted. Session Specific Extension key
PATH=/ciscoview/Routershare/monitor/invalid_rp_session_update_ack_errors.htm TITLE=Invalid RP Session Update Ack Errors Stats TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cCdmaSessUpdAckInvPakLenErrs) (cCdmaSessUpdAckInvProtocolErrs) Value Authentication (cCdmaSessUpdAckInvRUAEKeyErrs) (cCdmaSessUpdAckInvSPIErrs) (cCdmaSessUpdAckInvConnectionIDErrs) (cCdmaSessUpdAckInvMNIDErrs) (cCdmaSessUpdAckInvMNIDTypeErrs) Type (cCdmaSessUpdAckInvMSIDLenErrs) Length number of packet while parsing since system was last restarted. Specific Extension key Registration mobile node
PATH=/ciscoview/Routershare/monitor/ip_pool_group_statistics.htm TITLE=IP Pool Group Statistics TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. row Monitor button. following information appears: Available Address (cIpLocalPoolGroupFreeAddrs) Allocated (cIpLocalPoolGroupInUseAddrs) number of addresses use group. that have been
PATH=/ciscoview/Routershare/monitor/ip_pool_statistics.htm TITLE=IP Pool Statistics TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. row Monitor Button. following information appears: Available Address (cIpLocalPoolFreeAddrs) Used (cIpLocalPoolInUseAddrs) number of addresses. use range being
PATH=/ciscoview/Routershare/monitor/Low_Priority_Traffic_Media_Dependent_Interval.htm TITLE=Low Priority Traffic TEXT=Use this option to monitor low priority traffic reception statistics from physical medium-dependent layer information: current interval. particular side of SRP interface. Procedure access Right-click the port and select Interface pop-up menu. Media Dependent dialog box appears. Rx Category displays: information. Unicast Packets (srpRingCurUcastLowPriPktsIn) (srpRingCurUcastLowPriOctetsIn) Multicast (srpRingCurMcastLowPriPktsIn) (srpRingCurMcastLowPriOctetsIn) Number received during 15-minute octets Related Topics Using CiscoView Main Menu Selecting Components Configuring Devices Monitoring
PATH=/ciscoview/Routershare/monitor/Low_Priority_Traffic_Physical_Layer.htm TITLE=Low Priority Traffic TEXT=Use this option to monitor low priority traffic transmission statistics to physical medium-dependent layer information: current interval. particular side of SRP interface. Procedure access Right-click the port and select Interface from pop-up menu. Media Dependent dialog box appears. Tx Category displays: information. Unicast Packets (srpRingCurUcastLowPriPktsOut) (srpRingCurUcastLowPriOctetsOut) Multicast (srpRingCurMcastLowPriPktsOut) (srpRingCurMcastLowPriOctetsOut) Number going during 15-minute octets Related Topics Using CiscoView Main Menu Selecting Components Configuring Devices Monitoring
PATH=/ciscoview/Routershare/monitor/MIP_Security_Violations_Statistics.htm TITLE=MIP Security Violations Statistics TEXT=The dialog box displays the following information: Security Violations Count (mipSecViolationCounter) Vs (mipSecTotalViolations): Number of peer. violation entity.
PATH=/ciscoview/Routershare/monitor/mobile_ip_sec_violation_stats.htm TITLE=Mobile IP Security Violation Statistics TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. Configs from Category list. row Monitor button. following information appears: No of (cmiSecTotalViolations) total number violations this peer.
PATH=/ciscoview/Routershare/monitor/mobile_router_discovery_stats.htm TITLE=Mobile Router Discovery Statistics TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. Configs from Category list. row Monitor button. following information appears: (cmiMrMaAdvLifetimeRemaining) Lifetime (cmiMrMaHoldDownRemaining) Down remaining until advertisement expires. hold period
PATH=/ciscoview/Routershare/monitor/mobile_router_interface_stats.htm TITLE=Mobile Router Interface Statistics TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. Configs from Category list. row Monitor button. following information appears: Current Retransmissions (cmiMrIfSolicitRetransRemaining) No of (cmiMrIfSolicitRetransCount) Time (cmiMrIfCCoaRegRetryRemaining) remaining before retransmission interval expires. number solicitation. CCoA registration retry
PATH=/ciscoview/Routershare/monitor/Mobility_Agent_Advertisement_Group_Statistics.htm TITLE=Mobility Agent Advertisement Group Statistics TEXT=The dialog box displays the following information: Total Advertisements Sent(maAdvertisementsSent) Advertisements Solicitations(maAdvsSentForSolicitation) (maSolicitationsReceived) number of send by mobility. response to mobile node solicitations. received agent.
PATH=/ciscoview/Routershare/monitor/mobility_agent_mobile_router_reg_stats.htm TITLE=Mobility Agent and Mobile Router Registration Statistics TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cmiMaRegMaxInMinuteRegs) (cmiMaRegInLastMinuteRegs) Security Associations (cmiSecAssocsCount) maximum number of requests received minute by agent. last known entity, that is, entries cmiSecAssocTable.
PATH=/ciscoview/Routershare/monitor/mon00000.htm TITLE=Monitoring Router Performance TEXT=The CiscoView Monitor window Monitoring ports Monitoring compression Monitoring the device Monitoring environment
PATH=/ciscoview/Routershare/monitor/mon00001.htm TITLE=mon00001 TEXT=Alternatively, click the port to select it, then pull down the Monitor menu from the menubar and select Device .
PATH=/ciscoview/Routershare/monitor/mon00002.htm TITLE=mon00002 TEXT=Alternatively, click the port to select it, then pull down the Monitor menu from the menubar and select Card .
PATH=/ciscoview/Routershare/monitor/mon00003.htm TITLE=mon00003 TEXT=Alternatively, click the port to select it, then pull down the Monitor menu from the menubar and select .
PATH=/ciscoview/Routershare/monitor/mon00004.htm TITLE=The CiscoView Monitor Window TEXT=Use the CiscoView Monitor window to monitor various types of network performance information, such as port utilization errors. that displayed. depends upon What router selected (device, card, port) Information collection small dials stripchart graphs representing stored Management Base (MIB) variables. Labels indicate meanings Help button see more about are You can change polling interval from windows. Remember too frequent interfere with performance.
PATH=/ciscoview/Routershare/monitor/mon00005.htm TITLE=Using the Grapher Tool TEXT=If you see a Grapher button in the Monitor window, CiscoView is running on a network managementplatform that supports SunNet Manager graphing troubleshootingperformance problems. start tool, selected graphical display andclick button. represents value of mathematicalexpression involving more than one MIB variable, following error messageappears: Sorry, can’t formulas.
PATH=/ciscoview/Routershare/monitor/mon00006.htm TITLE=Monitoring Ports TEXT=To monitor port performance, right-click the port, and select Configure from the popup menu. The CiscoView window appears. For all types, except console auxiliary ports, displays interface level information by default. If more available then you can open CATEGORY additional of be displayed, as follows: Ethernet ( Errors Status ) Token Ring Frame Relay X.25 DS1 DS3 SONET See Also Displaying Configuration
PATH=/ciscoview/Routershare/monitor/mon00007.htm TITLE=Typical Interface Information TEXT=The CiscoView Monitor Port dialog box displays interface level utilization and performance information all ports. fields might vary according device types. following displayed many types: 100%) ifInErrors (locIfOutputQueueDrops) (locIfInputQueueDrops) (Last 5min) (locIfInBitsSec) (locIfOutBitsSec) Queue Drops (locIfCollisions) (locIfInIgnored) Packets Internal (locIfResets) Indicates rate of specified port. formula: calculate is: half duplex = (Delta[ifInOctets] + Delta[ifOutOctets]* 8 sysUpTime0)/100 (ifSpeed DELTA_TIME) full. (max (Delta[ifInOctects], Delta[ifOutOctets])* 100) where ifInOctects1 --- ifInOctects0 ifOutOctects1 ifOutOctects0 (sysUpTime1 > secs. will Number milli we have divide by get into sec) estimate current bandwidth bits second. value polling cycle. NEXT Example: chart refresh 30 sec, then ifInOctets0 times 12:10:20 ifInOctets1 12:10:50. Specifies incoming determined (ifInUcastPkts IfInNUcastPkts ifInDiscards ifInUnknownProtos)] 100. outgoing error ifOutErrors (ifOutUcastPkts ifOutNUcastPkts) Provides 5-minute exponentially decayed moving average input output dropped because was collisions detected this interface. that are ignored internally reset.
PATH=/ciscoview/Routershare/monitor/mon00018.htm TITLE=Token Ring Errors TEXT=The CiscoView Monitor Port dialog box displays the following error information for a Token Ring port: Beacon Frames (Hard (dot5StatsHardErrors) (dot5StatsSoftErrors) (dot5StatsReceiveCongestions) You can also select Unusual from CATEGORY menu additional information. Indicates number detected, immediately recoverable, fatal (that is, times interface transmits receives frames). soft (by MAC protocol) have been detected. This counter increments each there not enough buffer space incoming frame.
PATH=/ciscoview/Routershare/monitor/mon00022.htm TITLE=Unusual Token Ring Errors TEXT=Select Unusual Token Ring Errors from the CATEGORY menu to display the following information in the CiscoView Monitor Port dialog box: (dot5StatsInternalErrors) Frequency Aborted (AbortTransErrors) (dot5StatsRemove) Station Requests (dot5StatsLobeErrors) Data Path Errs Signals Lost This counter increments each times diagnoses internal error. (dot5StatsFreqErrors) Indicates number of that incoming signal. found outside expected range. transmits abort delimiter. Reqs interface has detected open short circuit path. Shows lobe (dot5StatsSignalLoss) specified loss
PATH=/ciscoview/Routershare/monitor/mon00029.htm TITLE=Ethernet Packet Anomalies TEXT=The CiscoView Monitor Port dialog box displays the following status information for an Ethernet port: Small Pkts (locIfInRunts) Large (locIfInGiants) Misaligned (locIfInFrame) Number of input packets that were smaller than physical media permitted. misaligned. larger
PATH=/ciscoview/Routershare/monitor/mon00033.htm TITLE=Ethernet Errors TEXT=The CiscoView Monitor Port window displays the following error information for an Ethernet port: MAC Tx (dot3StatsInternalMacTransmitErrors) Rx (dot3StatsInternalMacReceiveErrors) (dot3StatsSQETestErrors) Test (dot3StatsCarrierSenseErrors) Sense Giant Frames (dot3StatsFrameTooLongs) (dot3StatsLateCollisions) Collisions (dot3StatsAlignmentErrors) Check Errs Number software which transmission. failed because internal sub-layer transmit error. (These are that were cannot picked up any other count.) reception received times PLS generated Signal Quality particular interface. attempts carrier condition was lost never asserted. bigger than maximum permitted size. frame indicates nonlocal occurred protocol using nonstandard lengths use. collision detected later 64 octets into total included either network has too large propagation delay between reporting stations, some detecting/responding correctly. with alignment errors. occurs when integral pass FCS test. usually caused by problem.
PATH=/ciscoview/Routershare/monitor/mon00041.htm TITLE=Frame Relay Port Statistics TEXT=Procedure 1. Right-click on the chassis and select Device Summary > Modems from the popup menu. The dialog box. appears. 2. System CiscoView Category drop-down list Monitor window displays following information port: Error Percentage Traffic Specifies rate, port. To calculate uses formula: (frCircuitReceivedFECNs + frCircuitReceivedBECNs) / (frCircuitReceivedFrames 1) * 100 amount of through frCircuitSentFrames traffic.
PATH=/ciscoview/Routershare/monitor/mon00044.htm TITLE=X.25 Port Statistics TEXT=Procedure 1. Right-click on the port and select Monitor from the popup menu. The port monitor dialog box appears. 2. drop-down list box. CiscoView displays following performance information port: (x25CircuitInInterrupts) (x25CircuitOutInterrupts) (x25CircuitInOctets) (x25CircuitOutOctets) (x25CircuitDataRetransmissionTimeouts) RTx (x25CircuitResetTimeouts) Reset (x25CircuitInterruptTimeouts) number of interrupt packets received. sent. octets user data delivered upper layer. times T25 retransmission timer expired. T22 T26
PATH=/ciscoview/Routershare/monitor/mon00052.htm TITLE=Serial Statistics TEXT=The CiscoView Monitor Port dialog box displays the following information: Checksum Err Pkts (locIfInCRC) Aborted (locIfInAbort) Misaligned (locIfInFrame) Carrier Sig (locIfCarTrans) Overruns (locIfInOverrun) Number of input packets that were aborted. times interface detected signal transition. Shows amount arrived too quickly hardware receive. had cyclic redundancy check (CRC) errors.
PATH=/ciscoview/Routershare/monitor/mon00057.htm TITLE=Monitoring Compression TEXT=To monitor card performance, right-click the card and select Monitor from the popup menu. The CiscoView window appears. displays following: CSA. card: Compressed (csaInOctets) Received (In Sent (Out (csaInPackets) Input Dropped Output (csaNumberOfRestarts) of Restarts (csaCompressionRatio) (csaDecompressionRatio) Total octets). by (csaOutOctets) packets (csaOutPackets) (csaInPacketsDrop) dropped. large value indicates that too much data being passed process. (csaOutPacketsDrop) session restarts. one more Remote router incompatible. corrupted transmission. order not maintained. current ratio, expressed percentage which just processed was decompressed. 90% decompression; 1/10 size uncompressed (e.g. 100 were decompression times
PATH=/ciscoview/Routershare/monitor/mon00067.htm TITLE=Status (csaEnable) TEXT= Indicates whether compression services are currently enabled or disabled. 
PATH=/ciscoview/Routershare/monitor/mon00068.htm TITLE=Monitoring the Device TEXT=To monitor device-level performance information, right-click the device (that is, click some part of background image another card port) and select from popup menu. CiscoView window appears. It graphically displays memory usage bufferFail) status each device. fields may vary accordingly. type. Procedure then Category list. following displayed many types: ciscoMemoryPoolUsed % Failures CPU min)(avgBusy1) (5 sec)(busyPer) (1 min)(avgBusy5) percentage consumed. For IOS Versions priority 11.1, this calculated task, follows: 100 freeMem / processorRam * later, + ciscoMemoryPoolFree allocation requests failed. formula [ (bufferHgHit bufferLgHit bufferBgHit bufferMdHit bufferSmHit ] over first 5-second period. with scheduler. determines which takes triggers tasks -1 A cumulative average 1-minute variable, called by every seconds, computes time. last period, exponentially delayed 5-minute
PATH=/ciscoview/Routershare/monitor/mon00074.htm TITLE=Monitoring the Device Environment TEXT=The CiscoView Monitor Device window displays the following environment information. Use this option view status GGSN. Procedure Right-click and then select from Category list. foll. appears you hardware managing: Airflow Temp In Out Sensor +1.25V +2.5V Volt +1.50V +1.8V (PXF) (CPU) +3.3V +3.5V +5.2V +12.25V -12.2V +16V -16V +24V Reference current temperature of air entering router. (Cisco 7000). exhaust bottom 7401ASR). underneath front edge system board 7301). top near fans value (in millivolts) +1.2V line power supply. Parallel Express Forwarding (envTestPt3Measure) +5V (envTestPt4Measure) +12V +12.2V (envTestPt5Measure) -12V (envTestPt6Measure)
PATH=/ciscoview/Routershare/monitor/mon00075.htm TITLE=Status Information for GGSN and SGSN TEXT=Status Information for GGSN Use this option to view status information for GGSN. Procedure Right-click the device then select Monitor from Category list. following appears: (cgprsGtpCurRxPacketQueueSize) x-Packets Queue Size G-PDUs (cgprsGtpCurUnexpRxGpduCnt) Rejected (cgprsGtpCurRejPDPCxtActivationCnt) Context (cgprsGtpTotalPktsDropped) (cgprsGtpCurMTForPremiumQos) QoS Mean Throughput (cgprsGtpCurMTForNormalQos) (cgprsGtpCurMTForBestEffortQos) Effort Y-Time (x-cgprsGtpDroppedPktsTimeFrame,y-cgprsGtpDroppedPktsCnt) Indicates current of packets node. total number received non-existing inactive since system startup. activations dropped. because unknown GTPwithin header, throughput, bits per second, premium class users normal 'best-effort' how many are within particular timeframe. It represented graph. which defined by cgprsGtpDroppedPktscnt cgprsGtpDroppedPktsTimeFrame.
PATH=/ciscoview/Routershare/monitor/mon00076.htm TITLE=GTP Statistics for GGSN TEXT=Use this option to view status information for GGSN. Procedure Right-click the device and then select Monitor from Category list. following appears: Allocated IP IpAddresses (cgprsGtpTotalNumAllocIpAddr) (cgprsGtpChargingMsgCnt) Messages Number of total addresses charging queue.
PATH=/ciscoview/Routershare/monitor/mon00077.htm TITLE=IMA Group Statistics TEXT=The table displays the following information: Running Seconds Unavailable Seconds Near End Failures Far Available (imaGroupTxAvailCellRate) (imaGroupRxAvailCellRate) Rate (imaGroupNumRxCfgLnks) Configured Insufficient-Links) Active (imaGroupRunningSecs) Indicates length of times since transmit has been operational state. UnavailableSecs (imaGroupUnavailSecs) number 1-second intervals during which traffic machine down. Near-End (imaGroupNeNumFailures) failure (Config-Abort, reported power-up reboot. Far-End (imaGroupFeNumFailures) current (truncated value cells second) provided by direction, considering all links receive (imaGroupNumTxCfgLnks to group. (imaGroupNumTxActLnks) and are (imaGroupNumRxActLnks)
PATH=/ciscoview/Routershare/monitor/mon00078.htm TITLE=IMA Group Interval Statistics TEXT=The table displays following information: Unavailable Seconds Near End Failures Far End Failures UnavailableSecs (imaGroupIntervalUnavailSecs) Number of 1-second 96intervals during which traffic state machine down one 15minutes minutes each. Near-End (imaGroupIntervalNeNumFailures) times failure has been reported previous Far-End (imaGroupIntervalFeNumFailures)
PATH=/ciscoview/Routershare/monitor/mon00079.htm TITLE=IMA Group Current Statistics TEXT=The table displays following information: Unavailable Seconds Near End Failures Far End Failures UnavailableSecs (imaGroupCurrentUnavailSecs) Number of 1-second intervals which traffic state machine down 15-minutes interval. Near-End (imaGroupCurrentNeNumFailures) times failure has been reported Far-End (imaGroupCurrentFeNumFailures)
PATH=/ciscoview/Routershare/monitor/mon00080.htm TITLE=IMA Group Total Statistics TEXT=The table displays the following information: Unavailable Seconds Near End Failures Far End Failures UnavailableSecs (imaGroupTotalUnavailSecs) Number of 1-second intervals which traffic state machine was down previous 24-hour hour interval. Invalid 15-minute minute are counted 0. Near-End (imaGroupTotalNeNumFailures) times failure has been reported Far-End (imaGroupTotalFeNumFailures)
PATH=/ciscoview/Routershare/monitor/mon00081.htm TITLE=IMA Link Statistics TEXT=The table displays following information: Link Violations Oif Anomalies Near End Severely Errored Seconds Far Unavailable (imaLinkNeTxUnusableSecs) imaLinkNeRxUnusableSecs) (imaLinkFeRxUnusableSecs) (imaLinkNeTxNumFailures) (imaLinkTxStuffs) Inserted (imaLinkImaViolations) Indicates ICP including counter of erred, invalid, missing cells except during SES-IMA. UAS-IMA-FE conditions. (imaLinkOifAnomalies) Specifies number near-end, (imaLinkNeSevErroredSecs) 1-second intervals containing greater than equal to 30 per cent has IV-IMAs, one more link, LIF, LODS defects, condition. (imaLinkFeSevErroredSecs) Species RDI-IMA (imaLinkNeUnavailSecs) far-end. Unavailability begins onset 10 contiguous and ends with (imaLinkFeUnavailSecs) SES-IMA-FE. LSM. Seconds( unusable (imaLinkFeTxUnusableSecs) indications from times transmit failure alarm been entered link. Failures( imaLinkNeRxNumFailures) receive (imaLinkFeTxNumFailures) (imaLinkFeRxNumFailures) stuff events direction. (imaLinkRxStuffs) detected
PATH=/ciscoview/Routershare/monitor/mon00082.htm TITLE=IMA Link Current Statistics TEXT=The table displays following information: Link violations Oif Anomalies Near End Severely Errored Seconds Far Unavailable (imaLinkCurrentNeTxUnusableSecs) imaLinkCurrentNeRxUnusableSecs) (imaLinkCurrentFeRxUnusableSecs) Failures(imaLinkCurrentNeTxNumFailures) (imaLinkCurrentTxStuffs) Inserted (imaLinkCurrentImaViolations) Number of erred, invalid missing ICP cells 15-minute interval. (imaLinkCurrentOifAnomalies) near-end (imaLinkCurrentNeSevErroredSecs) 1-second intervals containing greater than equal to 30 per cent counted has IV-IMAs, one more defects, (imaLinkCurrentFeSevErroredSecs) RDI-IMA Seconds( imaLinkCurrentNeUnavailSecs) Count begins onset 10 contiguous SES-IMA. and ends with (imaLinkCurrentFeUnavailSecs) far-end contagious SES-IMA-FE. LSM unusable (imaLinkCurrentFeTxUnusableSecs) indications from times transmit failure alarm been entered (imaLinkCurrentNeRxNumFailures) Indicates how many receive (imaLinkCurrentFeTxNumFailures) (imaLinkCurrentFeRxNumFailures) condition stuff events direction (imaLinkCurrentRxStuffs) detected
PATH=/ciscoview/Routershare/monitor/mon00083.htm TITLE=IMA Link Total Statistics TEXT=The table displays following information: Link Violations Oif Anomalies Near End Severely Errored Seconds Far Unavailable (imaLinkTotalNeTxUnusableSecs) (imaLinkTotalNeRxUnusableSecs) (imaLinkTotalFeRxUnusableSecs) (imaLinkTotalNeTxNumFailures) (imaLinkTotalTxStuffs) Inserted (imaLinkTotalImaViolations) Number of erred, invalid, missing ICP cells during previous 24-hour hours, except SES-IMA. UAS-IMA-FE conditions. (imaLinkTotalOifAnomalies) near-end interval. Invalid intervals are counted has 0. (imaLinkTotalNeSevErroredSecs) 1-second containing greater than equal to 30 per cent IV-IMAs, one more link, LIF, LODS defects hours. (imaLinkTotalFeSevErroredSecs) RDI-IMA condition. (imaLinkTotalNeUnavailSecs) Count begins onset 10 contiguous and ends with (imaLinkTotalFeUnavailSecs) far-end SES-IMA-FE. LSM unusable (imaLinkTotalFeTxUnusableSecs) indication from times transmit failure alarm been entered (imaLinkTotalNeRxNumFailures) receive (imaLinkTotalFeTxNumFailures) (imaLinkTotalFeRxNumFailures) stuff events direction (imaLinkTotalRxStuffs) detected
PATH=/ciscoview/Routershare/monitor/mon00084.htm TITLE=IMA Link Interval Statistics TEXT=The table displays the following information: Near End Severely Errored Seconds Far End Severely Errored Unavailable (imaLinkIntervalNeTxUnusableSecs) (imaLinkIntervalNeRxUnusableSecs) (imaLinkIntervalFeRxUnusableSecs) (imaLinkIntervalNeTxNumFailures) (imaLinkIntervalTxStuffs) Inserted (imaLinkIntervalNeSevErroredSecs) Number of 1-second intervals containing greater than equal to 30 per cent ICP cells counted has IV-IMAs, one more defects previous 96 15 minutes each. (imaLinkIntervalFeSevErroredSecs) RDI-IMA (imaLinkIntervalNeUnavailSecs) near-end Unavailability begins onset 10 contiguous SES-IMA and ends with no (imaLinkIntervalFeUnavailSecs) far-end LSM unusable (imaLinkIntervalFeTxUnusableSecs) indications from times transmit failure alarm condition been entered (imaLinkIntervalNeRxNumFailures) receive (imaLinkIntervalFeTxNumFailures) (imaLinkIntervalFeRxNumFailures) stuff events direction (imaLinkIntervalRxStuffs) detected
PATH=/ciscoview/Routershare/monitor/mon00085.htm TITLE=CDMA PDSN System Statistics TEXT=Use this option to view system statistics details. Procedure To access CDMA PDSN System Statistics information: Right-click the device and select Monitor from popup menu. dialog box appears. displays: Currents Sessions(cCdmaSessionTotal) Ratio [Current Number of Vs (cCdmaSessionMaxAllowed)] PCF(cCdmaPcfTotal) (cCdmaPcfMaxAllowed)] (cCdmaSimpleIpFlowTotal) MoIP Flows(cCdmaMobileIpFlowTotal) Flows(cCdmaProxyMobileIpFlowTotal) Proxy Failures Count (cCdmaSessionFailTotal) Note: following variables are available PSDNv2.0. (cCdmaActiveSessions) (cCdmaDormantSessions) Related Topics Feature Overview Registration RP Update Information sessions. maximum total established with system. allowed by PCF. Packet control function interacting flows using simple service. A10/A11 occurred since Data Service Node agent restarted. sysUpTime can polled determine if was active state. dormant
PATH=/ciscoview/Routershare/monitor/mon00086.htm TITLE=CDMA PDSN PCF Statistics TEXT=CDMA PDSN PCF Table Use this option to view PDSN PCF details. Procedure To access CDMA PDSN PCF Statistics information: Right-click the device and select Monitor from popup menu. dialog box appears. Category row button. displays: Sessions Count (cCdmaPcfSessionTotal) (cCdmaPcfSessionMaxTotal) Number of Errors (cCdmaPcfErrorTotal) Related Topics Feature Overview System Registration RP Update Information connections established with Packet Control Function (PCF). Maximum simultaneous PCF. session
PATH=/ciscoview/Routershare/monitor/mon00087.htm TITLE=CDMA PDSN Session Statistics TEXT=Use this option to view CDMA PDSN session details. Procedure To access CDMA PDSN session information: Right-click the device and select Monitor from popup menu. dialog box appears. Table Category row button. displays: Data (cCdmaSessionSentOctets) (cCdmaSessionSentPkts) Received (cCdmaSessionRcvdOctets) (cCdmaSessionRcvdPkts) Outgoing Dropped (cCdmaSessionDiscardedOutPkts) Incoming (cCdmaSessionDiscardedInPkts) (cCdmaSessionGREFromIPPkts) (cCdmaSessionGREToIPPkts) Related Topics Feature Overview System PCF Registration RP Update Information number of octets sent mobile user since established. packets by was last restarted. Incomming encapsulated delivered transmission
PATH=/ciscoview/Routershare/monitor/mon00088.htm TITLE=Monitor MAC Layer Traffic TEXT=Use this option to monitor packet count for a source and destination address or monitor packet count souce particular SRP interface. Procedure access information: Right-click the port select Interface Statistics from pop-up menu. dialog box appears. Category displays: information. Packets Received (srpMACCountPktsBySource) Sent (srpMACCountPktsByDest) Number of node address. Discontinuities value can occur management system reinitialization depending srpMACSourceDiscontTimeStamp. Related Topics Using CiscoView Main Menu Selecting Components Configuring Devices Monitoring
PATH=/ciscoview/Routershare/monitor/mon00089.htm TITLE=Physical Layer Errors TEXT=SRP Physical Layer Errors Use this option to monitor physical medium dependent layer error statistics traffic reception information: the current interval. of particular side interface. Procedure 1. Right-click and select from popup menu. Port dialog box appears. 2. Category Interface Click button. that displays following TTL Exp. Packets Discard (srpErrCntCurrRingRxTtlExpPkts) (srpErrCntCurrRingRxShortPkts) (srpErrCntCurrRingRxGiantPkts) Aborted (srpErrCntCurrRingRxAbortPkts) (srpErrCntCurrRingRxCRC) Related Topics Higher Number discarded due expiry, received during 15 minute short packets, 9216 octets. less. giant larger than maximum size which are by abort sequence code. with errors,
PATH=/ciscoview/Routershare/monitor/mon00090.htm TITLE=Higher Layer Errors TEXT=SRP Higher Layer Errors Use this option to monitor higher layer error statistics traffic reception for the current interval. of particular side interface. Procedure 1. Right-click and select from popup menu. Port dialog box appears. 2. Category Interface Click button. that displays following information: Discarded Packets (srpErrCntCurrHostRxDiscardPkts) (srpErrCntCurrHostRxShortPkts) (srpErrCntCurrHostRxGiantPkts) Related Topics Physical Number cannot delivered due resource limitation, during 15 minute being too short, big,
PATH=/ciscoview/Routershare/monitor/mon00091.htm TITLE=Receive Side Physical Layer Errors TEXT=Use this option to monitor error statistics of traffic from layer 1 physical medium in a particular interval information: SRP interface. Procedure access Right-click the port and select Interface pop-up menu. dialog box appears. (srpRingIntRxErrorsDataParity) Category displays: information. Data Parity (srpRingIntRxErrorsShortPackets) (srpRingIntRxErrorsGiantPackets) Giant (srpRingIntRxErrorsSideBadPackets) (srpRingIntRxErrorsCRC) Number received layer-1 during 15-minute past 24 hours. short packets bad with Related Topics CiscoView Window Monitoring Ports Devices Environment Components
PATH=/ciscoview/Routershare/monitor/mon00092.htm TITLE=Receive Side Higher Layer Errors TEXT=Use this option to monitor error statistics of traffic from higher layer in a particular interval for SRP interface. Procedure access information: Right-click the port and select Interface pop-up menu. dialog box appears. (srpHostIntRxErrorsDataParity) Category displays: information. Data Parity (srpHostIntRxErrorsShortPackets) (srpHostIntRxErrorsGiantPackets) Giant (srpHostIntRxErrorsSideBadPackets) Number received during 15-minute past 24 hours. short packets bad Related Topics CiscoView Window Monitoring Ports Devices Environment Components
PATH=/ciscoview/Routershare/monitor/mon00093.htm TITLE=Receive Side Low Priority Traffic Statistics TEXT=Low Priority Traffic Use this option to monitor statistics of low priority traffic from higher layer in particular interval information: SRP interface. Procedure access Right-click the port and select Interface pop-up menu. dialog box. appears. Rx Category displays: information. Unicast Packets (srpHostIntUcastLowPriPktsIn) (srpHostIntUcastLowPriOctetsIn) Multicast (srpHostIntMcastLowPriPktsIn) (srpHostIntMcastLowPriOctetsIn) Number received during 15-minute past 24 hours. octets Related Topics CiscoView Window Monitoring Ports Devices Environment Components
PATH=/ciscoview/Routershare/monitor/mon00094.htm TITLE=Receive Side High Priority Traffic Statistics TEXT=Use this option to monitor statistics of high priority traffic from higher layer in a particular interval for SRP interface. Procedure access information: Right-click the port and select Interface pop-up menu. dialog box. appears. Rx Category displays: information. Unicast Packets (srpHostIntUcastHighPriPktsIn) (srpHostIntUcastHighPriOctetsIn) MultiCast (srpHostIntMcastHighPriPktsIn) (srpHostIntMcastHighPriOctetsIn) Number received 15-minute past 24 hours. octets Related Topics CiscoView Window Monitoring Ports Devices Environment Components
PATH=/ciscoview/Routershare/monitor/mon00095.htm TITLE=Transmit Side Low Priority Traffic Statistics TEXT=Use this option to monitor statistics of low priority traffic transmission to higher layer in a particular interval information: SRP interface. Procedure access Right-click the port and select Interface from pop-up menu. dialog box. appears. Tx Category displays: information. Unicast Packets (srpHostIntUcastLowPriPktsOut) (srpHostIntUcastLowPriOctetsOut) Multicast (srpHostIntMcastLowPriPktsOut) (srpHostIntMcastLowPriOctetsOut) Number total going during 15-minute past 24 hours. octets Related Topics CiscoView Window Monitoring Ports Devices Environment Components
PATH=/ciscoview/Routershare/monitor/mon00096.htm TITLE=Transmit Side High Priority Traffic Statistics TEXT=Use this option to monitor statistics of high priority traffic transmission to higher layer in a particular interval information: SRP interface. Procedure access Right-click the port and select Interface from pop-up menu. dialog box. appears. Tx Category displays: information. Unicast Packets (srpHostIntUcastHighPriPktsOut) (srpHostIntUcastHighPriOctetsOut) MultiCast (srpHostIntMcastHighPriPktsOut) (srpHostIntMcastHighPriOctetsOut) Number high-priority going during 15-minute past 24 hours. octets Related Topics CiscoView Window Monitoring Ports Devices Environment Components
PATH=/ciscoview/Routershare/monitor/mon00097.htm TITLE=Receive Side Low Priority Traffic Statistics TEXT=Dialog box displays following information: Unicast Low Priority Packets (srpHostIntUcastLowPriPktsIn) Octets (srpHostIntUcastLowPriOctetsIn) Multicast (srpHostIntMcastLowPriPktsIn) (srpHostIntMcastLowPriOctetsIn) Number of received from higher layer during 15-minute interval the past 24 hours.
PATH=/ciscoview/Routershare/monitor/mon00098.htm TITLE=Receive Side High Priroity Traffic Statistics TEXT=Dilog box displays following information: Unicast High Priority Packets (srpHostIntUcastHighPriPktsIn) Octets (srpHostIntUcastHighPriOctetsIn) MultiCast (srpHostIntMcastHighPriPktsIn) (srpHostIntMcastHighPriOctetsIn) Number of received from higher layer during 15-minute interval the past 24 hours.
PATH=/ciscoview/Routershare/monitor/mon00099.htm TITLE=Transmit Side Low Priority Statistics TEXT=Dialog box displays following information: Unicast Low Priority Packets (srpHostIntUcastLowPriPktsOut) Octets (srpHostIntUcastLowPriOctetsOut) Multicast (srpHostIntMcastLowPriPktsOut) (srpHostIntMcastLowPriOctetsOut) Number of total going the higher layer during 15-minute interval past 24 hours.
PATH=/ciscoview/Routershare/monitor/mon00100.htm TITLE=Transmit Side High Priority Traffic Statistics TEXT=Dialog box displays following information: Unicast High Priority Packets (srpHostIntUcastHighPriPktsOut) Octets (srpHostIntUcastHighPriOctetsOut) MultiCast (srpHostIntMcastHighPriPktsOut) (srpHostIntMcastHighPriOctetsOut) Number of going to higher layer during 15-minute interval past 24 hours. uncast
PATH=/ciscoview/Routershare/monitor/mon00101.htm TITLE=Receive Side Low Priority Traffic TEXT=Use this option to monitor statistics of low priority traffic reception from higher layer for current interval particular SRP interface. Procedure access information: Right-click the port and select Interface pop-up menu. dialog box. appears. Rx Category displays: information. Unicast Packets (srpHostCurUcastLowPriPktsIn) (srpHostCurUcastLowPriOctetsIn) Multicast (srpHostCurMcastLowPriPktsIn) (srpHostCurMcastLowPriOctetsIn) Number received during 15-minute interval. octets Related Topics CiscoView Window Monitoring Ports Devices Environment Components
PATH=/ciscoview/Routershare/monitor/mon00102.htm TITLE=Receive Side High Priority Traffic TEXT=Use this option to monitor statistics of high priority traffic reception from higher layer for current interval particular SRP interface. Procedure access information: Right-click the port and select Interface pop-up menu. dialog box. appears. Rx Category displays: information. Unicast Packets (srpHostCurUcastHighPriPktsIn) (srpHostCurUcastHighPriOctetsIn) Multicast (srpHostCurMcastHighPriPktsIn) (srpHostCurMcastHighPriOctetsIn) Number received during 15-minute interval. octets Related Topics CiscoView Window Monitoring Ports Devices Environment Components
PATH=/ciscoview/Routershare/monitor/mon00103.htm TITLE=Transmit Side Low Priority Traffic Statistics TEXT=Use this option to monitor statistics of low priority traffic reception to higher layer for current interval particular SRP interface. Procedure access information: Right-click the port and select Interface from pop-up menu. dialog box. appears. Tx Category displays: information. Unicast Packets (srpHostCurUcastLowPriPktsOut) (srpHostCurUcastLowPriOctetsOut) Multicast (srpHostCurMcastLowPriPktsOut) (srpHostCurMcastLowPriOctetsOut) Number going during 15-minute interval. octets Related Topics CiscoView Window Monitoring Ports Devices Environment Components
PATH=/ciscoview/Routershare/monitor/mon00104.htm TITLE=Transmit Side High Priority Traffic Statistics TEXT=Use this option to monitor statistics of high priority traffic reception to higher layer for current interval particular SRP interface. Procedure access information: Right-click the port and select Interface from pop-up menu. dialog box. appears. Tx Category displays: information. Unicast Packets (srpHostCurUcastHighPriPktsOut) (srpHostCurUcastHighPriOctetsOut) Multicast (srpHostCurMcastHighPriPktsOut) (srpHostCurMcastHighPriOctetsOut) Number going during 15-minute interval. octets Related Topics CiscoView Window Monitoring Ports Devices Environment Components
PATH=/ciscoview/Routershare/monitor/mon00105.htm TITLE=Receive Side LowPriority Traffic Statistics TEXT=Receive Side Low Priority Traffic Statistics Use this option to monitor statistics of low priority traffic reception from physical medium-dependent layer information: particular SRP interface. Procedure access Right-click the port and select Interface pop-up menu. Media Dependent dialog box. appears. Rx Category displays: information. Unicast Packets (srpRingIntUcastLowPriPktsIn) (srpRingIntUcastLowPriOctetsIn) Multicast (srrpRingIntMcastLowPriPktsIn) (srpRingIntMcastLowPriOctetsIn) Number received during 15-minute interval. octets Related Topics CiscoView Window Monitoring Ports Devices Environment Components
PATH=/ciscoview/Routershare/monitor/mon00106.htm TITLE=Receive Side High Priority Traffic Statistics TEXT=Use this option to monitor statistics of high priority traffic reception from physical medium-dependent layer information: particular SRP interface. Procedure access Right-click the port and select Interface pop-up menu. Media Dependent dialog box. appears. Rx Category displays: information. Unicast Packets (srpRingIntUcastHighPriPktsIn) (srpRingIntUcastHighPriOctetsIn) Multicast (srpRingIntMcastHighPriPktsIn) (srpRingIntMcastHighPriOctetsIn) Number received 15-minute interval during past 24 hours. octets Related Topics CiscoView Window Monitoring Ports Devices Environment Components
PATH=/ciscoview/Routershare/monitor/mon00107.htm TITLE=Transmit Side Low Priority Traffic Statistics TEXT=Use this option to monitor statistics of low priority traffic reception to physical medium-dependent layer interval particular information: SRP interface. Procedure access Right-click the port and select Interface from pop-up menu. Media Dependent dialog box. appears. Tx Category displays: information. Unicast Packets (srpRingIntUcastLowPriPktsOut) (srpRingIntUcastLowPriOctetsOut) Multicast (srpRingIntMcastLowPriPktsOut) (srpRingIntMcastLowPriOctetsOut) Number going 15-minute during past 24 hours. octets Related Topics CiscoView Window Monitoring Ports Devices Environment Components
PATH=/ciscoview/Routershare/monitor/mon00108.htm TITLE=Transmit side High Priority Traffic Statistics TEXT=Use this option to monitor statistics of high priority traffic reception to physical medium-dependent layer interval particular information: SRP interface. Procedure access Right-click the port and select Interface from pop-up menu. Media Dependent dialog box. appears. Tx Category displays: information. Unicast Packets (srpRingIntUcastHighPriPktsOut) (srpRingIntUcastHighPriOctetsOut) Multicast (srpRingIntMcastHighPriPktsOut) (srpRingIntMcastHighPriOctetsOut) Number going during 15-minute past 24 hours. octets Related Topics CiscoView Window Monitoring Ports Devices Environment Components
PATH=/ciscoview/Routershare/monitor/Monitor_Access_Point_Statistics.htm TITLE=Monitor Access Point Statistics TEXT=Access Point Statistics Monitor1 Procedure Right-click the device, then select Configure . The Device Configuration dialog box displayed. from Category list. desired row and following details are displayed: No of IP Addresses Allocated (cgprsAccPtIpAddrAllocations) Total PDP Context (cgprsAccPtMsActivatedPdps) Successfully completed (cgprsAccPtSuccMsActivatedPdps) Dynamic (cgprsAccPtMsActivatedDynPdps) (cgprsAccPtSuccMsActivatedDynPdps) deactivation (cgprsAccPtMsDeactivatedPdps) (cgprsAccPtSuccMsDeactivatedPdps) Shows number MS. procedures initiated. by any this APN. successfully. When requests address PLMN,
PATH=/ciscoview/Routershare/monitor/Monitor_Real_Server_Info.htm TITLE=Monitor Real Server Info TEXT=Monitor Real Server Procedure Right-click the device, then select Configure > SLB Statistics . With a load balancing (SLB) instance selected, Servers table displayed. entry Handled following iformation displayed: (slbRealNumberOfConnections) Count Operating (slbRealOperWeight) (slbRealMetric) values (slbRealConsecutiveFails) fails (slbRealTotalFails) (slbRealTotalConnections) -64bit (slbRealHCTotalConnections) number of TCP UDP connections assigned server. actual weight used by algorithms. can adjusted dynamically Dynamic Feedback Protocol (DFP). zero shows that no new will Higher accept more work. Value least algorithm. divided gives metric. value. are given smaller failures. when SYN timeouts RST received from times failed since creation row. was configured. This 64-bit version slbRealTotalConnections.
PATH=/ciscoview/Routershare/monitor/Monitor_SLB_Statistics.htm TITLE=Monitor SLB Status TEXT=SLB Statistics (64-bit) Procedure Right-click the device, then select Configure > SLB Statistics . With server load balancing (SLB) instance selected, Bit following information displayed. Packets Forwarded-64bit (slbStatsUnassistedSwitchingHCPks) Handled-64bit (slbStatsAssistedSwitchingHCPkts) (slbStatsCreatedHCConnections) Created-64 Established-64bit (slbStatsEstablishedHCConnections) Destroyed-64bit (slbStatsDestroyedHCConnections) Reassinged-64bit (slbStatsReassignedHCConnections) Zombie-64bit (slbStatsHCZombies) Forwarded&#150;64bit number software. forwarded by manager This version slbStatsUnassistedSwitchingPkts. Handled&#150;64bit switched via highest-performance switching path. slbStatsAssistedSwitchingPkts. Created&#150;64 connections created since was configured. TCP/IP after seeing SYN/ACK connection. UDP based source destination, removed timer. slbStatsCreatedConnections. Established&#150;64bit established through SLB. reach ESTAB state exchange. data sent from client server. Destroyed&#150;64bit destroyed, either teardown timeout. can only timed slbStatsDestroyedConnections. Reassinged&#150;64bit reassigned one real another. slbStatsReassignedConnections. Zombie&#150;64bit currently zombie waiting timers expire. slbStatsZombies.
PATH=/ciscoview/Routershare/monitor/Monitor_Virtual_Server_Info.htm TITLE=Monitor Virtual Server Info TEXT=Monitor Virtual Server Procedure Right-click the device, then select Configure > SLB Statistics . With load balancing (SLB) instance selected, Servers entry table handled following information displayed: Current (slbVirtualNumberOfConnections) (slbVirtualTotalConnections) Connnections-64bit (slbVirtualHCTotalConnections) number of connections assigned server. since was configured. Connnections&#150;64bit This 64-bit version slbVirtualTotalConnections.
PATH=/ciscoview/Routershare/monitor/mr_statistics.htm TITLE=MR Statistics TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cmiMrRegNewHa) MR-HA Registration (cmiMrBetterIfDetected) Interface Detected Packets (cmiMrTunnelPktsRcvd) (cmiMrTunnelPktsSent) (cmiMrTunnelBytesRcvd) Received (cmiMrTunnelBytesSent) (cmiMrRedStateActive) Redundancy (cmiMrRedStatePassive) Passive number of times mobile router-home registers with different home agent due changes / priority. that has better interface. tunnel. sent through bytes state changed active. passive.
PATH=/ciscoview/Routershare/monitor/new_ip_pool_statistics.htm TITLE=New IP Pool Statistics TEXT=Navigation Right-click the device, and select Configure . The Device Configuration dialog box appears. from Category list. row Monitor button. following information appears: Address Available (cIpLocalPoolStatFreeAddrs) cilpPercentAddrUsedLoNotif (cIpLocalPoolStatInUseAddrs) Low Percentage (cIpLocalPoolPercentAddrThldLo) High (cIpLocalPoolPercentAddrThldHi) number of addresses used this local pool. being When falls below threshold value, notification generated. After once, will again until equals exceeds indicated by cIpLocalPoolPercentAddrThldHi. object should never greater than cilpPercentAddrUsedHiNotif cIpLocalPoolPercentAddrThldLo. smaller
PATH=/ciscoview/Routershare/monitor/OSPF_Area_Specific_Information_Monitoring.htm TITLE=OSPF Area Specific Information TEXT=Monitoring The OSPF Area Specific Information Monitor dialog box monitors area specific information of OSPF. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure list, double-click Device Configuration appears. Protocols from Category list. SelectProtocol Details button. rows table. and later: Note left frame displays categories right If displayed, variable which indexed key values listed below category. view particular Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane box. following appears: Intra-area routers Table Update (ospfSpfRuns) Total ABR Reachable (ospfAreaBdrRtrCount) ASBR (ospfASBdrRtrCount) (ospfAreaLSACount) Gauge Related Topics Interface State General Neighbor Virtual Number times has been calculated using this area's link-state database. typically done Dijkstra's algorithm. border within area. initially zero, Pass. autonomous system advertisements database, excluding External LSA's.
PATH=/ciscoview/Routershare/monitor/OSPF_Interface_State_Monitoring.htm TITLE=OSPF Interface State TEXT=The OSPF Interface State Monitor dialog box monitors the transition state of the interface. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure list, double-click Device Configuration appears. Protocols from Category list. SelectProtocol Details button. rows table. and later: Note left frame displays categories right (ospfIfEvents) displayed, variable which indexed key values are listed below category. view particular Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane box. Area following information appears: Counter Related Topics Specific Monitoring LSA General Neighbor Virtual Number times this has changed its state, error occurred.
PATH=/ciscoview/Routershare/monitor/OSPF_LSA_General_Monitoring.htm TITLE=OSPF LSA General Monitoring TEXT=The OSPF LSA General Monitor dialog box displays LSA general monitoring details of OSPF. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure list, double-click Device Configuration appears. Protocols from Category list. SelectProtocol button. Click and later: Note left frame categories right table. If displayed, variable which indexed key values are listed below category. view particular rows Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane box. following information appears: AS-external-LSA Gauge(ospfExternLSACount) (ospfOriginateNewLSAs) (ospfRxNewLSAs) Originated Counter Received Related Topics Area Specific Interface State Neighbor Virtual Number (LS type 5) link-state advertisements. database. newer have been originated. This incremented each time router originates LSA. determined instances. does not include instantiations self-originated
PATH=/ciscoview/Routershare/monitor/OSPF_Neighbor_State_Monitoring.htm TITLE=OSPF Neighbor State TEXT=Monitoring The OSPF Neighbor State Monitor dialog box monitors the state of the neighbor. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure list, double-click Device Configuration appears. Protocols from Category list. SelectProtocol Details button. rows table. and later: Note left frame displays categories right If displayed, variable which indexed key values are listed below category. view particular Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane box. Area following information appears: Relation. Transition (ospfNbrEvents) Retransmission Queue Length (ospfNbrLSRetransQLen) Related Topics Specific Interface LSA General Virtual Number times relationship has changed state, error occurred. Current queue.
PATH=/ciscoview/Routershare/monitor/OSPF_Virtual_Interface_State_Monitoring.htm TITLE=OSPF Virtual Interface State TEXT=Monitoring The OSPF Virtual Interface State Monitor dialog box monitors the transition state of the interface. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure list, double-click Device Configuration appears. Protocols from Category list. SelectProtocol Details button. rows table. and later: Note left frame displays categories right (ospfVirtIfEvents) displayed, variable which indexed key values are listed below category. view particular Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane box. Area following information appears: Counter Related Topics Specific LSA General Neighbor Number changes error events link.
PATH=/ciscoview/Routershare/monitor/OSPF_Virtual_Neighbor_State_Monitoring.htm TITLE=OSPF Virtual Neighbor State TEXT=The OSPF Virtual Neighbor State Monitor dialog box monitors the state of the virtual neighbor. Procedure For CiscoView versions earlier than 5.2: Right-click device. Then select Configure list, double-click Device Configuration appears. Protocols from Category list. indexed SelectProtocol Details button. rows table. and later: Note left frame displays categories right If displayed, variable which key values are listed below category. view particular Multiple indexes table, any, nested manner. about that value. lowest indexing row. pane box. Area following information appears: Relation. Transition (ospfVirtNbrEvents) Retransmission Queue Length (ospfVirtNbrLSRetransQLen) Related Topics Specific Monitoring Interface LSA General Number times link has changed its state, error occurred. Current queue.
PATH=/ciscoview/Routershare/monitor/port_monitor_aal5VccDrops.htm TITLE=AAL5 VCC Drops TEXT=The ATM Adaptation Layer type 5 Virtual Circuit Connections (AAL5 VCC) Drops dialog box shows the AAL5 for selected path identifier (VPI) and (VCI) values. displays sub interfaces; port, Procedure Right-click then Monitor. Select Performance from Category list. row displayed. following information appears: Rx Side Packet (cAal5VccInDroppedPkts) Tx (cAal5VccOutDroppedPkts) (cAal5VccInDroppedOctets) (cAal5VccOutDroppedOctets) number of CPCS PDUs/Interval. dropped reception associated with entity. unit transmission octets Octets/Interval.
PATH=/ciscoview/Routershare/monitor/port_monitor_aal5VccPerfStatTable.htm TITLE=AAL5 VCC Performance TEXT=The ATM Adaptation Layer type 5 Virtual Circuit Connections (AAL5 VCC) Performance dialog box gives path identifier (VPI) and (VCI) values. Procedure Right-click port, then select Monitor from Category list. following information. displayed: Sub Interface (ifIndex) Description (ifDescr) (ifAlias) Value (aal5VccVpi) (aal5VccVci) Identifies sub-interface, which entry contains management Presents (for example, product name, manufacturer, hardware version). alias specified by network manager. of identified ifIndex.
PATH=/ciscoview/Routershare/monitor/PPPoE_System_Sessions_Exceeded_System_Sessions.htm TITLE=PPPoE_System_Sessions_Exceeded_System_Sessions TEXT=PPPoE System Sessions-Exceeded System Sessions The PPPoE System Session-Exceeded System Sessions dialog monitors exceeded errors information specified interval. Procedure Right-click device, then select Click Monitor following appears: (cPppoeSystemExceededSessionErrors) accumulated number of establishing session due cPppoeSystemCurrSessions value. exceeds cPppoeSystemMaxAllowedSessions
PATH=/ciscoview/Routershare/monitor/PPPoE_System_Sessions_Exceeded_VCL_Sessions.htm TITLE=PPPoE_VCL_Session_Exceeded_VCL_Sessions TEXT=PPPoE VCL Session-Exceeded VCL Sessions The PPPoE VCL (Virtual Circuit Link) Session-Exceeded System dialog box monitors exceeded errors information specified attempts/interval this VCL. unit Procedure Right-click device, then select row from Info Table, Choose required and Monitor (cPppoeVcExceededSessionErrors) following appears: accumulated number of establishing session due cPppoeVcCurrSessions value. exceeds cPppoeVcMaxAllowedSessions
PATH=/ciscoview/Routershare/monitor/Registration_Statistics.htm TITLE=Registration Statistics TEXT=CDMA PDSN Registration Accepted Use this option to view accepted registration statistics. Procedure To access information: Right-click the device and select Monitor from popup menu. dialog box appears. Category displays: (cCdmaRPRegValidRequests) Received (cCdmaRPRegAcceptedReplies) Requet (cCdmaRPRegLifeTimeZeroRequests) Time 0 (cCdmaRPDeRegAcceptedReplies) Related Topics Feature Overview System PCF Session Update Information Number of valid requests since startup. replies with lifetime zero
PATH=/ciscoview/Routershare/monitor/rejected_pdp_stat_per_cause_1.htm TITLE=Rejected PDP Statistics per Cause - 1 TEXT=Procedure Right-click the device and then select Monitor . In the category drop-down box select Rejected following information appears: Unsupported (cGgsnVersionNotSupportedRejPdps) Unknown (cGgsnUnkownMessageRejPdps) too short (cGgsnMsgTooShortRejPdps) Mandatory IE (cGgsnMandIeMissingRejPdps) (cGgsnMandIeIncorrectRejPdps) Optional (cGgsnOptIeInvalidRejPdps) number of contexts that were due Supported. This counter triggered by create/update PPP request message. Short. Missing. Incorrect. Invalid.
PATH=/ciscoview/Routershare/monitor/rejected_pdp_stat_per_cause_2.htm TITLE=Rejected PDP Statistics per Cause - 2 TEXT=Procedure Right-click the device and then select Monitor . Select Rejected PDP Statistics per Cause from Category drop-down box. following information appears: (cGgsnIeUnknownRejPdps) IE (cGgsnIeOutOfOrderRejPdps) of Order. (cGgsnIeUnexpectedRejPdps) (cGgsnIeDuplicatedRejPdps) Optional (cGgsnOptIeIncorrectRejPdps) TFT already exists. (cGgsnPdpWithoutTftExistsRejPdps) number contexts that due Unknown. This counter triggered by create/update PPP request message. Unexpected. Duplicated. Incorrect. were without
PATH=/ciscoview/Routershare/monitor/rp_reg_discard_stats.htm TITLE=RP Registration Discard Statistics TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select CDMA PDSN PCF & SO Based from Category list. row button following information appears: Initial A11 Requests (cCdmaPcfSoRpInitRegDiscardedReqs) Re-registration (cCdmaPcfSoRpReRegDiscardedReqs) De-registration (cCdmaPcfSoRpDeRegDiscardedReqs) (cCdmaPcfSoRpHandoffRegDiscardedReqs) number silently discarded since system was last restarted. handoff
PATH=/ciscoview/Routershare/monitor/rp_reg_reply_errors.htm TITLE=RP Registration Reply Errors TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cCdmaRegRplyInternalErrs) Memory Allocation Failure (cCdmaRegRplyMemFailErrs) Security Association Not found (cCdmaRpRplyPCFNoSecOrParseErrs) number of replies sent due internal during processing, since system was last restarted. failures Cannot send error Request,
PATH=/ciscoview/Routershare/monitor/rp_reg_req_errors_invalid_reasons.htm TITLE=RP Registration Request Errors of Invalid Reasons TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: Packet Length (cCdmaRegReqInvPakLenErrs) (cCdmaRegReqInvProtocolErrs) Value (cCdmaRegReqInvFlagsErrs) Authentication (cCdmaRegReqInvMHAEKeyErrs) (cCdmaRegReqInvSPIErrs) (cCdmaRegReqInvConnectionIDErrs) (cCdmaRegReqInvMNIDErrs) (cCdmaRegReqInvMNIDTypeErrs) Type number requests due while parsing since system was last restarted. protocol Session Specific Extension flags key Mobile-Home connection mobile node
PATH=/ciscoview/Routershare/monitor/rp_reg_req_errors_invalid_reasons_contd.htm TITLE=RP Registration Request Errors of Invalid Reasons Contd TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select following information appears: (cCdmaRegReqInvMSIDLenErrs) Length (cCdmaRegReqInvOrderErrs) Extension (cCdmaRegReqInvVendorIDInVSEErrs) Specific (cCdmaRegReqInvVSEErrs) Application (cCdmaRegReqInvAppTypeInVSEErrs) (cCdmaRegReqInvAppSubTypeInVSEErrs) Accounting Attribute (cCdmaRegReqAcctInvLenAttrErrs) Sequence Number (cCdmaRegReqAcctInvSeqNumErrs) (cCdmaRegReqInvAirlinkRecErrs) Requests since system was last restarted. order extensions vendor-specific type sub airlink record that have been silently discarded
PATH=/ciscoview/Routershare/monitor/rp_reg_req_errors_stats_1.htm TITLE=RP Registration Request Errors Stats 1 TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select Stats1 from Category list. following information appears: (cCdmaRegReqMismatchSPIErrs) Mismatch Session Extension (cCdmaRegReqMissingSSEErrs) Authentication (cCdmaRegReqMissingMHAEErrs) Duplicate Application (cCdmaRegReqDupAppTypeInVSEErrs) Critical Vendor (cCdmaRegReqDupCVSEErrs) Unknown Accounting Attribute (cCdmaRegReqAcctUnknwnAttrErrs) (cCdmaRegReqAcctDupAttrErrs) Sequence Number & Record Same (cCdmaRegReqAcctRecRetransErrs) of Requests Mobile-Home since system was last restarted. vendor-specific missing type extensions received airlink not updated
PATH=/ciscoview/Routershare/monitor/rp_reg_req_errors_stats_2.htm TITLE=RP Registration Request Errors Stats 2 TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cCdmaRegReqDuplicateGREKeyErrs) (cCdmaRegReqSameGREKeySetupRcvdErrs) (cCdmaRegReqGREKeyChngNoSetupErrs) Same Changed De-Registration Requests Denied (cCdmaRegReqDeRegNoSessionErrs) Re-Registration Received (cCdmaRegReqReRegInDisconnectErrs) Discarded (cCdmaRegReqMemFailErrs) Rejected due Maximum (cCdmaRpRegReqMaxSessionReachedErrs) number of duplicate key different MSID PCF, since system was last restarted. airlink setup non-existing session, without sessions disconnecting deleting state. memory allocation failure during processing limit configured reached.
PATH=/ciscoview/Routershare/monitor/rp_reg_req_stats.htm TITLE=RP Registration Request Statistics TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select CDMA PDSN PCF & SO Based from Category list. row button. following information appears: Initial A11 Requests (cCdmaPcfSoRpInitRegRcvdReqs) Re-registration (cCdmaPcfSoRpReRegRcvdReqs) De-registration (cCdmaPcfSoRpDeRegRcvdReqs) (cCdmaPcfSoRpHandoffRegRcvdReqs) (cCdmaPcfSoRpReRegAirlinkStarts) Start (cCdmaPcfSoRpReRegAirlinkStops) (cCdmaPcfSoRpDeRegAirlinkStops) number received since system was last restarted. handoff containing
PATH=/ciscoview/Routershare/monitor/rp_reg_update_ack_errors_stats.htm TITLE=RP Registration Update Ack Errors Stats TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cCdmaRegUpdAckNoSessionErrs) Extensions (cCdmaRegUpdAckMissingSSEErrs) Authentication (cCdmaRegUpdAckMissingRUAEErrs) Invalid (cCdmaRegUpdAckInvOrderErrs) of Vendor Specific (cCdmaRegUpdAckInvVSEErrs) Discarded Memory Allocation Failure (cCdmaRegUpdAckMemFailErrs) number session extension missing since system was last restarted. order vendor-specific due during processing,
PATH=/ciscoview/Routershare/monitor/rp_reg_update_errors.htm TITLE=RP Registration Update Errors TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: (cCdmaRegUpdInternalErrs) Memory Allocation Failures (cCdmaRegUpdMemFailErrs) number of updates not sent due internal during processing, since system was last restarted.
PATH=/ciscoview/Routershare/monitor/rp_session_update_ack_errors_stats.htm TITLE=RP Session Update Ack Errors Stats TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select from Category list. following information appears: Specific Extension (cCdmaSessUpdAckMissingSSEErrs) Authentication (cCdmaSessUpdAckMissingRUAEErrs) Invalid (cCdmaSessUpdAckInvOrderErrs) of Vendor (cCdmaSessUpdAckInvVSEErrs) Discarded (cCdmaSessUpdAckNoSessionErrs) Memory Allocation Failure (cCdmaSessUpdAckMemFailErrs) number missing since system was last restarted. order extensions vendor-specific due during processing,
PATH=/ciscoview/Routershare/monitor/rp_session_update_errors.htm TITLE=RP Session Update Errors TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select category from list. following information appears: (cCdmaSessUpdInternalErrs) Memory Allocation Failures (cCdmaSessUpdMemFailErrs) number of updates not sent due internal during processing, since system was last restarted.
PATH=/ciscoview/Routershare/monitor/rp_update_regi_failures_contd.htm TITLE=RP Update Registration Failures Contd TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select CDMA PDSN PCF & SO Based Statistics from Category list. row button. following information appears: Unspecified Reasons (cCdmaSoRpUpdHandoffReaUnSpecFails) Administrative Prohibition (cCdmaSoRpUpdHandoffAdmProhibFails) (cCdmaSoRpUpdHandoffMNAuthenFails) Authentication Identity (cCdmaSoRpUpdHandoffIdMismatchFails) Poorly Formed Request (cCdmaSoRpUpdHandoffBadReqFails) number registrations that failed reason since system was last restarted. sent result inter handoff. due mobile node failure mismatch
PATH=/ciscoview/Routershare/monitor/RP_Update_Statistics_Info.htm TITLE=RP Update Statistics Info TEXT=Use this option to view valid and accepted request statistics. Procedure To access RP update statistics information: Right-click Authentication device select Monitor from popup menu. dialog box displays: Received (cCdmaRPUpdValidRequests) (cCdmaRPUpdAcceptedReplies) Failed Unspecified (cCdmaRPUpdReasonUnSpecFailures) Administrative (cCdmaRPUpdAdminProhibFailures) (cCdmaRPUpdMNAuthenFailures) Identity (cCdmaRPUpdIdentMismatchFailures) Poor (cCdmaRPUpdBadRequestFailures) Related Topics CDMA PDSN Feature Overview System PCF Session Registration Number of valid, updated, requests since startup. replies registrations reason due prohibition failure mismatch poorly formed
PATH=/ciscoview/Routershare/monitor/rp_update_stats_contd.htm TITLE=RP Update Statistics Contd TEXT=Navigation Right-click the device, and select Monitor . The Monitor Device dialog box appears. Select CDMA PDSN PCF & SO Based from Category list. row button. following information appears: Inter (cCdmaSoRpUpdPcfHandoffs) Registrations Unacknowledged Updates (cCdmaSoRpUpdHandoffNotAckedReqs) Acknowledged (cCdmaSoRpUpdHandoffReceivedAcks) (cCdmaSoRpUpdHandoffAcceptedReqs) (cCdmaSoRpUpdHandoffDeniedReqs) Acknowledgements (cCdmaSoRpUpdHandoffDiscardedAcks) Initial (cCdmaSoRpUpdHandoffInitTxdReqs) Retransmitted (cCdmaSoRpUpdHandoffReTxdReqs) number (sent result handoffs) since system was last restarted. total A11 registration which corresponding have been received that were with Status field set non-zero, indicates accepted, denied, discarded handoffs, excluding re-transmitted updates, because not
PATH=/ciscoview/Routershare/monitor/SLB_Statistics.htm TITLE=SLB Statistics TEXT=(32-bit) Procedure Right-click the device, then select Configure > SLB Statistics . With a server load balancing (SLB) instance selected, Bit Monitor .The following information displayed. Packets Forwarded (slbStatsUnassistedSwitchingPkts) Handled (slbStatsAssistedSwitchingPkts) (slbStatsCreatedConnections) Created (slbStatsEstablishedConnections) (slbStatsDestroyedConnections) (slbStatsReassignedConnections) (slbStatsZombies) number Software by manager software. switched via highest-performance switching path. TCP/IP UDP connections since was configured. established through SLB. reach ESTAB state after SYN/ACK exchange. data sent from client server. destroyed, either teardown timeout. can only timed reassigned one real another. currently zombie waiting timers expire.
PATH=/ciscoview/Routershare/monitor/SSG_General_Information.htm TITLE=SSG General Information TEXT=The SSG General Information category of the Monitor dialog box allows you to monitor general information service selection gateway (SSG). Procedure Right-click device, authentication Select from list. following appears: (cssgStatsLoginAttempts) Attempts (cssgStatsLoginsSuccessful) (cssgStatsActiveSessions) Sessions (cssgStatsActiveHosts) (cssgStatsActiveServices) Packets Death (cssgStatsPODs) Number made successful logins active hosts services sent remote dial-in user client.
PATH=/ciscoview/Routershare/monitor/ssg_tal_stats.htm TITLE=SSG TAL Statistics TEXT=Procedure Right-click the device and then select Monitor . Select SSG TAL Statistics from the Category list. following information appears: (cssgTalWaitingForAuthUsers) waiting Authorization (cssgTalUnidentifiedUsers) (cssgTalSuspectUsers) Pass-through (cssgTalPassthroughUsers) number of currently existing users. authorization. unidentified These transparent which there was not response received AAA hence clear they valid suspect
PATH=/ciscoview/Routershare/monitor/Status_Information_for_GGSN_Ratio.htm TITLE=GPRS Status Information Ratio TEXT=Status Information for GGSN-Ratio Use this option to view status information ratio for GGSN. Procedure Right-click then device (cgprsGtpCurGSNBandwidthResrcUsed*100/cgprsGtpGSNTotalBandwidthResrc) select Monitor from Category list. The following appears: Established (cgprsGtpCurActivatedPDPCxtsCnt*100 contexts / cgprsGtpMaxNumPDPCxts) Used x-Packets Y-Time (x-cgprsGtpDroppedPktsTimeFrame,y-cgprsGtpDroppedPktsCnt) Indicates percentage of cgprsGtpMaxNumPDPCxts. current number node. maximum allowed. contains session mangement parameters necessary transfer between SGSNs Inter routing update procedure. amount bandwidth resource available obtained by deducting value. total how many packets are dropped. GTPwithin particular timeframe. It represented graph. which GTP defined cgprsGtpDroppedPktscnt cgprsGtpDroppedPktsTimeFrame.
PATH=/ciscoview/Routershare/monitor/Temperature_Status.htm TITLE=Temperature Status TEXT=The Temperature Status dialog monitors the temperature of Network Processing Engine (NPE-G100) or Network Services (NSE-100) CISCO 7304 device. Procedure Right-click chassis, then select Monitor from drop-down list. measured various test points. are: outlet) inlet) hotspot) db)
PATH=/ciscoview/Routershare/monitor/Voltage_Status.htm TITLE=Voltage Status TEXT=The Voltage Status dialog monitors the voltage levels on Network Processing Engine (NPE-G100) or on Services (NSE-100) CISCO 7304 device. Procedure Right-click chassis, then select Monitor from drop-down list. are: measured various test points. outlet 1.8V) 2.5V) 3.3V) 12V) inlet hotspot db 1.65V) 5.0 12.0 3.3c 1.5 1.2c
