# GGSN Access Point Route Probe Table

## Procedure

1. Right-click the device and then select Configure, or double-click the device.

2. Select GGSN Access Point Route Probe Table from the Category drop-down box.

The following information appears:

> Access Point Identifier (cgprsAccPtIndex)

> Destination IP Address (cgprsAccPtRpDestAddr)

> Protocol Type (cgprsAccPtRpProtocol)

> Port (cgprsAccPtRpDestPort)

> TTL Value (cgprsAccPtRpTtl)

### Access Point Identifier (cgprsAccPtIndex)

Locally unique identifier for this access point on the Gateway GPRS support node (GGSN).

### Destination IP Address (cgprsAccPtRpDestAddr)

Destination IP address to which the route probe packet will be sent.

### Protocol Type (cgprsAccPtRpProtocol)

Protocol type of the route probe packet. There are two possible values:

> udp

> icmp

This object can be set only after cgprsAccPtRpDestAddr has first been set.

### Port (cgprsAccPtRpDestPort)

Destination port number of the route probe packet when cgprsAccPtRpProtocol is set to udp. This object can be set only after cgprsAccPtRpDestAddr has first been set.

### TTL Value (cgprsAccPtRpTtl)

Indicates the TTL value set in the route probe packet. This object can be set only after cgprsAccPtRpDestAddr has first been set.