# CDMA PDSN PCF & SO Based Statistics

From this dialog box, you can view Packet Control Function (PCF) and Service Option (SO)-based statistics.

## Navigation

1. Right-click the Mobile Wireless Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN PCF & SO Based Statistics.

The following information is displayed:

> IP Address (cCdmaPcfSoRpRegIpAddr)

> Service Option (cCdmaPcfSoRpRegServiceOption)

With an entry selected in the PCFs & Service Options table, you can open the following dialog boxes:

> Click RP Registration Statistics to open the RP Registration Accepted Statistics dialog box.

> Click RP Update Statistics to open the RP Update Statistics dialog box.

> Click PPP Setup Statistics to open the PPP Setup Statistics dialog box.

### IP Address (cCdmaPcfSoRpRegIpAddr)

IP address of the PCF that serves the mobile node.

### Service Option (cCdmaPcfSoRpRegServiceOption)

The service option received as part of the registration request.