# X.25 Operational Status

The X.25 operations status dialog box shows the parameters for a port configured for X.25.

The following information appears:

> Interface Mode (x25OperInterfaceMode)

> Max Supported Circuits (x25OperMaxActiveCircuits)

> No PVCs Configured (x25OperNumberPVCs)

> Data Link ID(x25OperDataLinkId)

> X.25 Protocol Version (x25OperProtocolVersionSupported)

Interface Mode (x25OperInterfaceMode)

Identifies DCE/DTE mode in which the interface operates. A value of dxe indicates the role will be determined by XID negotiation at the Link Layer and that negotiation has not yet taken place.

Max Supported Circuits (x25OperMaxActiveCircuits)

Maximum number of circuits the PLE (Packet Level Entity) can support.

No PVCs Configured (x25OperNumberPVCs)

The number of PVCs configured for the PLE (Packet Level Entity). The PVCs use channel numbers from 1 to this number.

Data Link ID (x25OperDataLinkId)

This identifies the instance of the index object in the first table of the most device specific MIB for the interface used by the PLE (Packet Level Entity).

X.25 Protocol Version (x25OperProtocolVersionSupported)

Displays an object identifier that refers to a specific version of the X.25 packet layer protocol.