# Displaying Daughter Board Configuration for a CIP Port

To display the daughter board configuration on a CIP Port from the CiscoView Configure Port window, select Daughter Board from the CATEGORY popup menu:

The following information is displayed:

Type (cipCardDtrBrdType)

Microcode Status (cipCardDtrBrdStatus)

Signal (cipCardDtrBrdSignal)

Online (cipCardDtrBrdOnline)

# Type (cipCardDtrBrdType)

Indicates the channel path interface type.

# Microcode Status (cipCardDtrBrdStatus)

Indicates whether the microcode for the daughter board has been successfully loaded and is executing.

# Signal (cipCardDtrBrdSignal)

In a network using ESCON (Enterprise Systems Connection) channel architecture, the Signal field displays the value True if light has been seen on the fiber and synchronization has been established.

In a network using PCA (Parallel Channel Adapter) architecture with Bus and Tag connections, the Signal field displays the value True if the value Operational Out has been sensed.

# Online (cipCardDtrBrdOnline)

In a network using ESCON channel architecture, the Online field displays the value True when a path has been established with at least one channel.

In a network using PCA (Parallel Channel Adapter) architecture with Bus and Tag connections, the Online field displays the value True when the PCA is online to the channel.