# CDMA PDSN Inter PCF Handoff Registration Update Statistics

From this dialog box, you can view statistics for inter-Packet Control Function (PCF) handoff registration updates.

## Navigation

1. Right-click the Mobile Wireless Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN Inter PCF Handoff Registration Update Statistics.

The following information is displayed:

> Updates by PCF Handoffs (cCdmaRpUpdPcfHandoffs)

> Updates Not Acknowledged (cCdmaRpUpdHandoffNotAckedReqs)

> Updates Acknowledged (cCdmaRpUpdHandoffReceivedAcks)

> Updates Accepted (cCdmaRpUpdHandoffAcceptedReqs)

> Updates Denied (cCdmaRpUpdHandoffDeniedReqs)

> Registration Acknowledgements Discarded (cCdmaRpUpdHandoffDiscardedAcks)

> Initial Updates Sent (cCdmaRpUpdHandoffInitTxdReqs)

> Retransmitted Updates (cCdmaRpUpdHandoffReTxdReqs)

> Note: These statistics are a result of inter-PCF handoffs.

### Updates by PCF Handoffs (cCdmaRpUpdPcfHandoffs)

Number of updated registrations sent as a result of inter-PCF handoffs since system startup.

### Updates Not Acknowledged (cCdmaRpUpdHandoffNotAckedReqs)

Number of A11 registration updates received that were unacknowledged since system startup.

### Updates Acknowledged (cCdmaRpUpdHandoffReceivedAcks)

Number of A11 registration updates received that were acknowledged since system startup.

### Updates Accepted (cCdmaRpUpdHandoffAcceptedReqs)

Number of A11 registration acknowledgements received with the Status field set to zero since system startup.

### Updates Denied (cCdmaRpUpdHandoffDeniedReqs)

Number of A11 registration acknowledgements received with the Status field set to a non-zero value since system startup.

### Registration Acknowledgements Discarded (cCdmaRpUpdHandoffDiscardedAcks )

Number of A11 registration acknowledgements discarded since system startup.

### Initial Updates Sent (cCdmaRpUpdHandoffInitTxdReqs)

Number of initial A11 registration updates sent as the result of inter-PCF handoffs since system startup.

### Retransmitted Updates (cCdmaRpUpdHandoffReTxdReqs)

Number of A11 registration updates that were retransmitted because the initial registration update was not acknowledged or was denied since system startup.