# Physical

Port>Configure>Physical

The following information is displayed:

Name of the Port (portName)

Name assigned to the port by the network administrator.

Type (portType)

Type of physical layer medium used on the port. For example, the type for multimode fiber FDDI would be fddi.

Status (portOperStatus)

Current operational status of the port. The possible values are ok or other.

Configured Speed (portAdminSpeed)

Current operational speed of the port in megabits per second. Possible values include auto detect (the speed is automatically detected from the port), 4Mbps, 10 Mbps, 16Mbps, 100 Mbps, 155 Mbps, or 1Gbps.

Duplex (portDuplex)

Indicates whether the port is operating in half-duplex mode, full-duplex mode, disagree mode (which occurs when the port cannot agree with the far end on port duplex), or auto mode (the port automatically determines and sets the appropriate duplex mode). This field does not apply to Token Ring ports.

Port's VLAN (vlanPortVlan)

VLAN identification number for this port.

VLAN Port Admin Status (vlanPortAdminStatus)

Indicates whether the port will get assigned to a VLAN statically or dynamically. When set to dynamic, the needed information is accessed from one of the VLAN Membership Policy Servers specified in the vmpsTable. The default value is static (1).

Note: vlanPortAdminStatus cannot be set to dynamic (2) for a port that has portSecurityAdminStatus set to enabled (1), or for a port that currently has a vlanPortIslOperStatus of trunking (1).

VLAN Port Operational Status (vlanPortOperStatus)

Indicates the current VLAN port status. Inactive (1) status indicates a dynamic port without a VLAN assigned or a static on dynamic port with an inactive assigned VLAN. Active (2) status indicates an active assigned VLAN. Shutdown (3) status indicates the port has been shut down as a result of a VMPS response on a dynamic port. A status of vlanActiveFault (4) only applies to token ring ports.

Voice VLAN ID (vmVoiceVlanId)

The Voice VLAN ID (VVID) to which this port belongs. Valid values range from zero to 4096, as described below:

- 0—CDP packets transmitting through this port contain an Appliance VLAN-ID TLV with a value of zero. VoIP and related packets are both sent and received with a VLAN-ID of zero and an 802.1p priority.
- 1 through 4094—CDP packets transmitting through this port contain an Appliance VLAN-ID TLV with a value of N (where N equals the VVID specifed by this object). VoIP and related packets are both sent and received with a VLAN-ID of N and an 802.1p priority.
- 4095—CDP packets transmitting through this port contain an Appliance VLAN-ID TLV with a value of 4095. VoIP and related packets are both sent and received untagged without an 802.1p priority set.
- 4096—CDP packets transmitting through this port do not contain an Appliance VLAN-ID TLV. Or, if this VVID is not supported by the port, then this MIB object cannot be configured and returns a value of 4096.

Click Apply to make your changes take effect, or click Cancel to close the dialog box without making any changes. Click Print to print the contents of the dialog box.