# RS-232A Port Configuration Information

The RS232A port configuration information dialog box shows the following information for an EIA/TA-232A port:

> Index (rs232AsyncPortIndex)

> Bits per Char (rs232AsyncPortBits)

> Stop Bits (rs232AsyncSTopBits)

> Parity (rs232AsyncPortParity)

> Auto Baud (rs232AsyncPortAutoBaud)

Index (rs232AsyncPortIndex)

Specifies the rs232PortIndex number of the port.

Bits per Char (rs232AsyncPortBits)

Specifies the number of bits in a character.

Stop Bits (rs232AsyncPortSTopBits)

Specifies the number of stop bits. Possible values are 1, 2, 1 1/2, and dynamic.

Parity (rs232AsyncPortParity)

Specifies the type of parity bit for each character. Possible values are none, odd, even, mark, and space.

Autobaud (rs232AsyncPortAutobaud)

Specifies whether the port is enabled for autobaud transmission. Enabled means that the port senses input speed, parity, and character size automatically.