# SRP Configure Destination

Use this option to view packet count and number of packets rejected for a destination address on a particular SRP interface.

## Procedure

To access configure destination information:

1. Right-click the port and select SRP Interface Statistics from the pop-up menu.

The MAC Layer Traffic dialog box appears.

2. Select SRP Configure Destination from the Category menu to display configure destination information.

Configure Destination dialog box displays:

Send Packets (srpMACCountPktsByDestinationFlag)

Address to Send Packets (srpMACCountPktsByDestAddress)

Last Change (srpMACDestDiscontTimeStamp)

Reject Packets (srpMACRejectPktsByDestFlag)

Reject Packets to Address (srpMACRejectPktsByDestAddress)

## Related Topics

Using CiscoView Interface

Using the Main Menu

Selecting Components

Configuring Devices and Components

Monitoring Devices and Components

### Send Packets (srpMACCountPktsByDestinationFlag)

Shows that packets are counted for a particular destination address.

### Address to Send Packets (srpMACCountPktsByDestAddress)

Shows the destination address for which packets are counted when corresponding instance of srpMACCountPktsByDestinationFlag is true.

### Last Change (srpMACDestDiscontTimeStamp)

sysUpTime when there was a change in the corresponding instances of either srpMACCountPktsByDestAddress or srpMACCountPktsByDestFlag.

### Reject Packets (srpMACRejectPktsByDestFlag)

Shows that packets are rejected for a particular destination address.

### Reject Packets to Address (srpMACRejectPktsByDestAddress)

Shows the destination address for which packets are to be rejected when corresponding instance of srpMACCountPktsByDestFlag is true.