# Transmit Side High Priority Traffic Statistics

Dialog box displays following information:

Unicast High Priority Packets (srpHostIntUcastHighPriPktsOut)

UniCast High Priority Octets (srpHostIntUcastHighPriOctetsOut)

MultiCast High Priority Packets (srpHostIntMcastHighPriPktsOut)

MultiCast High Priority Octets (srpHostIntMcastHighPriOctetsOut)

Unicast High Priority Packets (srpHostIntUcastHighPriPktsOut)

Number of high priority unicast packets going to higher layer during a 15-minute interval during past 24 hours.

UniCast High Priority Octets (srpHostIntUcastHighPriOctetsOut)

Number of high priority uncast octets going to higher layer during a 15-minute interval during past 24 hours.

MultiCast High Priority Packets (srpHostIntMcastHighPriPktsOut)

Number of high priority multicast packets going to higher layer during a 15-minute interval during past 24 hours.

MultiCast High Priority Octets (srpHostIntMcastHighPriOctetsOut)

Number of high priority multicast octets going to higher layer during a 15-minute interval during past 24 hours.