# SSG TCP Redirect Group

This dialog box displays details on the Service Selection Gateway (SSG) TCP redirect group.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select SSG TCP Redirect Group from the Category list.

The following information is displayed:

> Redirect-Group Name (cssgTcpRedirectGrpName)

> Redirect Server Type (cssgTcpRedirectGrpServerAddrType)

> Redirect Server (cssgTcpRedirectGrpServerAddr)

> Redirection port (cssgTcpRedirectGrpServerPort)

> Redirection Row Status (cssgTcpRedirectGrpRowStatus)

### Redirect-Group Name (cssgTcpRedirectGrpName)

Name of the redirect group.

### Redirect Server Type (cssgTcpRedirectGrpServerAddrType)

Value that represents the type of address stored in cssgTcpRedirectGrpServerAddr.

### Redirect Server (cssgTcpRedirectGrpServerAddr)

IP address of the server in the server group.

### Redirection port (cssgTcpRedirectGrpServerPort)

Port of the server to which TCP traffic is to be redirected.

### Redirection Row Status (cssgTcpRedirectGrpRowStatus)

Status of the table entry. Change the status to create a new table entry or delete an existing one.

- To create a row, set the object to createAndGo. There are no mandatory objects in a create request.

- To delete a row, set the object to destroy.