# Policy Names

Configuration > Policies > Policer Names

This dialog box displays a list of configured flow policies. A flow policy is a rule consisting of normal rate, excess rate, burst rate, and drop-or-mark indication. From here, you can launch dialog boxes to add, edit, or delete policies.

To view the definition for this MIB variable, click the following link:

- Configured Policies (caqFlowPolicerName)

The following list specifies buttons in this dialog box, as well as their function:

- Click Add Policy to open the Add/Edit Policy dialog box and add a new policy.

- Click Edit Policy to open the Add/Edit Policy dialog box and edit an existing policy.

- Click Delete Policy to remove an existing policy.

- Click OK to continue.

- Click Cancel to close the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access the online help.

Configured Policies (caqFlowPolicerName)

The name of a policy.

The following table outlines which policy types are supported by the IP, IPX, and MAC interfaces on Sup1 and Sup2 supervisor cards.

Table 1: Policy Types Supported

Policy Type | Sup1 Card | Sup2 Card
IP | IPX | MAC | IP | IPX | MAC
Micro Flow | Yes | No | No | Yes | No | No
Aggregate Flow | Yes | Yes | Yes | Yes | Yes | Yes
No Trust | Yes | Yes | Yes | Yes | No | No
Trust CoS | Yes | Yes | Yes | Yes | Yes | Yes
DSCP | Yes | No | No | Yes | No | No
IP Prec | Yes | No | No | Yes | No | No