# RP Registration Accepted Statistics

From this dialog box, you can view Packet Control Function (PCF) and Service Option (SO)-based Radio Packet (RP) registration accepted statistics.

## Navigation

1. Right-click the Mobile Wireless Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN PCF & SO Based Statistics.

4. With an entry selected in the PCFs & Service Options table, click RP Registration Statistics.

The following information is displayed:

> Registration Requests Received (cCdmaPcfSoRpRegRcvdReqs)

> Registration Requests Accepted (cCdmaPcfSoRpRegAcptdReqs)

> New Connection Requests Accepted (cCdmaPcfSoRpInitRegAcptdReqs)

> Re-registration Requests Accepted (cCdmaPcfSoRpReRegAcptdReqs)

> De-registration Requests Accepted (cCdmaPcfSoRpDeRegAcptdReqs)

> Accepted Handoff A11 Registrations (cCdmaPcfSoRpHandoffRegAcptdReqs)

### Registration Requests Received (cCdmaPcfSoRpRegRcvdReqs)

Number of A11 registration requests received since system startup.

### Registration Requests Accepted (cCdmaPcfSoRpRegAcptdReqs)

Number of A11 registration requests accepted since system startup.

### New Connection Requests Accepted (cCdmaPcfSoRpInitRegAcptdReqs)

Number of A11 registration requests meant for establishing new RP connections that have been accepted since system startup.

### Re-registration Requests Accepted (cCdmaPcfSoRpReRegAcptdReqs)

Number of A11 registration requests meant for refreshing established RP connections that have been accepted since system startup.

### De-registration Requests Accepted (cCdmaPcfSoRpDeRegAcptdReqs)

Number of A11 registration requests meant for closing established RP connections that have been accepted since system startup.

### Accepted Handoff A11 Registrations (cCdmaPcfSoRpHandoffRegAcptdReqs)

Total number of accepted handoff A11 Registration Requests meant for already existing sessions, since the system was last restarted.

Note: This object is available for PDSN version 3.0 and later.