# IPSec VLAN Configuration

The IPSec VLAN Configuration dialog box enables you to create crypto VLANs and specify the configuration mode.

## Procedure

1. Right-click the IPSec VPN Service Blade, then select VPN Service Blade Setup Wizard. The IPSec VPN Service Blade VLAN Configuration dialog box appears.

2. Click Create.

The following information appears:

Mode of Operation

Click Configure to configure the VLAN in the selected mode.

### Mode of Operation

Mode in which the crypto VLAN can be configured. Mode can be access, routed, or trunk.