# GGSN Transmitted

The GGSN Transmitted category of the Chassis Monitoring dialog box lists statistics of what the GGSN transmitted.

Note: This dialog can be viewed if cGtpGSNService is set to 'ggsn'.

## Procedure

1. Right-click the device, and select Monitor.

2. Select GGSN Transmitted.

The following information appears:

GTP Sent (cGgsnSentSigMessages)

G-PDU Sent (cGgsnSentGPDUs)

G-PDU Total bytes sent (cGgsnHCSentGPDUOctets)

### GTP Sent (cGgsnSentSigMessages)

The number of GTP signaling messages sent by the GGSN.

### G-PDU Sent (cGgsnSentGPDUs)

The number of G-PDU messages sent by the GGSN.

### G-PDU Total bytes sent (cGgsnHCSentGPDUOctets)

The number of total bytes sent in G-PDU messages.