# CDMA PDSN Cluster Controller General

This dialog box is applicable to Controller clusters. From here, you can view the general controller details of the packet data serving node (PDSN).

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Configure.

3. Select CDMA PDSN Cluster Controller General.

The following information is displayed:

> Max Sessions Allowed (cCdmaClusterSessHighThreshold)

> Low Sessions Allowed (cCdmaClusterSessLowThreshold)

> Record Count (cCdmaClusterTotalMembers)

### Max Sessions Allowed (cCdmaClusterSessHighThreshold)

Maximum number of allowed sessions. The agent generates a notification when this threshold is reached during call setup.

### Low Sessions Allowed (cCdmaClusterSessLowThreshold)

Minimum number of allowed sessions. The agent generates a notification when this threshold is reached during call release.

### Record Count (cCdmaClusterTotalMembers)

Total number of records in the PDSN cluster controller.