# FDDI Station Management Information

In addition to the card interface-level information that is common to all cards, the CiscoView configure card window displays two card configuration fields that are exclusive to FDDI cards:

| Station ID (fddimibSMTStationId) | Displays an 8-octet string that uniquely identifies the FDDI station.
| Operation Version (fddimibSMTOpVersionId) | Specifies an ANSI-defined version of SMT that is being used for operation.