# SSG Service Table

This dialog box displays details on the Service Selection Gateway (SSG) service table.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select SSG Service Table from the Category list.

The following information is displayed:

> Service Name (cssgServiceName)

> Service Mode (cssgServiceMode)

> Service Type (cssgServiceType)

> Idle Timeout (cssgServiceIdleTimeout)

> Session Length (cssgServiceSessionTimeout)

> Active Sessions (cssgServiceActiveSessions)

> Primary DNS Type (cssgServiceDNSPrimaryIpType)

> Primary DNS (cssgServiceDNSPrimary)

> Secondary DNS Type (cssgServiceDNSSecondaryIpType)

> Secondary DNS (cssgServiceDNSSecondary)

> Upstream Status (cssgServiceUpstreamQOSEnabled)

> Downstream Status (cssgServiceDownStreamQOSEnabled)

> Open Garden Status (cssgServiceOpenGarden)

> Prepaid Status (cssgServicePrepaid)

### Service Name (cssgServiceName)

Name of the service profile.

### Service Mode (cssgServiceMode)

An optional attribute that indicates whether you can log in to another service while using the SSG service. There are three possible values:

Value | Description
1 | unknown
2 | concurrent
3 | sequential (you cannot log in to another service)

### Service Type (cssgServiceType)

Type of service. There are four possible values:

Value | Description
1 | unknown
2 | pass-through: Means that user authentication is not done during logon to this service. This is the default.
3 | tunnel: L2TP tunneled service
4 | proxy: Means that SSG performs authentication during logon to the service.

### Idle Timeout (cssgServiceIdleTimeout)

Amount of time, in seconds, a session can idle before it times out.

### Session Length (cssgServiceSessionTimeout)

Maximum length of a session in seconds.

### Active Sessions (cssgServiceActiveSessions)

Number of active connections to the service.

### Primary DNS Type (cssgServiceDNSPrimaryIpType)

IP address type of the primary DNS server for the service.

### Primary DNS (cssgServiceDNSPrimary)

Primary DNS server for the service.

### Secondary DNS Type (cssgServiceDNSSecondaryIpType)

IP address type of the secondary DNS server for the service.

### Secondary DNS (cssgServiceDNSSecondary)

Secondary DNS server for the service.

### Upstream Status (cssgServiceUpstreamQOSEnabled)

Indicates whether upstream policing is enabled for the service.

### Downstream Status (cssgServiceDownStreamQOSEnabled)

Indicates whether downstream policing is enabled for the service.

### Open Garden Status (cssgServiceOpenGarden)

Indicates whether the service is of the open garden type.

An open garden service can be accessed without authentication.

### Prepaid Status (cssgServicePrepaid)

Indicates whether the service is pre-paid.