# Foreign Agent Registration Statistics2

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select Foreign Agent Registration Statistics2.

The following information is displayed:

> Encapsulation Unavailable - Regns Rejected (faEncapsulationUnavailable)

> VJ Comp Unavailable - Regns Rejected(faVJCompressionUnavailable)

> HA Unreachable - Regns Rejected ( faHAUnreachable)

> Regn Replies Received (faRegRepliesRecieved)

> Regn Replies Relayed (faRegRepliesRelayed)

> HA Authentication Failure - Regns Rejected (faHAAuthenticationFailure)

> Poorly Formed Replies (faPoorlyFormedReplies)

### Encapsulation Unavailable - Regns Rejected (faEncapsulationUnavailable)

Total number of registration requests denied by the foreign agent—requested encapsulation unavailable (code 72).

### VJ Comp Unavailable - Regns Rejected(faVJCompressionUnavailable)

Total number of registration requests denied by the foreign agent—requested Van-Jacobson header compression unavailable (code 73).

### HA Unreachable - Regns Rejected ( faHAUnreachable)

Total number of registration requests denied by the foreign agent—home agent unreachable (codes 80-95).

### Regn Replies Received (faRegRepliesRecieved)

Total number of well-formed registration replies received from by the foreign agent.

### Regn Replies Relayed (faRegRepliesRelayed)

Total number of registration replies relayed to the mobile node by the foreign agent.

### HA Authentication Failure - Regns Rejected (faHAAuthenticationFailure)

Total number of registration replies denied by the foreign agent—home agent failed authentication (code 68).

### Poorly Formed Replies (faPoorlyFormedReplies)

Total number of registration replies denied by the foreign agent—poorly formed reply (code 71).