# Aggregator Configuration

Device > Configure > Aggregator

The Aggregator Configuration dialog box provides information on the protocol and address mode configurations for this device. The following data is displayed:

- Distribution Protocol (clagAggDistributionProtocol)

- Distribution Address Mode (clagAggDistributionAddressMode)

This dialog box also provides a table which lists the ports associated with each aggregator on the system. The following data is displayed:

- Index (dot3adAggIndex)

- Port List (dot3adAggPortListPorts)

Do one of the following:

- Click OK to continue.

- Click Apply to save the changes made in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Distribution Protocol (clagAggDistributionProtocol)

Controls the protocol address type (for example, MAC or IP) used on this LACP interface to distribute outgoing data frames among its component interfaces.

Distribution Address Mode (clagAggDistributionAddressMode)

Load balancing address mode for the device. It can be a Source address, Destination address, or both.

Index (dot3adAggIndex)

Unique identifier assigned to this aggregator by the local system.

Port List (dot3adAggPortListPorts)

Complete set of ports currently associated with this aggregator. Port numbers are displayed in the following format: module/port(s). For example, the value "4/2-3" indicates that module 4, ports 2 and 3 are associated with this aggregator.