# Fabric Error Recovery Objects

## Navigation

Device > Configure > Error Recovery

The following information appears:

> Threshhold Link (cc6kxbarErrRcvryThreshLink)

> ThreshPers Link (cc6kxbarErrRcvryThreshPersLink)

> Switchover Enable (cc6kxbarErrRcvrySwitchoverEnable)

### Threshhold Link (cc6kxbarErrRcvryThreshLink)

The threshold configured for fabric link errors that take place in a fabric error recovery channel.

### ThreshPers Link (cc6kxbarErrRcvryThreshPersLink)

The threshold configured for persistent fabric link errors that take place in a fabric error recovery channel.

### Switchover Enable (cc6kxbarErrRcvrySwitchoverEnable)

Indicates whether the switchover to the standby fabric module is enabled upon the detection of excessive fabric link errors that have taken place in a fabric error recovery channel.