# Encryption Engine Status Table

Provides the following essential identification and status information for each encryption engine:

Engine ID(cieEngineID)

Engine Card Number(cieEngineCardIndex)

ESA Tampered With(cieEsaTampered)

ESA Authenticated(cieEsaAuthenticated)

ESA Mode(cieEsaMode)

Engine Public Key(cieEnginePublicKey)

# Engine ID(cieEngineID)

A value uniquely identifying an encryption engine. Software engines use the processor ID, the ESA card uses its own ID.

# Engine Card Number(cieEngineCardIndex)

The card number of the ESA. A software engine uses the value 0 (zero).

# ESA Tampered With(cieEsaTampered)

Indicates whether the ESA card has been tampered with. Software encryption engines do not provide this value.

# ESA Authenticated(cieEsaAuthenticated)

Indicates whether or not this ESA card has been properly authenticated for this router. Software encryption engines do not provide this value.

# ESA Mode(cieEsaMode)

The current operating mode of the ESA card, corresponding to the LED status shown on the ESA card. Software engines do not provide this value.

# Engine Public Key(cieEnginePublicKey)

The public key that the particular engine uses.