# GGSN APN Generic

The GGSN APN Generic dialog box lists access point system information.

Note: This dialog box is available only if the value of cGtpGSNService is set to ggsn.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select GGSN APN Generic from the Category drop-down box.

The following information is displayed:

> Notification Controller (cgprsAccPtCfgNotifEnable)

> Max History Table Size (cgprsAccPtCfgNotifHistMax)

> Latest Entries Index (cgprsAccPtCfgNotifLatestIndex)

### Notification Controller (cgprsAccPtCfgNotifEnable)

When the value of this object is true(1), cgprsAccPtCfgNotif notifications are generated. Otherwise, they are not.

Note: Entries in cgprsAccPtCfgNotifHistTable are generated regardless of the value of this object.

### Max History Table Size (cgprsAccPtCfgNotifHistMax)

Maximum number of entries in the event history table cgprsAccPtCfgNotifHistTable.

When the table is full, the oldest entries are removed to make space for new entries.

### Latest Entries Index (cgprsAccPtCfgNotifLatestIndex)

Value of cgprsAccPtCfgNotifIndex for the most recently created entry in cgprsAccPtCfgNotifHistTable.