# Home Agent Mobility Table

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Configure.

3. Select Home Agent Mobility Table.

The following information is displayed:

> MN Ip Address (haMobilityBindingMN)

> MN Care of Address (haMobilityBindingCOA)

> Source Ip Address (haMobilityBindingSourceAddress)

> Registration Flags (haMobilityBindingRegFlags)

> 4 LSBs of Identifier (haMobilityBindingRegIDLow)

> 4 MSBs of Identifier (haMobilityBindingRegIDHigh)

> Total Registration Lifetime (haMobilityBindingTimeGranted)

> Remaining Lifetime (haMobilityBindingTimeRemaining)

### MN Ip Address (haMobilityBindingMN)

Home IP address of the mobile node.

### MN Care of Address (haMobilityBindingCOA)

Mobile node's care-of-address. One mobile node can have multiple bindings with different care-of-addresses.

### Source Ip Address (haMobilityBindingSourceAddress)

Source IP address of the registration request received by the home agent. This is either a mobile node's co-located care-of-address or an address of the foreign agent.

### Registration Flags (haMobilityBindingRegFlags)

Registration flags sent by the mobile node.

### 4 LSBs of Identifier (haMobilityBindingRegIDLow)

Low-order 32 bits of identification used in a binding by the mobile node.

### 4 MSBs of Identifier (haMobilityBindingRegIDHigh)

High-order 32 bits of identification used in a binding by the mobile node.

### Total Registration Lifetime (haMobilityBindingTimeGranted)

Lifetime, in seconds, granted to the mobile node for this registration.

### Remaining Lifetime (haMobilityBindingTimeRemaining)

Seconds remaining until the registration expires. This object has the same initial value as haMobilityBindingTimeGranted and is counted down by the home agent.