# RSVP Sender Information

Displays the status information displayed by senders in PATH messages.

> Sender Number (rsvpSenderNumber)

> Sender Type (rsvpSenderType)

> Destination Address (rsvpSenderDestAddr)

> Sender Address (rsvpSenderAddr)

> Destination Address Length (rsvpSenderDestAddrLength)

> Sender Address Length (rsvpSenderAddrLength)

> Protocol (rsvpSenderProtocol)

> Destination Port (rsvpSenderDestPort)

> Sender Port (rsvpSenderPort)

> Flow ID (rsvpSenderFlowId)

> Sender Policy (rsvpSenderPolicy)

> Sender Status (rsvpSenderStatus)

> Sender TTL (rsvpSenderTTL)

Sender Number (rsvpSenderNumber)

Number of the specified sender. This value is used for SNMP Indexing only and has no relation to any protocol value.

Sender Type (rsvpSenderType)

Type of session. The value could be IP4, IP6, or IP6 with flow information.

Destination Address (rsvpSenderDestAddr)

Destination address used by all senders in a session. The value of this object may not be changed when the value of the RowStatus object is active.

Sender Address (rsvpSenderAddr)

Source address used by the specified sender in a session.

The value of this object may not be changed when the value of the RowStatus object is active.

Destination Address Length (rsvpSenderDestAddrLength)

CIDR prefix length of the destination address in bits. The value for IP4 hosts and multicast addresses is 32. The value of this object may not be changed when the value of the RowStatus object is active.

Sender Address Length (rsvpSenderAddrLength)

CIDR prefix length of the sender's address in bits. The value for IP4 hosts and multicast addresses is 32. The value of this object may not be changed when the value of the RowStatus object is active.

Protocol (rsvpSenderProtocol)

Indicates the internet protocol used by a session.

Value of this object may not be changed when the value of RowStatus object is active.

Destination Port (rsvpSenderDestPort)

UDP or TCP port number used as a destination port for all senders in a session.

If the IP protocol in use, specified by rsvpSenderProtocol, is 50 (ESP) or 51 (AH), this represents a virtual destination port number. If the value is zero, the IP protocol in use does not have any port.

The value of this object may not be changed when the value of the RowStatus object is active.

Sender Port (rsvpSenderPort)

UDP or TCP port number used as a source port the sender in a session.

If the IP protocol is 50 (ESP) or 51 (AH), the destination port represents a virtual destination port number. If the value is zero, the IP protocol does not have any port. The value of this object may not be changed when the value of the RowStatus object is active.

FlowId (rsvpSenderFlowId)

Indicates the flow ID the sender is using for an Ipv6 session.

Sender Policy (rsvpSenderPolicy)

Contents of the policy object, displayed as an uninterrupted string of octets, including the object header. Value is zero if no policy object is present.

Sender Status (rsvpSenderStatus)

Status of PATH messages. Active is displayed for all active PATH messages.

Sender Status is used for installing or deleting PATH information.

Sender TTL (rsvpSenderTTL)

TTL value in the last received RSVP header.