# CDMA PDSN Cluster

This dialog box is applicable to Controller, Member, and Peer to Peer clusters. From here, you can view the packet data serving node (PDSN) cluster details for this card.

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Configure.

3. Select CDMA PDSN Cluster.

The following information is displayed:

> PDSN Cluster (cCdmaClusterType)

> Role in Cluster (cCdmaClusterRole)

### PDSN Cluster (cCdmaClusterType)

Type of PDSN cluster. There are three possible values:

Value | Description
0 | nonCluster
1 | peerToPeer
2 | controllerMember

### Role in Cluster (cCdmaClusterRole)

Role the PDSN plays within a controller member type of cluster. There are three possible values:

Value | Description
0 | notApply - Means the PDSN does not play any cluster role. PDSN has this role if cCdmaClusterType is not controllerMember.
1 | controller - PDSN is the controller of the cluster.
2 | member - PDSN is a member of the cluster.