# Crossbar Channel Statistics

Supervisor module > Configure > Crossbar Channel Statistics

This dialog box monitors crossbar channel statistics for this module.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Module Slot Number (cc6kxbarStatisticsModule)

- Crossbar Statistics Channel (cc6kxbarStatisticsChannel)

- Cross Bar In Errors (cc6kxbarStatisticsInErrors)

- Cross Bar Out Errors (cc6kxbarStatisticsOutErrors)

- Cross Bar Out Dropped (cc6kxbarStatisticsOutDropped)

- Channel Input Utilization (cc6kxbarStatisticsInUtil)

- Channel Output Utilization (cc6kxbarStatisticsOutUtil)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Module Slot Number (cc6kxbarStatisticsModule)

Module slot number.

Crossbar Statistics Channel (cc6kxbarStatisticsChannel)

Fabric channel number associated with the statistics module.

Cross Bar In Errors (cc6kxbarStatisticsInErrors)

Total number of error packets received on cc6kxbarStatisticsChannel for cc6kxbarStatisticsModule.

Cross Bar Out Errors (cc6kxbarStatisticsOutErrors)

Total number of error packets transmitted on cc6kxbarStatisticsModule through the cc6kxbarStatisticsChannel.

Cross Bar Out Dropped (cc6kxbarStatisticsOutDropped)

Total number of dropped packets transmitted on the cc6kxbarStatisticsChannel for cc6kxbarStatisticsModule.

Channel Input Utilization (cc6kxbarStatisticsInUtil)

Input utilization of the cc6kxbarStatisticsChannel for cc6kxbarStatisticsModule.

Channel Output Utilization (cc6kxbarStatisticsOutUtil)

Output utilization of the cc6kxbarStatisticsChannel for cc6kxbarStatisticsModule.