# MR Statistics

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Statistics button.

4. Select category MR Statistics.

The following information appears:

New HA Registration (cmiMrRegNewHa)

> Better Interface Detect (cmiMrBetterIfDetected)

> Packets on MR-HA Tunnel (cmiMrTunnelPktsRcvd)

> Packets Sent (cmiMrTunnelPktsSent)

> Bytes Received (cmiMrTunnelBytesRcvd)

> Bytes Sent (cmiMrTunnelBytesSent)

> Active Redundancy State (cmiMrRedStateActive)

> Passive Redundancy State (cmiMrRedStatePassive)

### New HA Registration (cmiMrRegNewHa)

Number of times a mobile router registers with a different home agent due to changes in home agent / home agent priority.

### Better Interface Detect (cmiMrBetterIfDetected)

Number of times that the mobile router has detected a better interface.

### Packets on MR-HA Tunnel (cmiMrTunnelPktsRcvd)

Number of packets received on the mobile router-home agent tunnel.

### Packets Sent (cmiMrTunnelPktsSent)

Number of packets sent through the mobile router-home agent tunnel.

### Bytes Received (cmiMrTunnelBytesRcvd)

Number of bytes received on the mobile router-home agent tunnel.

### Bytes Sent (cmiMrTunnelBytesSent)

Number of bytes sent through the mobile router-home agent tunnel.

### Active Redundancy State (cmiMrRedStateActive)

Number of times the redundancy state of the mobile router changed to active.

### Passive Redundancy State (cmiMrRedStatePassive)

Number of times the redundancy state of the mobile router changed to passive.