# Frame Relay Port Configuration Information

Data Link Connection Management Information:

State

Address

Address Length

Status Enq Msg Intervals

Max Errs Enq Status Msg

Multicast Service

Max Virtual Circuits

Data Link Connection Identifier Information:

Oper State

Last Change

Max Committed Bits

Max Uncommitted Bits

# State (frDlcmiState)

Displays the type of connection management scheme that is active at this interface. Possible values are noLmiConfigured, LmiRev1, ansiT1-617-D, or ansiT1-617-B.

# Address (frDlcmiAddress)

Displays the address format used. Possible values are as follows:

Address Format | Meaning
21 | bit DLCI
22March90 | bit DLCI
22November90 | bit DLCI
22 | final standard

# Address Length (frDlcmiAddressLen)

Specifies the address length in octets. Possible values are two-octets, three-octets, or four-octets. For the address format q922, the length includes both the address and control portions.

# Status Enq Msg Intervals (frDlcmiFullEnquiryInterval)

Displays the number of status inquiry intervals before a full status inquiry message is issued. Possible values are 1 to 255.

# Max Errs Enq Status Msg (frDlcmiErrorThreshold)

Displays the maximum number of unanswered status inquiries allowed before the interface is declared down. Possible values are 1 to 10.

# Multicast Service (frDlcmiMulticast)

Indicates whether the interface uses a multicast service. Possible values are nonBroadcast or broadcast.

# Max Virtual Circuits (frDlcmiMaxSupportedVCs)

Specifies the maximum number of virtual circuits allowed for this interface.

# Oper State (frCircuitState)

Displays the operational state of this circuit. Possible values are invalid, active, or inactive.

If you set an entry to invalid, the circuit is deleted.

# Last Change

Specifies in time ticks the value of the sysUpTime MIB descriptor when the state of the virtual circuit last changed.

# Max Committed Bits (frCircuitCommittedBurst)

Specifies the maximum bits of data that the network agrees to transfer under normal conditions during the measurement interval.

# Max Uncommitted Bits (frCircuitExcessBurst)

Specifies the number of uncommitted bits of data that the network attempts to transfer under normal conditions during the measurement interval.