# RP Update Registration Failures Contd

## Navigation

1. Right-click the device, and select Monitor. The Monitor Device dialog box appears.

2. Select CDMA PDSN PCF & SO Based Statistics from the Category list.

3. Select a row and click the RP Update Statistics button.

4. Select RP Update Registration Failures Contd from the Category list.

The following information appears:

> Unspecified Reasons (cCdmaSoRpUpdHandoffReaUnSpecFails)

> Administrative Prohibition (cCdmaSoRpUpdHandoffAdmProhibFails)

> MN Authentication (cCdmaSoRpUpdHandoffMNAuthenFails)

> Registration Identity Mismatch (cCdmaSoRpUpdHandoffIdMismatchFails)

> Poorly Formed Request (cCdmaSoRpUpdHandoffBadReqFails)

### Unspecified Reasons (cCdmaSoRpUpdHandoffReaUnSpecFails)

The number of update registrations that failed for an unspecified reason since the system was last restarted. The update is sent as a result of inter PCF handoff.

### Administrative Prohibition (cCdmaSoRpUpdHandoffAdmProhibFails)

### The number of update registrations that failed due to administrative prohibition since the system was last restarted. The update is sent as a result of inter PCF handoff.

### MN Authentication (cCdmaSoRpUpdHandoffMNAuthenFails)

The number of update registrations that failed due to mobile node authentication failure since the system was last restarted. The update is sent as a result of inter PCF handoff.

### Registration Identity Mismatch (cCdmaSoRpUpdHandoffIdMismatchFails)

The number of registrations that failed due to registration identity mismatch since the system was last restarted. The update is sent as a result of inter PCF handoff.

### Poorly Formed Request (cCdmaSoRpUpdHandoffBadReqFails)

The number of update registrations that failed due to poorly formed request since the system was last restarted. The update is sent as a result of inter PCF handoff.