# GGSN GTP Director

The GGSN GTP Director category of the Chassis Configuration dialog box displays the GGSN GTP director information.

Note This dialog can be viewed if cGtpGSNService is set to 'gtpdirector'.

## Procedure

1. Right-click the device and then select Configure, or double-click the device.

2. Select GGSN GTP Director from the Category list.

The following information appears:

GPRS Service Type (cGtpGSNService)

Retry same GGSN Timer (cgdCreatePdpRequestInfoSaveTimer)

Send GTP Director Notifications (cgdNotifEnable)

### GPRS Service Type (cGtpGSNService)

Type of GPRS service enabled on the device:

Value | Description
undefined | GPRS service functionality is turned off.
ggsn | Device functions as a GGSN.
sgsn | Device functions as SGSN.
gtpdirector | Device functions as GDM.

When the device is configured to function as GDM, all other objects in this MIB will not be accessible and the CISCO-GTP-DIRECTOR-MIB should be used for managing the device.

### Retry same GGSN Timer (cgdCreatePdpRequestInfoSaveTimer)

When a GDM receives a request to create PDP, it processes and forwards the request to the GGSN and saves information related to the request. This timer defines the time during which the information is maintained by the GDM. Any subsequent retries by the SGSN within this time period is forwarded to the same GGSN, but the timer is not reset if a retry occurs before it expires.

### Send GTP Director Notifications (cgdNotifEnable)

Indicates whether ciscoGtpDirectorNotifications notification is sent when it is generated by the device.

Value | Description
true | Enables the device to send the notification.
false | Prevents the device from sending out the notification.