# CSG Quota Manager Table

## Navigation

1. Right-click the Service and Application Module for IP (SAMI) card and then select Configure.
2. Select SAMI module from the Category drop-down box.
3. With a device selected, click Statistics.
4. Select Content Services Gateway from the Category drop-down box.
5. Select CSG Quota Server from the Category drop-down box.

The following information appears:

> Quota Server VRF Name (ccsQuotaMgrVrfName)

> IP Address Type (ccsQuotaMgrIpAddrType)

> IP Address (ccsQuotaMgrIpAddr)

> Port (ccsQuotaMgrPort)

> Quota Manager State (ccsQuotaMgrState)

### Quota Server VRF Name (ccsQuotaMgrVrfName)

Name of the VPN routing/forwarding (VRF) instance over which communication with the quota manager occurs. If no VRF instance is specified, then the global routing table is used.

### IP Address Type (ccsQuotaMgrIpAddrType)

Indicates the address type of ccsQuotaMgrIpAddr.

### IP Address (ccsQuotaMgrIpAddr)

IP address of a quota manager.

### Port (ccsQuotaMgrPort)

UDP port configured for a quota manager.

### Quota Manager State (ccsQuotaMgrState)

Status of a quota manager. There are six possible values:

> standby—The quota manager is ready to become active.

> failed—The quota manager has failed to respond to requests.

> active—The quota manager is ready to receive requests.

> echowait—An echo request has been sent to this quota manager and is waiting for a response.

> nawait—A node-alive request has been sent to this quota manager and is waiting for a response.

> suspended—The quota manager has received a stop request from the operator.