# MIP Security Associations table

The table displays the following information:

Peer Entity's IpAddress (mipSecPeerAddress)

Security Parameter Index(mipSecSPI)

Security Algorithm (mipSecAlgorithmType)

Security Mode (mipSecAlgorithmMode)

Replay-Protection Method (mipSecReplayMethod)

### Peer Entity's IpAddress (mipSecPeerAddress)

IP address of the peer entity with which the node shares the mobility security association.

### Security Parameter Index(mipSecSPI)

The SPI is the 4-byte opaque index within the Mobility Security Association which selects the specific security parameters to be used to authenticate the peer.

### Security Algorithm (mipSecAlgorithmType)

Type of security algorithm.

Possible values are:

other (1)

md5 (2)

### Security Mode (mipSecAlgorithmMode)

Security mode used by the algorithm.

Possible values are:

other (1)

prefixSuffix (2)

### Replay-Protection Method (mipSecReplayMethod)

The replay-protection method supported for this SPI within the Mobility Security Association.