# GGSN GSN Addressing

The GGSN GSN Addressing category in the Chassis Configuration dialog box lists the GGSN GSN addressing details.

Note This dialog can be viewed if cGtpGSNService is set to 'ggsn'.

## Procedure

1. Right-click the device and then select Configure, or double-click the device.

2. Select GGSN GSN Addressing from the Category list.

The following information appears:

GSN Address Type (cGtpGSNAddressType)

GSN Address (cGtpGSNAddress)

GTP Version (cGtpGSNVersion)

### GSN Address Type (cGtpGSNAddressType)

Type of Internet address by which cGtpGSNAddress can be accessed.

### GSN Address (cGtpGSNAddress)

IP address that uniquely identifies a GSN node.

### GTP Version (cGtpGSNVersion)

GTP version supported by the GSN node, identified by cGtpGSNAddressType and cGtpGSNAddress.

Values are:

- version0 - represents GTP version 0

- version1 - represents GTP version1