# GGSN Service Aware Failure Statistics

1. Right-click on the MWAM Card and select Configure.
2. Select category MWAM module.
3. Select a row and click the Statistics button.
4. Select the category GGSN Service Aware Failure Statistics.

The following information appears:

> GGSN Failures (cGgsnSATotalGgsnFailures )

> CSG Failures (cGgsnSATotalCsgFailures )

> DCCA Total Failures (cGgsnSATotalDccaFailures)

> DCCA Failures (cGgsnSARejDccaFailures)

> CSG Failures (cGgsnSARejCsgFailures)

### GGSN Failures (cGgsnSATotalGgsnFailures )

Number of GGSN failures, such as, when GGSN fails to communicate with the Content Service Gateway (CSG) or fails to receive a response from the Diameter Credit Control Application (DCCA) server.

### CSG Failures (cGgsnSATotalCsgFailures )

Number of Content Service Gateway failures in communication with the quota server.

### DCCA Total Failures (cGgsnSATotalDccaFailures)

Number of failures in the DCCA server.

### DCCA Failures (cGgsnSARejDccaFailures)

Number of Packet Data Protocol (PDP) sessions that have been rejected due to DCCA failure.

### CSG Failures (cGgsnSARejCsgFailures)

Number of rejected PDPs due to CSG failure.