# Mobility Agent Advertisement Table

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Configure.

3. Select Mobility Agent Advertisement Table.

The following information is displayed:

> Source Ip Address (maInterfaceAddress)

> Max Registration Lifetime (maAdvMaxRegLifetime)

> Prefix Length Extension (maAdvPrefixLengthInclusion)

> Destination Ip Address (maAdvAddress)

> Max Advertisement Interval (maAdvMaxInterval)

> Min Advertisement Interval (maAdvMinInterval)

> Advertise On Solicitation (maAdvResponseSolicitationOnly)

> Row Status (maAdvStatus)

### Source Ip Address (maInterfaceAddress)

IP address of the advertisement interface.

### Max Registration Lifetime (maAdvMaxRegLifetime)

Longest lifetime, in seconds, that the mobility agent is willing to accept in any registration request.

### Prefix Length Extension (maAdvPrefixLengthInclusion)

When this object is set to "true", advertisements sent over the interface include the prefix-lengths extension.

### Destination Ip Address (maAdvAddress)

IP destination address to be used for advertisements sent from the interface. The only permissible values are the all-systems multicast address (224.0.0.1) or the limited-broadcast address (255.255.255.255).

### Max Advertisement Interval (maAdvMaxInterval)

Maximum time interval, in seconds, between successive transmissions of agent advertisements from the interface.

### Min Advertisement Interval (maAdvMinInterval)

Minimum time interval, in seconds, between successive transmissions of agent advertisements from the interface.

### Advertise On Solicitation (maAdvResponseSolicitationOnly)

Indicates whether an advertisement should only be sent from the interface in response to an agent solicitation message.

### Row Status (maAdvStatus)

Status of a particular row in the agent advertisement table. If the current status of a column is "active", the manager should not modify any columns associated with that row.