# IP Permit

Device>Configure>IP Permit

Use the IP Permit dialog box to configure the IP Permit feature on the device and list the addresses of known IP Permit hosts.

IP Permit (ipPermitEnable)

Enables or diables the IP Permit feature. Change this value as necessary and click Apply.

The IP Permit List Table displays up to 10 IP addresses with the network masks of IP permit hosts. Click Create to add a new entry to the table, or click Delete to delete the selected entry.

IP Address (ipPermitAddress)

IP address of an IP permit host.

IP Mask (ipPermitMask)

IP network mask for this IP permit host.

IP Access Type (ipPermitAccessType)

IP access type of a IP permit host.

The Access Attempts From Invalid IP Addresses Table lists up to 10 of the most recently denied IP addresses with the access type.

Address (ipPermitDeniedAddress)

IP address of a IP permit denied access.

Time (ipPermitDeniedTime)

The time (in hundredths of a second) since the IP permit denied access happened.

Access Type (ipPermitDeniedAccess)

Denied access type: Telnet or SNMP.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.