# CDMA PDSN Inter PCF Handoff Registration Update Failures

Use this option to view Inter Packet Control Function (PCF) Handoff Registration Update Failures.

## Procedure

To access CDMA PDSN Inter PCF Handoff Registration Update Failures information

1. Right-click the device and select Monitor from the popup menu.

2. Select CDMA PDSN Inter PCF Handoff Registration Update Failures from the Category menu.

The following information appears:

> Unspecified Failures (cCdmaRpUpdHandoffReaUnSpecFails)

> Administrative Failures (cCdmaRpUpdHandoffAdmProhibFails)

> MN Authentication Failures (cCdmaRpUpdHandoffMNAuthenFails)

> ID Mismatch Failures (cCdmaRpUpdHandoffIdMismatchFails)

> Bad Request Failures (cCdmaRpUpdHandoffBadReqFails)

> Note: All these statistics are a result of inter PCF handoffs.

### Unspecified Failures (cCdmaRpUpdHandoffReaUnSpecFails)

Number of updated registrations that failed due to an unspecified reason since system startup.

### Administrative Failures (cCdmaRpUpdHandoffAdmProhibFails)

Number of updated registrations that failed due to administrative prohibition since system startup.

### MN Authentication Failures (cCdmaRpUpdHandoffMNAuthenFails)

Number of updated registrations that failed due to MN authentication failure since system startup.

### ID Mismatch Failures (cCdmaRpUpdHandoffIdMismatchFails)

Number of registrations that failed due to a registration identity mismatch since system startup.

### Bad Request Failures (cCdmaRpUpdHandoffBadReqFails)

Number of updated registrations that failed due to a poorly formed request since system startup.