# Extended RMON Netflow Monitor

Device>Configure>Extended RMON Netflow Monitor

Use the Extended RMON Netflow Monitor feature to receive Netflow Data Export information, process it, and map it to an RMON2 group on your Clear Lake module. This feature can only be enabled for Catalyst 5000 switches with Earl2 and Clear Lake modules installed.

Note: In order to enable this feature, you must first obtain a special password from your Agent Option license.

Password (sysExtendedRmonNetflowPassword)

Accepts the password that enables the Extended RMON Netflow feature. The password must be set before the Extended RMON Netflow can be enabled.

Extended RMON Netflow (sysExtendedRmonNetflowEnable)

Indicates whether the Extended RMON Netflow feature is enabled or not; the default value is Disabled. Setting this object to disabled will automatically clear the password. Without a valid password entry, a setting of Enabled will be rejected and an error message displayed.