# Physical

Card>Configure>Physical

The CiscoView Configure Card window displays the following information:

Name (moduleName)

Name assigned to the module or card by the network administrator, such as “London.”

Module Model (moduleModel)

Manufacturer’s model number for the card or module.

Serial Number (moduleSerialNumberString)

Serial number of the card or module (for example, 900000023).

Hardware Version (moduleHwVersion)

Version number of the card being managed (for example, 3.1).

Firmware Version (moduleFwVersion)

Firmware version of the card being managed (for example, 2.0).

Software Version (moduleSwVersion)

Software version of the card being managed (for example, 3.2).

Status (moduleStatus)

Current status of the module or card. Possible values are ok, minorFault, majorFault, or other. If the status is not ok, the value of the Diagnostic Errors field gives more information about the cause of the problem.

Diagnostic Errors (moduleTestResult)

Result of the module’s self-test. None indicates that the module passed all tests.

Daughter Card1 (moduleSubType)

Type of daughterboard attached to this module, if any.

Note: This MIB is supported by all Supervisor modules.

Daughter Card2 (moduleSubType2)

Type of additional daughterboard attached to this module, if any.

Note: This MIB is supported by the Supervisor III module only.

Click Apply to make your changes take effect, or click Cancel to close the dialog box without making any changes. Click Print to print the contents of the dialog box.