# DS3 Configuration Information

To display DS3 configuration information, select DS3 Configuration from the CATEGORY pulldown menu while a CT3IP card is selected. The following information is displayed:

DS3 Interface ID (dsx3LineIndex)

DS3 Line Type (dsx3LineType)

DS3 Time Elapsed (dsx3TimeElapsed)

DS3 Valid Intervals (dsx3ValidIntervals)

DS3 Line Coding (dsx3LineCoding)

DS3 Send Code (dsx3SendCode)

DS3 Circuit Identifer (dsx3CircuitIdentifier)

DS3 Loopback Configuration (dsx3LoopbackConfig)

DS3 Line Status (dsx3LineStatus)

# DS3 Interface ID (dsx3LineIndex)

Identifies a DS3/E3 Interface on a managed device. If the ifEntry is directly associated only with this DS3/E3 interface, the value is same as ifIndex. If the ifEntry is not directly associated, then number the dsx3LineIndices with an unique identifier greater than the ifNumber. Choose even numbers for inside interfaces and odd numbers for outside interfaces.

# DS3 Line Type (dsx3LineType)

The kind of DS3 C-bit or E3 application that is implementing this interface. (Affects the interpretation of usage and error statistics.)

# DS3 Time Elapsed (dsx3TimeElapsed)

The number of seconds since the beginning of the current error-measurement period for the near end.

# DS3 Valid Intervals (dsx3ValidIntervals)

The number of previous near-end intervals for which valid data was collected. The value is the number of complete 15-minute near-end intervals since the interface came online, up to a maximum of 96 (24 hours).

# DS3 Line Coding (dsx3LineCoding)

The kind of zero code suppression used on this interface.

# DS3 Send Code (dsx3SendCode)

The type of code that the device is sending across the DS3/E3 interface.

# DS3 Circuit Identifier (dsx3CircuitIdentifier)

The transmission vendor's circuit identifier. Used to help with troubleshooting.

# DS3 Loopback Configuration (dsx3LoopbackConfig)

The loopback configuration of the DS3/E3 interface.