# Mobile Router Discovery Configs

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Configure button.

4. Select category Mobile Router Discovery Configs.

The following information appears:

> MA Address Type (cmiMrMaAddressType)

> HA Address (cmiMrMaAddress)

> Is Home Agent (cmiMrMaIsHa)

> Interface Index (cmiMrMaAdvRcvIf)

> Advertising Interface (cmiMrMaIfMacAddress)

> Sequence No (cmiMrMaAdvSequence)

> Advertisement Flags (cmiMrMaAdvFlags)

> Longest Registration Lifetime (cmiMrMaAdvMaxRegLifetime)

> Max Time of Validity (cmiMrMaAdvMaxLifetime)

> Max Advertisement Received (cmiMrMaAdvTimeReceived)

> First Advertisement Received (cmiMrMaAdvTimeFirstHeard)

##

### MA Address Type (cmiMrMaAddressType)

Type of IP address stored in cmiMrMaAddress. Only IPv4 address type is supported.

### HA Address (cmiMrMaAddress)

IP address of the mobile agent from which the advertisement was received. Only IPv4 addresses are supported.

### Is Home Agent (cmiMrMaIsHa)

Indicates whether the mobile agent is a home agent for the mobile router or not. If true, the agent is one of the mobile router's configured home agents.

### Interface Index (cmiMrMaAdvRcvIf)

ifIndex value from Interfaces table of MIB II for the interface of mobile router on which the advertisement from the mobile agent was received.

### Advertising Interface (cmiMrMaIfMacAddress)

Mobile agent advertising interface MAC address.

### Sequence No (cmiMrMaAdvSequence)

Sequence number of the most recently received agent advertisement. The sequence number ranges from 0 to 0xffff. After the sequence number attains the value 0xffff, it rolls over to 256.

### Advertisement Flags (cmiMrMaAdvFlags)

Flags contained in the 7th byte in the extension of the most recently received mobility agent advertisement:

reverseTunnel | Agent supports reverse tunneling
gre | Agent offers Generic Routing Encapsulation
minEnc | Agent offers Minimal Encapsulation
foreignAgent | Agent is a Foreign Agent
homeAgent | Agent is a Home Agent
busy | Foreign Agent is busy
regRequired | FA registration is required

### Longest Registration Lifetime (cmiMrMaAdvMaxRegLifetime)

Longest registration lifetime in seconds that the agent is willing to accept in any registration request.

### Max Time of Validity (cmiMrMaAdvMaxLifetime)

Maximum number of seconds during which the advertisement is considered valid in the absence of further advertisements.

### Max Advertisement Received (cmiMrMaAdvTimeReceived)

Time at which the most recently received advertisement was received.

### First Advertisement Received (cmiMrMaAdvTimeFirstHeard)

Time at which the first advertisement from the mobile agent was received.