PIB Interface Type

# PIB Interface Type

Device>Configure>PIB>Interface Type

This table describes the interface types that exist on the device.

Interface (qosInterfaceTypeId)

This table field provides the ID of the instance.

Queue Type (qosInterfaceQueueType)

This table field provides the interface type in terms of the number of queues and thresholds.

Roles (qosInterfaceTypeRoles)

This table field provides a combination of roles on at least one interface of type qosInterfaceType.

Capabilities (qosInterfaceTypeCapabilities)

This table field provides an enumeration of interface capabilities and is used by the PDP to select policies and configuration to push to the PEP.

The number in the bracket is the position of the bit in this field.

Bit 0 : not specified

- Classification support - inputL2Classification (1), inputIpClassification (2), outputL2Classification (3), outputIpClassification (4), inputPortClassification (19), outputPortClassification (20)

- Policing support - inputUflowPolicing (5), inputAggregatePolicing (6), outputUflowPolicing (7), outputAggregatePolicing (8), policeByMarkingDown (9), policeByDropping (10), inputUflowShaping (21), inputAggregateShaping (22), outputUflowShaping (23), outputAggregateShaping (24)

- Supported scheduling mechanisms - fifo (11), wrr (12), wfq (13), cq (14), pq (15), cbwfq (16), pqWrr (25), pqCbwfq (26)

- Supported congestion control mechanisms - tailDrop (17), wred (18)