# IMA Group Interval Statistics

The table displays following information:

Unavailable Seconds

Near End Failures

Far End Failures

UnavailableSecs (imaGroupIntervalUnavailSecs)

Number of 1-second intervals during which the IMA group traffic state machine is down in one of the 96intervals of 15 minutes each.

Near-End Failures (imaGroupIntervalNeNumFailures)

Number of times a near-end group failure has been reported in one of the previous 96intervals of 15 minutes each.

Far-End Failures (imaGroupIntervalFeNumFailures)

Number of times a far-end group failure has been reported in one of the previous 96 intervals of 15minutes each.