# RP Registration Failures (contd..)

Use this option to view Packet Control Function (PCF) and Service Option (SO) based RP Registration Failures.

## Procedure

To access RP Registration Failures (contd..) information:

1. Right-click the device and select Monitor from the popup menu.

2. Select CDMA PDSN PCF & SO Based Statistics from the Category menu.

3. Select any row and click on RP Registration Statistics.

4. Select RP Registration Failures (contd..) from the Category menu.

The following information appears:

> Unknown PDSN/HA Failures (cCdmaPcfSoRpRegUnkPdsnFails)

> Reverse Tunnel Setup Failures (cCdmaPcfSoRpRegNoRevTunFails)

> T-Bit Set Failures (cCdmaPcfSoRpRegTBitNSetFails)

> Bad CVSE Failures (cCdmaPcfSoRpRegBadCVSEFails)

### Unknown PDSN/HA Failures (cCdmaPcfSoRpRegUnkPdsnFails)

Number of registration requests that failed due to an unknown PDSN/HA address since system startup.

### Reverse Tunnel Setup Failures (cCdmaPcfSoRpRegNoRevTunFails)

Number of registration requests that failed due to the failure of Foreign Agent (FA) to Home Agent (HA) reverse tunnel setup since system startup.

### T-Bit Set Failures (cCdmaPcfSoRpRegTBitNSetFails)

Number of registration requests that failed because the T-bit required for the reverse tunnel was not set since system startup.

### Bad CVSE Failures (cCdmaPcfSoRpRegBadCVSEFails)

Number of registration requests that failed because of unsupported vendor codes in Customer/Vendor Specific Extension (CVSE) since system startup.