# Real Server Info

This dialog box provides information about the real server,such as the IP address of the server, the port , the connections handled, and the name of the server farm to which it belongs.

## Procedure

1. Right-click the device, then select Configure > SLB Statistics.

2. With a server load balancing (SLB) instance selected, click Real Servers. The following information is displayed.

> Server Farm Name (slbRealServerFarmName)

> Real IP Address (slbRealIpAddress)

> Real Port (slbRealPort)

> Real State (slbRealState)

> Reserved Connections (slbRealNumberOfDummyConnections)

> Maximum Connections (slbRealMaxConnections)

> Configured Weight (slbRealAdminWeight)

> Reassigned Real Server (slbRealReassign)

> Retry Time Interval (slbRealRetryInterval)

> Real Server Fails (slbRealFailedConnections)

> Client Fails (slbRealFailedClients)

> Real Row status (slbRealRowStatus)

### Server Farm Name (slbRealServerFarmName)

The name of the server farm .

### Real IP Address (slbRealIpAddress)

The IP address of the real server.

### Real Port (slbRealPort)

The TCP or UDP port of the real server. This port is used if SLB NAT is configured. Zero if SLB is not using NAT.

### Real State (slbRealState)

The current state of the real server.

### Reserved Connections (slbRealNumberOfDummyConnections)

The current number of idle dummy connections that are not in use but are reserved for the real server to accomplish slow-start.

### Maximum Connections (slbRealMaxConnections)

The maximum configured concurrent connections that SLB delivers to the real server.

### Configured Weight (slbRealAdminWeight)

The user-configured weight of the real server for load-balancing algorithms. The value zero shows that no new connections will be assigned to the real server. Higher weight values shows a greater availability of the real server to accept more work.

### Reassigned Real Server (slbRealReassign)

The number of consecutive unanswered TCP SYNs sent to the real server before reassigning the connection to another real server.

### Retry Time Interval (slbRealRetryInterval)

The time interval between retries while the server is in the Failed state.

### Real Server Fails (slbRealFailedConnections)

The number of failed connections after which the real server goes to Failed state. When connection fails, a SYN timesout or an RST is received from the real server.

### Client Fails (slbRealFailedClients)

The number of connections with distinct client IP addresses that fails before the server goes to Failed state. When connection fails, a SYN timesout or an RST is received from the real server.

### Real Row status (slbRealRowStatus)

The management station uses row status to create or delete a row entry in slbRealTable following the RowStatus text convention.