# GGSN Access Point Generic Server Table

## Procedure

1. Right-click the device and then select Configure, or double-click the device.

2. Select GGSN Access Point Generic Server Table from the Category drop-down box.

The following information appears:

> Access Point Identifier (cgprsAccPtIndex)

> Primary DNS Server (cgprsAccPtPriDnsServer)

> Secondary DNS Server (cgprsAccPtSecDnsServer)

> Primary NetBIOS Server (cgprsAccPtPriNetbiosServer)

> Secondary NetBIOS Server (cgprsAccPtSecNetbiosServer)

### Access Point Identifier (cgprsAccPtIndex)

Locally unique identifier for this access point on the Gateway GPRS support node (GGSN).

### Primary DNS Server (cgprsAccPtPriDnsServer)

IP address of the primary DNS server.

### Secondary DNS Server (cgprsAccPtSecDnsServer)

IP address of the secondary DNS server.

Note: A secondary server can be configured only when a primary server has already been configured.

### Primary NetBIOS Server (cgprsAccPtPriNetbiosServer)

IP address of the primary NetBIOS name server (NBNS).

### Secondary NetBIOS Server (cgprsAccPtSecNetbiosServer)

IP address of the secondary NBNS.

Note: A secondary server can be configured only when a primary server has already been configured.